* Time table / log
|      When? | What?                                                                      | Notes |
| 2019-02-21 | Kick-Off                                                                   | x     |
|            | Finish all admin points                                                    | x     |
|            | Know when/how to coordinate                                                | x     |
| 2019-02-21 | Clarifications Ueli Maurer (Mentor)                                        | x     |
|            | Write mail / phone                                                         | x     |
| 2019-02-22 | Have all papers handed in                                                  |       |
|            |                                                                            |       |
| 2019-02-22 | Have rough definition of tasks                                             | x     |
|            |                                                                            |       |
| 2019-02-23 | python2 / ipaddress is buggy                                               | x     |
|            | p4utils is python2 only support                                            |       |
|            | bmpy_utils is not installable with pip                                     |       |
|            | python2 / latest ipaddress==1.0.22 still has the bug                       |       |
|            | ipaddress.ip_network("2001:db8:61::/64")                                   |       |
|            | IPv6Network(u'3230:3031:3a64:6238:3a36:313a:3a2f:3634/128')                |       |
|            |                                                                            |       |
|            | egress routing                                                             | x     |
|            |                                                                            |       |
| 2019-02-24 | non reliable neighbor entries / flushing addresses puts into failed        |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-02-28 | Meet Laurent #2                                                            |       |
|            | - Status                                                                   |       |
|            | * Setup base code                                                          |       |
|            | * Parser for all protocols (udp,tcp,icmp,icmp6)                            |       |
|            | * Started with icmp translation                                            |       |
|            | * Investigating into IPv6 based checksums                                  |       |
|            | * Reading into various RFCs, NDP, MLD                                      |       |
|            | * Reading about multicast / trying to figure out dynamic membership        |       |
|            |                                                                            |       |
|            | - Challenges                                                               |       |
|            | * Some issues with python2 (ipaddr) - slowing down                         | x     |
|            | https://github.com/phihag/ipaddress/issues/46                              |       |
|            | * Forwarded and received icmp6 packets are not "accepted"                  |       |
|            |                                                                            |       |
|            | - Questions                                                                |       |
|            | * Multicast: in controller                                                 | x     |
|            | * Re-using code (lee howard)  -> ok & mention                              | x     |
|            | * A lot of redundant code / different tables / repeating: use if's         | x     |
|            | * 65k parsing is insane                                                    | x     |
|            |                                                                            |       |
|            | - Next steps:                                                              |       |
|            | * Supporting MLD                                                           |       |
|            | * Save stuff in the controller                                             |       |
|            | * checkout ipaddr bug / status                                             |       |
|            | * Variable length / icmp6 in the controller                                |       |
|            | * Go simple...                                                             |       |
|            | * Meeting Edgar & Alexander week after                                     |       |
|            | * Summary on Slack                                                         |       |
|            | * 1130 meeting now                                                         |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-03-01 | Feature list / priority list / roadmap clear                               | x     |
|            | Joining P4 Slack                                                           |       |
|            |                                                                            |       |
| 2019-03-03 | icmp6 revised:                                                             |       |
|            | - add address to table for forwarding to controller                        | x     |
|            | - select correct format for forwarding                                     |       |
|            | - decode in controller                                                     |       |
|            | - send back to switch                                                      |       |
|            | - test with host                                                           |       |
|            |                                                                            |       |
| 2019-03-06 | Meet Laurent #3                                                            |       |
|            | - Checksum's in scapy                                                      | x     |
|            | - Python2 ipaddress fix (import future)                                    | x     |
|            | - Added custom package format / additional information in packet           | x     |
|            | - (partial) NDP working in controller                                      | x     |
|            | - P4 checksum_with_payload                                                 | x     |
|            | - Reading scapy / inet6                                                    | x     |
|            | - Further checksum tests -> required everywhere in IPv6                    | x     |
|            | - icmp6 echo request working in controller                                 | x     |
|            | - Hosts can ping6 the switch                                               | x     |
|            | - Ran into P4 casting bug: https://github.com/p4lang/p4c/issues/1765       | x     |
|            | -> seems to be more than just casting bug                                  | x     |
|            | - Default route for ipv6 hosts                                             | x     |
|            |                                                                            |       |
|            | Next target:                                                               |       |
|            | - Focus on enabling the "Internet" with ICMP6 translation                  | x     |
|            |                                                                            |       |
|            | Next steps:                                                                |       |
|            | - Investigate again into checksumming with payload in P4                   | x     |
|            | - Answering icmp6 echo request *in* in the switch                          | x     |
|            | - Translate icmp6 to icmp                                                  | x     |
|            | - Translate icmp to icmp6                                                  |       |
|            | - Multiple branches:                                                       | x     |
|            | * Work on checksumming / p4                                                | x     |
|            | * Work on metadata passing / p4                                            | x     |
|            | * Work on static mapping (w/ incorrect checksum) 1:1                       |       |
|            | * v1model/                                                                 |       |
|            |                                                                            |       |
|            | Notes:                                                                     |       |
|            | * Edgar back on Friday // check tofino checksumming                        |       |
|            | * Bugs mentioning in thesis                                                |       |
|            | * Maybe run static mapping on tofino / p4_14                               |       |
|            | * Tofino p4_16: alpha compiler                                             |       |
|            | * Send recap / mail next week                                              |       |
|            | * week after 1130 Thursday                                                 |       |
|            |                                                                            |       |
| 2019-03-07 | ICMP6 checksumming works!!!                                                | x     |
|            | -> more fields needed to be included!                                      |       |
|            |                                                                            |       |
| 2019-03-13 | Tried/trying to get vagrant VM or P4* running on the notebook              |       |
|            |                                                                            |       |
| 2019-03-14 | NAT64 static rewrite                                                       | x     |
|            | - table support                                                            |       |
|            | - checksum not yet ported for translations                                 |       |
|            | - how to get mask from lpm table match?                                    |       |
|            | - how to get network from lpm match?                                       |       |
|            | - Create p4lang/p4-spec bug                                                |       |
|            | https://github.com/p4lang/p4-spec/issues/745                               |       |
|            |                                                                            |       |
| 2019-03-21 | Meet Laurent #4 - post poned - sick                                        | x     |
|            | https://github.com/p4lang/p4-spec/issues/660 sizeof() missing              |       |
|            |                                                                            |       |
|            | - Need to introduce new headers                                            |       |
|            | - Might need deeper parsing for icmp6_ns                                   |       |
|            | - Need hwaddr in icmp6_na                                                  |       |
|            | - Need to find out how to handle imcp6 options after target address        |       |
|            |                                                                            |       |
| 2019-03-23 | Parsing down to link layer option                                          | x     |
|            | Parsing on wrong field detected by unset fields in wireshark               |       |
|            | Correcting parser->leads to incorrect checksum                             |       |
|            | - NDP is answered to, but icmp6 echo request isn't -> extend table         |       |
|            |                                                                            |       |
|            | Problem with multiple LPM keys in table                                    |       |
|            | - logical problem, overlapping length matches                              |       |
|            | - priority / ordering would be helpful                                     |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-03-25 |                                                                            | x     |
|            | Writing down double LPM problem                                            |       |
|            | Removing source network support, documenting limitation                    |       |
|            | Rewriting code to use multiple NAT64 destinations                          |       |
|            | New test.py v6_static_mapping tests                                        |       |
|            |                                                                            |       |
|            | Again checksum errors in NDP answer                                        |       |
|            | Added debug code to send table ID towards controller                       |       |
|            |                                                                            |       |
| 2019-03-26 |                                                                            | x     |
|            | Find out where packet is stuck                                             |       |
|            |                                                                            |       |
| 2019-03-27 |                                                                            |       |
|            | switch cannot be used in actions!                                          |       |
|            | Refactor program to use multiple tables instead of switch                  |       |
|            | Ethernet frame check sequence error                                        |       |
|            |                                                                            |       |
| 2019-03-28 | Meet Laurent #4                                                            |       |
|            | - Router solicitation for finding router on startup                        |       |
|            | - test.py for TDD                                                          |       |
|            | - Parsing icmp6 is not enough - one layer deeper                           |       |
|            | - No LPM priorities                                                        |       |
|            | - if/switch action logic                                                   |       |
|            | - partial translation working to IPv4                                      |       |
|            | - Focus on checksumming work (again)                                       |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | Notes:                                                                     |       |
|            | - Later using ternary matching                                             |       |
|            | - Document (nested) if's in action (in thesis)                             |       |
|            | - SW and HW Targets Tofino [Albert, Thomas]                                |       |
|            | - P414/P416 for Tofino?                                                    |       |
|            | - Barefoot support/question: Ticket/Support System                         |       |
|            | - Can try P416 compiler                                                    |       |
|            | - Next week Laurent not around: send email + Albert/Thomas/Edgar meeting   |       |
|            |                                                                            |       |
| 2019-03-30 |                                                                            |       |
|            | Refactoring code                                                           |       |
|            | Hitting expression bug                                                     |       |
|            | Translating TO icmp4 works!                                                |       |
|            |                                                                            |       |
| 2019-04-02 |                                                                            |       |
|            | ARP egress support                                                         |       |
|            |                                                                            |       |
| 2019-04-03 |                                                                            |       |
|            | ARP corrections -- ARP working for the switch!                             | x     |
|            | ICMP w/ incorrect checksum                                                 | x     |
|            | ICMP w/ correct checksum - PING REPLIES!!!                                 | x     |
|            | Next: check / verify / translate nat46                                     |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-04-04 |                                                                            |       |
|            | Report [no meeting w/ Laurent]                                             |       |
|            |                                                                            |       |
|            | Added arp handling                                                         |       |
|            | Added icmp handling                                                        |       |
|            | Need to setup hardware addresses -> in theor resolution -> hardcoded atm   |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-04-04 | NAT64 1:1 table ICMP, ICMPv6 working                                       | x     |
|            | Will need some switch local ip addresses                                   | x     |
|            |                                                                            |       |
| 2019-04-11 | PLAN: NAT64 1:1 table UDP working                                          |       |
|            | checksums in both directions                                               |       |
|            |                                                                            |       |
| 2019-04-11 |                                                                            |       |
|            | Meeting Laurent                                                            |       |
|            |                                                                            |       |
|            | Status:                                                                    |       |
|            | - Minimal ARP working (for the switch address)                             |       |
|            |                                                                            |       |
|            | - echo ping/request icmp<->icmp6 working                                   |       |
|            | - udp_v6->udp_v4 working                                                   |       |
|            | - tcp_v6->tcp_v4 working                                                   |       |
|            | - udp_v4->udp_v6 working                                                   |       |
|            | - tcp_v4->udp_v6 working                                                   |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | Next steps:                                                                |       |
|            | - Hardware                                                                 |       |
|            | - icmp++                                                                   |       |
|            | - pmtu                                                                     |       |
|            | - sessions main step                                                       |       |
|            |                                                                            |       |
|            | Notes:                                                                     |       |
|            | - broadcast link only                                                      |       |
|            | - About 2w delivery time                                                   |       |
|            | - Get in touch with Tobias                                                 |       |
|            | - Scalability analysis -> how many connections/connections/s               |       |
|            | - Forwarding information in tables                                         |       |
|            | - Hendrik: semester thesis / NetPFGA                                       |       |
|            | - Tobias: advising Hendrik / Netpfga                                       |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-04-18 | PLAN: NAT64 1:1 table TCP/UDP working                                      | x     |
|            |                                                                            |       |
| 2019-04-23 |                                                                            |       |
|            | Meet Laurent                                                               |       |
|            |                                                                            |       |
|            | General                                                                    |       |
|            | - Get a better understanding of what others did                            |       |
|            |                                                                            |       |
|            | Review docs / specs                                                        |       |
|            | - Jool EAMT/SIIT fully                                                     |       |
|            |                                                                            |       |
|            | - IPv4 embedding                                                           |       |
|            | * Motivation/objective: working with real world DNS64                      |       |
|            | * RFC6052 suffix support                                                   |       |
|            | * RFC4291 IPv4-Compatible IPv6 Address (16 0s)                             |       |
|            | * RFC4291 IPv4-Mapped IPv6 Address (16 1s)                                 |       |
|            |                                                                            |       |
|            | - Session handling                                                         |       |
|            | * RFC6145: Translation ip/icmp, obsoleted by RFC 7915                      |       |
|            | * RFC6146: NAT64 definition, only TCP, UDP, and ICMP traffic               |       |
|            | * RFC6052: embedding support                                               |       |
|            | * Mode: IPv6 outgoing -> "masquarading"                                    |       |
|            | * Mode: IPv4                                                               |       |
|            |                                                                            |       |
|            | - Translation details                                                      |       |
|            | * How to handle ICMP4->icmp6 correctly (RFC7915)                           |       |
|            |                                                                            |       |
|            | - Hardware                                                                 |       |
|            | * NetFPGA                                                                  |       |
|            | * Hardware machine for software comparison?                                |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | New todos:                                                                 |       |
|            |                                                                            |       |
|            | - Translate fragment header                                                |       |
|            | - Support MTU / packet too big                                             |       |
|            | - Support PMTU, tcp mss                                                    |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | Meeting notes                                                              |       |
|            | - difference based                                                         |       |
|            | - first physical access                                                    |       |
|            | - tofino: if it compiles -> line rate                                      |       |
|            | - chaining switches / OS -> single port rate                               |       |
|            | - netpfga                                                                  |       |
|            | - reason about what in hardware and what in software -> reason tradeoff    | !!!   |
|            | - table gets full                                                          |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | Follow up:                                                                 |       |
|            |                                                                            |       |
|            | - what's the MTU of an interface? have a table                             |       |
|            | - have port/mtu                                                            |       |
|            | - total packeth length -> from IP                                          |       |
|            | - tables not in data plane                                                 |       |
|            | - Meeting Hendrik                                                          |       |
|            | - Meeting Kamila                                                           |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | - 768k                                                                     |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-05-02 | Jool SIIT / range / offset support https://www.jool.mx/en/run-vanilla.html | x     |
|            | Jool EAMT support https://www.jool.mx/en/run-eam.html                      |       |
|            | Bidirectional support                                                      |       |
|            | Will need IPv6 embedding suport https://tools.ietf.org/html/rfc6052        |       |
|            |                                                                            |       |
| 2019-04-18 | NAT64 prefix based IPv6->IPv4 conversion [tayga]                           |       |
|            | Use case: IPv6 hosts send to specific /96                                  |       |
|            |                                                                            |       |
| 2019-05-23 | NAT64 dynamic pool implementation: n:1 ipv6 to ipv4 mapping                |       |
|            | And n:1 stateful mappings https://www.jool.mx/en/run-nat64.html            |       |
|            | Needs active controller                                                    |       |
|            | Needs timeout / leases                                                     |       |
|            | Might work w/ registers                                                    |       |
|            |                                                                            |       |
| 2019-06-16 |                                                                            |       |
|            | Laurent meeting                                                            |       |
|            |                                                                            |       |
|            | - Vivado installation: silent errors, infinite loop, missing libncurses5   |       |
|            |                                                                            |       |
|            | - Compiling netfpga: 82k lines of code that are interdependent             |       |
|            | - Many non critical error messages on the way                              |       |
|            | - Zero exit fatal errors                                                   |       |
|            |                                                                            |       |
|            | - Code is not persistent in flash -> not there after power down            |       |
|            |                                                                            |       |
|            | - Not Receiving                                                            |       |
|            | - tcpdump on local nfX doesn't work -> can only debug on other endpoint    |       |
|            |                                                                            |       |
|            | - Writing tables fails                                                     |       |
|            |                                                                            |       |
|            | - Output all ports -> unclear how test data should look like               |       |
|            | - Found out broad/multicasting in theory -> bitmask                        |       |
|            |                                                                            |       |
|            | - HW test                                                                  |       |
|            | * compiling for 3 days                                                     |       |
|            | * Execution fails due to missing djtgcfg                                   |       |
|            |                                                                            |       |
|            | Payload to control plane                                                   |       |
|            | - digest not possible due to missing                                       |       |
|            | - might work with working                                                  |       |
|            |                                                                            |       |
|            | Next steps:                                                                |       |
|            | - Debug ioctl errors when writing table entries                            |       |
|            |                                                                            |       |
|            | - Understand HDL or PX user engines for writing checksum part              |       |
|            | - Adjust controller to digest                                              |       |
|            |                                                                            |       |
|            | HDL notes                                                                  |       |
|            | - cycle limitations                                                        |       |
|            | - variable length might be a problem                                       |       |
|            |                                                                            |       |
|            | Next steps after discussion:                                               |       |
|            |                                                                            |       |
|            | - checkout ipv6 test on netpfga / modify v6 packet                         |       |
|            | - checkout whether diff is possible on checksum -> see ttl                 |       |
|            | - checkout externs of Hendrik / report                                     |       |
|            | - Asses checksum difficulty                                                |       |
|            |                                                                            |       |
|            | Handing in thesis:                                                         |       |
|            |                                                                            |       |
|            | - Email pdf                                                                |       |
|            | - code on    github                                                        |       |
|            | - tar.gz of the code                                                       |       |
|            |                                                                            |       |
|            | - Decleration of -> from tobias                                            |       |
|            | - Week after: presentation                                                 |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            | - 15m talk                                                                 |       |
|            | - 15m q&a                                                                  |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-06-24 |                                                                            |       |
|            | Laurent meeting                                                            |       |
|            |                                                                            |       |
|            | Checksums                                                                  |       |
|            | - 16 bit sum of fields, later one/two complement                           |       |
|            | - various implementations                                                  |       |
|            | - is a sum -> commutative law                                              |       |
|            | - overflow (delta > payload) handling unclear                              |       |
|            |                                                                            |       |
|            | Netpfga                                                                    |       |
|            | - Old one had several failure messages (one in DDR area)                   |       |
|            | - New one: tables can be written                                           |       |
|            | - Need 3 ports: v4, v6, management                                         |       |
|            |                                                                            |       |
|            | Next steps:                                                                |       |
|            | - Test checksums delta on software switch                                  |       |
|            | - Begin to port code to netpfga one-by-one                                 |       |
|            |                                                                            |       |
|            | Follow up notes:                                                           |       |
|            | - Checkout Hendrik thesis / right / left shift                             |       |
|            | - Fix computer in lab                                                      |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-06-27 |                                                                            |       |
|            | Target Hardware: code running                                              |       |
|            |                                                                            |       |
| 2019-07-01 |                                                                            |       |
|            | Meeting Laurent                                                            |       |
|            |                                                                            |       |
|            | - Diff'ing in python:                                                      |       |
|            | * offsetting works                                                         |       |
|            | * Need to adjust to actual translation code                                |       |
|            |                                                                            |       |
|            | - Phasing in netpfga code / copy & compile & fix                           |       |
|            | * Code structure w/o apply logic                                           |       |
|            | * DIFF: Output port selection                                              |       |
|            | * DIFF: Sending to CPU                                                     |       |
|            |                                                                            |       |
|            | - Diff'ing in P4                                                           |       |
|            | * IPv4 checksum is w/o payload                                             |       |
|            |                                                                            |       |
|            | - Different generated output                                               |       |
|            |                                                                            |       |
|            | Next steps:                                                                |       |
|            | - Implement in BMV2 diff                                                   |       |
|            | - Checksum assignment / calc phase not clear                               |       |
|            | - Check if action has to be used                                           |       |
|            | - Check if ifdef makes a difference                                        |       |
|            | - Defense: list of dates                                                   |       |
|            |                                                                            |       |
|            | - iperf (alternative: hping) -> test on production setup                   |       |
|            |                                                                            |       |
|            | Late tests:                                                                |       |
|            | - Performance tests                                                        |       |
|            | - Extra things                                                             |       |
|            | - Maybe compile to openvswitch                                             |       |
|            |                                                                            |       |
| 2019-07-06 |                                                                            |       |
|            | Test case for delta in P4/BMV2:                                            |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-07-11 |                                                                            |       |
|            | Integrated org-documentation into latex / export working                   |       |
|            | https://bastibe.de/2014-09-23-org-cite.html                                |       |
|            | http://viveks.info/org-mode-academic-writing-bibliographies-org-ref/       |       |
|            | https://github.com/jkitchin/org-ref                                        |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-07-25 | Benmarking results between P4, Jool, Tayga                                 |       |
|            | Real hardware of advantage                                                 |       |
|            |                                                                            |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-08-01 | Latest start writing documentation                                         |       |
|            |                                                                            |       |
|            |                                                                            |       |
| 2019-08-21 | hand in thesis                                                             |       |
|            |                                                                            |       |
* Thesis implementation
** DONE Setup test VM for P4: 2a0a:e5c0:2:12:400:f0ff:fea9:c3e3
** DONE Get feature list of jool
** DONE Get feature list of tayga
** DONE Setup P4 base / structure
** DONE Create minimal controller for populating tables
** DONE Checkout / review egress settings
** DONE Create Basis to translate ipv6 --> ipv4 with a (freely programmable) prefix; test ping6_switch
*** DONE Insert prefix into switch: v6_networks
*** DONE Support multiple ipv6 source networks: need new table w/ 2 keys! -> not at the moment
*** DONE Write test.py to generate correct destination packets
>>> a = ipaddress.ip_network("2001:db8::/32")
>>> b = ipaddress.ip_address("10.0.0.1")
>>> a[int(b)]
IPv6Address('2001:db8::a00:1')
*** DONE Using test.py, new NDP packets been seen, bur zero icmp on the outgoing side
p4@ubuntu:~/master-thesis/p4app$ python test.py  --method v6_static_mapping --debug
INFO:main:Trying to reach 10.0.0.1 (64:ff9b::a00:1) from h1
sudo: unable to resolve host ubuntu
PING 64:ff9b::a00:1(64:ff9b::a00:1) 56 data bytes

--- 64:ff9b::a00:1 ping statistics ---
1 packets transmitted, 0 received, 100% packet loss, time 0ms

p4@ubuntu:~/master-thesis/p4app$
\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x87\x00\x08+\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_GENERAL ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x87\x00\x08+\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=2001:db8::42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x82b res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x02\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x87\x00\x08+\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_GENERAL ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x87\x00\x08+\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=2001:db8::42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x82b res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x02\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x87\x00\x08+\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_GENERAL ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x87\x00\x08+\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=2001:db8::42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x82b res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>

*** DONE Debug why neighbor discover does not work anymore
**** log
p4@ubuntu:~$ mx h1 tcpdump -lni any
sudo: unable to resolve host ubuntu
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on any, link-type LINUX_SLL (Linux cooked), capture size 262144 bytes

19:57:53.258805 IP6 fe80::200:aff:fe00:1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8::42, length 32
19:57:54.256924 IP6 2001:db8::1 > 2001:db8::1: ICMP6, destination unreachable, unreachable address 64:ff9b::a00:1, length 112

EBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x01\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x007\xdf\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_NS ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff\xfe\x80\x00\x00\x00\x00\x00\x00\x02\x00\n\xff\xfe\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x007\xdf\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
INFO:main:Doing neighbor solicitation
DEBUG:main:OUTGOING: <Ether  dst=00:00:0a:00:00:01 src=00:00:0a:00:00:42 type=0x86dd |<IPv6  nh=ICMPv6 hlim=255 src=2001:db8::42 dst=fe80::200:aff:fe00:1 |<ICMPv6ND_NA  cksum=None R=0 S=1 tgt=2001:db8::42 |<ICMPv6NDOptDstLLAddr  lladdr=00:00:0a:00:00:42 |>>>>
DEBUG:main:INCOMING: <Ether  dst=00:00:0a:00:00:01
src=00:00:0a:00:00:42 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32
nh=ICMPv6 hlim=255 src=2001:db8::42
dst=fe80::200:aff:fe00:1 |<ICMPv6ND_NA  type=Neighbor Advertisement
code=0 cksum=0xa5e9 R=0 S=1 O=1 res=0x0
tgt=2001:db8::42 |<ICMPv6NDOptDstLLAddr  type=2 len=1
lladdr=00:00:0a:00:00:42 |>>>>


After removing noise:

DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>

**** Do we have routing for fe80::/10? Probably not. Shouldn't we see it in the controller then?
**** NDP is controller only!
*** DONE Finish NDP in switch
**** DONE Need to set R/S/O bits
**** DONE Need to parse R/S/O bits
*** DONE Maybe merge v6_address and v6_networks - /128 is the same
*** DONE Implement address learning? -> not at the moment
*** DONE Not sure whether we should react on router solicitation -> not at the moment
    - Using static routes -> should do the job
*** DONE Implement the calculation
Currently offset + ip address
*** DONE Sketch the flow for session handling for icmp6 w/o packet loss
      - switch receives icmp6 packet for known prefix
      - controller needs to create session entry (?)

Not sure what I meant to do here - closing.
*** DONE Create table entry for mapping v4->v6 [net]
*** DONE Create table entry for mapping v6->v4 [net]
** DONE Implement ICMP <-> ICMP6 translation
*** DONE 2019-02-28 / icmp testing / first NDP steps
**** DONE pinging in router mode: nothing shown in the controller, multicast forwarded -> "ok"

 root@ubuntu:~/master-thesis/p4app# ping6 -c1 2001:db8:61::42
 PING 2001:db8:61::42(2001:db8:61::42) 56 data bytes
 From 2001:db8:61::1 icmp_seq=1 Destination unreachable: Address unreachable

 --- 2001:db8:61::42 ping statistics ---
 1 packets transmitted, 0 received, +1 errors, 100% packet loss, time 0ms

 root@ubuntu:~/master-thesis/p4app#


 sudo: unable to resolve host ubuntu
 tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
 listening on h1-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
 09:47:07.191569 IP6 2001:db8:61::1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8:61::42, length 32
 09:47:08.190331 IP6 2001:db8:61::1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8:61::42, length 32
 09:47:09.190279 IP6 2001:db8:61::1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8:61::42, length 32
**** DONE special rule for ff02::1:ff00:42

 Semi works, replies are there, but host still retries:

 p4@ubuntu:~/master-thesis$ h=1; mx h$h tcpdump -lni h$h-eth0
 sudo: unable to resolve host ubuntu
 tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
 listening on h1-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
 09:58:04.786979 IP6 2001:db8:61::1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8:61::42, length 32
 09:58:04.793560 IP6 2001:db8:61::42 > 2001:db8:61::1: ICMP6, neighbor advertisement, tgt is 2001:db8:61::42, length 32
 09:58:05.786311 IP6 2001:db8:61::1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8:61::42, length 32
 09:58:05.790506 IP6 2001:db8:61::42 > 2001:db8:61::1: ICMP6, neighbor advertisement, tgt is 2001:db8:61::42, length 32
 09:58:06.786254 IP6 2001:db8:61::1 > ff02::1:ff00:42: ICMP6, neighbor solicitation, who has 2001:db8:61::42, length 32
 09:58:06.792325 IP6 2001:db8:61::42 > 2001:db8:61::1: ICMP6, neighbor advertisement, tgt is 2001:db8:61::42, length 32


 Maybe checksums?
*** DONE Parse icmp
*** DONE Parse icmpv6
*** DONE Add (static) egress configuration
*** DONE Calculate ICMP6 checksums in controller
**** Need to include the payload!?!!
*** DONE Implement minimal neighbor discovery in controller
**** DONE For the switch
***** DONE Register IPv6 address in table
***** DONE Parse ICMPv6 up to neighbor solicitation -> no: checksum problem
***** DONE Use NDP (Neighbor Solicitation (NDP)	, Neighbor Advertisement (NDP)) -> no: controller
***** Approach 2: use cpu header, forward information to controller
***** DONE Fix the ip address match/mapping: 42 -> 2a -> use hex originally
***** DONE Find out why wrong type is used -> overlapping with NDP
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x03\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
p=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x03\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=DEBUG ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:o=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd3a4 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:Debug purpose only
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x03\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
p=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x03\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=DEBUG ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:o=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd3a4 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:Debug purpose only
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x03\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
p=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x03\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=DEBUG ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:o=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd3a4 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:Debug purpose only
***** Disable debug by default -> gives correct packets

DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x01\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_NS ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:o=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd3a4 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:Doing neighbor solicitation
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x01\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_NS ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:o=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd3a4 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:Doing neighbor solicitation
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x4242 |<Raw  load='\x00\x01\x00\x01\x86\xdd`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:cpu = <CpuHeader  task=ICMP6_NS ingress_port=1 type=0x86dd |<Raw  load='`\x00\x00\x00\x00 :\xff \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\xff\x00\x00B\x87\x00\xd3\xa4\x00\x00\x00\x00 \x01\r\xb8\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00B\x01\x01\x00\x00\n\x00\x00\x01' |>>
DEBUG:main:o=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd3a4 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:Doing neighbor solicitation

**** DONE For other nodes -> multicast
**** TODO Maybe implement link local addresses (missing at the moment)
***** ff02::/??
***** rfc4861
"Neighbor Solicitation messages are multicast to the  solicited-node
multicast address of the target address."
***** DONE multicasting / groups
****** create a group ("node") that contains "all other" ports
****** create a multicast group with an ID
****** associate the "node" with the multicast group ID
**** If destination is within ff02::1:ff00:0/104, multicast

*** DONE Make switch answer icmp6 echo request for
*** DONE Introduce mixed mode: switch: icmp6 echo reply, controller: NDP
**** DONE try 1: reply seen, but checksum is incorrect
**** DONE try 2: analysing tagya checksumming code
static uint16_t ip6_checksum(struct ip6 *ip6, uint32_t data_len, uint8_t proto)
{
	uint32_t sum = 0;
	uint16_t *p;
	int i;

	for (i = 0, p = ip6->src.s6_addr16; i < 16; ++i)
		sum += *p++;
	sum += htonl(data_len) >> 16;
	sum += htonl(data_len) & 0xffff;
	sum += htons(proto);

	while (sum > 0xffff)
		sum = (sum & 0xffff) + (sum >> 16);

	return ~sum;
}

static uint16_t convert_cksum(struct ip6 *ip6, struct ip4 *ip4)
{
	uint32_t sum = 0;
	uint16_t *p;
	int i;

	sum += ~ip4->src.s_addr >> 16;
	sum += ~ip4->src.s_addr & 0xffff;
	sum += ~ip4->dest.s_addr >> 16;
	sum += ~ip4->dest.s_addr & 0xffff;

	for (i = 0, p = ip6->src.s6_addr16; i < 16; ++i)
		sum += *p++;

	while (sum > 0xffff)
		sum = (sum & 0xffff) + (sum >> 16);

	return sum;
}
...
static int xlate_payload_4to6(struct pkt *p, struct ip6 *ip6)
{
	uint16_t *tck;
	uint16_t cksum;

	if (p->ip4->flags_offset & htons(IP4_F_MASK))
		return 0;

	switch (p->data_proto) {
	case 1:
		cksum = ip6_checksum(ip6, htons(p->ip4->length) -
						p->header_len, 58);
		cksum = ones_add(p->icmp->cksum, cksum);
		if (p->icmp->type == 8) {
			p->icmp->type = 128;
			p->icmp->cksum = ones_add(cksum, ~(128 - 8));
		} else {
			p->icmp->type = 129;
			p->icmp->cksum = ones_add(cksum, ~(129 - 0));
		}
		return 0;
*** DONE Add default route for v6  hosts
p4@ubuntu:~/master-thesis$ mx h1 ip -6 r
sudo: unable to resolve host ubuntu
2001:db8::/64 dev h1-eth0  proto kernel  metric 256  pref medium
fe80::/64 dev h1-eth0  proto kernel  metric 256  pref medium
default via 2001:db8::42 dev h1-eth0  metric 1024  pref medium
p4@ubuntu:~/master-thesis$
*** DONE TEST ping6ing an emulated ipv6 host / Translate icmp <-> icmp6: test v6_static_mapping
**** DONE try1: only packets on h1 + controller -> wrong checksum 2019-03-25
+ filename=static_nat64-2019-03-25-1121-h1.pcap
+ intf=h1-eth0
+ mx h1 tcpdump -ni h1-eth0 -w static_nat64-2019-03-25-1121-h1.pcap
tcpdump: listening on h1-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
^C10 packets captured
10 packets received by filter
0 packets dropped by kernel
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>


That looks like NDP is not working again. Why: checksum seems to be
incorrect according to wireshark. Why? Checksum is the SAME as in the
request -> probably not updated. After inserting marker: it's clear
that the checksum code DOES NOT work on the task field!

Problem: task field might be overriden for controller use in different
table -> need different task field!

**** DONE try2: checksum ok, but no packets on h3
***** DONE Setup a default rule for the IPv4 world to debug on controller
Still not seeing the converted packet, however seeing icmp6_ns packets
which should not be there:

table entry for ns:

ff:02:00:00:00:00:00:00:00:00:00:01:ff:00:00:42/128

debug packet seen in controller:

DEBUG:main:v6 reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:v6 reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:v6 reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>

DEBUG:main:v6 reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=920946 plen=64 nh=ICMPv6 hlim=64 src=2001:db8::1 dst=2001:db8:1::a00:1 |<ICMPv6EchoRequest  type=Echo Request code=0 cksum=0xf981 id=0x5f7c seq=0x1 data='N\xc6\x98\\\x00\x00\x00\x00\x12\x1b\t\x00\x00\x00\x00\x00\x10\x11\x12\x13\x14\x15\x16\x17\x18\x19\x1a\x1b\x1c\x1d\x1e\x1f !"#$%&\'()*+,-./01234567' |>>>

debugging MIGHT come from nat64 table!

**** DONE try3: re-rewrite: no packets on h3 again (2019-03-30)
p4@ubuntu:~$ ~/master-thesis/p4app/sniff-host.sh h1 static_nat64
+ cd /home/p4/master-thesis/pcap
+ host=h1
+ name=static_nat64
+ date +%F-%H%M
+ now=2019-03-30-1608
+ filename=static_nat64-2019-03-30-1608-h1.pcap
+ intf=h1-eth0
+ mx h1 tcpdump -ni h1-eth0 -w static_nat64-2019-03-30-1608-h1.pcap
tcpdump: listening on h1-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
^C10 packets captured
10 packets received by filter
0 packets dropped by kernel

p4@ubuntu:~$
p4@ubuntu:~/master-thesis/pcap$ ../p4app/sniff-host.sh h3 static_nat64
+ cd /home/p4/master-thesis/pcap
+ host=h3
+ name=static_nat64
+ date +%F-%H%M
+ now=2019-03-30-1608
+ filename=static_nat64-2019-03-30-1608-h3.pcap
+ intf=h3-eth0
+ mx h3 tcpdump -ni h3-eth0 -w static_nat64-2019-03-30-1608-h3.pcap
tcpdump: listening on h3-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
^C0 packets captured
0 packets received by filter
0 packets dropped by kernel

p4@ubuntu:~/master-thesis/pcap$

-> NDP is going to the controller instead of being handled by the switch
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS

-> checksums likely broken again due to checksum changes
-> solved, test case for verification is

#+BEGIN_SRC
p4@ubuntu:~$ python ~/master-thesis/p4app/test.py -m v6_static_mapping --debug
INFO:main:Trying to reach 10.0.0.1 (2001:db8:1::a00:1) from h1
PING 2001:db8:1::a00:1(2001:db8:1::a00:1) 56 data bytes
From 2001:db8::1 icmp_seq=1 Destination unreachable: Address unreachable

--- 2001:db8:1::a00:1 ping statistics ---
1 packets transmitted, 0 received, +1 errors, 100% packet loss, time 0ms

p4@ubuntu:~$ python ~/master-thesis/p4app/test.py -m ping6_switch --debug
INFO:main:Trying to reach 2001:db8::42 from h1
PING 2001:db8::42(2001:db8::42) 56 data bytes
64 bytes from 2001:db8::42: icmp_seq=1 ttl=64 time=6.30 ms

--- 2001:db8::42 ping statistics ---
1 packets transmitted, 1 received, 0% packet loss, time 0ms
rtt min/avg/max/mdev = 6.304/6.304/6.304/0.000 ms


#+END_SRC
**** DONE try4: h3 receives packet, but length seems to be off
     - Seeing frame check sequence error
     - total length ipv4 = 69 (h3)
     - ipv6 payload length = 64 (h1)
     - comes from         hdr.ipv4.totalLen       = (bit<16>) hdr.ipv6.payload_length + 5;
     - https://tools.ietf.org/html/rfc791:
     Total Length is the length of the datagram, measured in octets,
     including internet header and data.
     - checksum = 0 -> offset incorrect???
     - ipv4 checksum is 0
     - nat64 frame length = 98 bytes
     - theory: ethernet: 48+48+16 = 112 bit -> 12 bytes
     - nat64: 76 bytes inside ethernet frame
     - nat64: 69 bytes according to total_len
     - nat64: -5 bytes = icmp4 = 64 bytes
     - icmp6 == 64 bytes
     - diff of 7 bytes :-)
     - icmp should be:
     - type+code+checksum = 4 bytes
     - seq + identifier = 4 bytes
     - data = variable, source is 56 bytes
     - real world ping: total_length = 84, 48 bytes icmp data
     - header length in both cases = 5
     - identification 0 in nat64, 0x2cad in real
     - flags 0 in nat64, 0x4000 (DF) in real
     - ttl = 64 both
     - proto = icmp both cases
     - header checksum = 0 in nat64, set in real
     - data is shorter in nat64, due to total_len error
     - real world icmp contains time stamp data ???
     - wireshark EXPECTS timestamp data in echo request! + 8 bytes
       and then data
     - almost fits diff 7 vs. 8
     - 8 bytes in one block in wireshark
     - after ipv4: 6 + 8 + 3*(16) + 2 = 64 -- wtf??
     - icmp6: data == 56 bytes
     - nat64 and realping4 frame == 98 bytes




***** TODO Correct IPv4 header checksum
***** TODO Correct ICMP header checksum
***** TODO Fix length issue
      - Seems like total_len is too short - but why?
**** DONE try5: packet is good, but routing is "strange": default route == 10.0.0.66
root@ubuntu:~# ip r
default via 10.0.0.66 dev h3-eth0
10.0.0.0/24 dev h3-eth0  proto kernel  scope link  src 10.0.0.1
root@ubuntu:~#
**** DONE try6: host sees packet, but does not react on it, manually tring gateway ping

p4@ubuntu:~$ mx h3 tcpdump -lni h3-eth0
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on h3-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
09:06:02.636669 IP 10.1.1.1 > 10.0.0.1: ICMP echo request, id 31058, seq 1, length 64

in h3:

root@ubuntu:~# ip a
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN group default qlen 1
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    inet 127.0.0.1/8 scope host lo
       valid_lft forever preferred_lft forever
    inet6 ::1/128 scope host
       valid_lft forever preferred_lft forever
2: h3-eth0@if38: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 9500 qdisc netem state UP group default qlen 1000
    link/ether 00:00:0a:00:00:03 brd ff:ff:ff:ff:ff:ff link-netnsid 0
    inet 10.0.0.1/24 scope global h3-eth0
       valid_lft forever preferred_lft forever
root@ubuntu:~#

no arp entries:

root@ubuntu:~# arp -an
root@ubuntu:~#

root@ubuntu:~# ping -c1 10.0.0.66
PING 10.0.0.66 (10.0.0.66) 56(84) bytes of data.
From 10.0.0.1 icmp_seq=1 Destination Host Unreachable

--- 10.0.0.66 ping statistics ---
1 packets transmitted, 0 received, +1 errors, 100% packet loss, time 0ms

root@ubuntu:~#

**** DONE try7: checkout dump from ping4_gw-2019-03-31-0916-h3.pcap: regular arp
**** DONE Get a real world arp trace
root@line:/home/nico/vcs/master-thesis/pcap# tcpdump -ni wlan0 -w ping4_realworld_p7 icmp or arp or host 192.168.4.1
tcpdump: listening on wlan0, link-type EN10MB (Ethernet), capture size 262144 bytes
root@line:~# arp -an
? (192.168.4.188) at 00:0d:b9:46:3b:d4 [ether] on wlan0
root@line:~# ping -c1 192.168.4.1
PING 192.168.4.1 (192.168.4.1) 56(84) bytes of data.
64 bytes from 192.168.4.1: icmp_seq=1 ttl=64 time=15.5 ms

--- 192.168.4.1 ping statistics ---
1 packets transmitted, 1 received, 0% packet loss, time 0ms
rtt min/avg/max/mdev = 15.533/15.533/15.533/0.000 ms
root@line:~#

**** TODO Implement default route handling, maybe implement ARP?
***** DONE create arp table
***** TODO Multiple tables not supported
p4c --target bmv2 --arch v1model --std p4-16 "../p4src/static-mapping.p4" -o "/home/p4/master-thesis/p4src"
../p4src/static-mapping.p4(366): error: Program is not supported by this target, because table MyIngress.v6_networks has multiple successors
    table v6_networks {
          ^^^^^^^^^^^
Compilation Error

***** Entry in v4_networks?
*** DONE Add table name support in debug messages
*** DONE Why getting IPv6 packets in
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_NAT64
INFO:main:unhandled reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=920946 plen=64 nh=ICMPv6 hlim=64 src=2001:db8::1 dst=2001:db8:1::a00:1 |<ICMPv6EchoRequest  type=Echo Request code=0 cksum=0x3d1a id=0xade seq=0x1 data='\x1f\x92\x9a\\\x00\x00\x00\x00WU\x02\x00\x00\x00\x00\x00\x10\x11\x12\x13\x14\x15\x16\x17\x18\x19\x1a\x1b\x1c\x1d\x1e\x1f !"#$%&\'()*+,-./01234567' |>>> from table TABLE_V4_NETWORKS
*** DONE Solve logic problem: Valid headers
- If ipv6 header is valid && nat64 will be made and afterwards v4 egress needs to be applied
- If ipv4 header is valid && nat46 will be made and afterwards v6 egress needs to be applied
*** DONE Check translated fields
**** DONE source correctly translated to 10.1.1.1
**** DONE destination correctly translated to 10.0.0.1 -> pings h3
**** DONE egress is correct, comes out at h3
**** DONE protocol 58 is wrong -> should be 1
**** DONE figure out switch() syntax
**** DONE transform protocol specific: icmp6 -> icmp
***** DONE Implement double table, as there are no if's in actions
***** DONE Debug Ethernet frame check sequence error -> need to compute checksum
       https://en.wikipedia.org/wiki/Frame_check_sequence

According to Edgar this should not be seen anyway.
***** DONE Calculate ICMP checksum
***** DONE Check field lengths
***** DONE Fix resolve / mac addresses -> ethernet is wrong!
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS

According to pcap/static_nat64-2019-04-03-0932-h3.pcap ethernet frame
looks good. Still no reply / reaction from host h3.
***** DONE Fix IPv4 header checksum // wrong according to wireshark
When & how to update?
***** DONE check packets static_nat64-2019-04-03-0957-h1.pcap: answer not outputted/natted!
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x37df res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:03 type=0x800 |<IP  version=4 ihl=5 tos=0x0 len=84 id=60628 flags= frag=0 ttl=64 proto=icmp chksum=0x78d2 src=10.0.0.1 dst=10.1.1.1 options=[] |<ICMP  type=echo-reply code=0 chksum=0x9138 id=0x26e9 seq=0x1 |<Raw  load='\x8b\x83\xa4\\\x00\x00\x00\x00S*\x06\x00\x00\x00\x00\x00\x10\x11\x12\x13\x14\x15\x16\x17\x18\x19\x1a\x1b\x1c\x1d\x1e\x1f !"#$%&\'()*+,-./01234567' |>>>> from table TABLE_V6_NETWORKS
****** DONE Is 10.1.1.1/x in the nat64 table? yes
Adding entry to lpm match table nat46
match key:           LPM-0a:01:01:00/24
action:              nat46_static
runtime data:        20:01:0d:b8:00:00:00:00:00:00:00:00:00:00:00:00    0a:01:01:00     20:01:0d:b8:00:01:00:00:00:00:00:00:00:00:00:00
Entry has been added with handle 0
****** DONE if nat46_static is called, why is the ethernet type still ipv4? -> log!
******* DONE nat46 table is applied
****** DONE Check why there is a miss in the table -> c&p bug?
[09:57:31.415] [bmv2] [T] [thread 9332] [105.0] [cxt 0] Applying table 'MyIngress.v6_networks'
[09:57:31.415] [bmv2] [D] [thread 9332] [105.0] [cxt 0] Looking up key:
 * hdr.ipv6.dst_addr   : 20010db8000000000000000000000001

[09:57:31.415] [bmv2] [D] [thread 9332] [105.0] [cxt 0] Table 'MyIngress.v6_networks': miss

**** DONE transform protocol specific: icmp -> icmp6
***** DONE Make switch answer IPv4 icmp echo request for
****** DONE Make switch respond to ARP
****** DONE Make switch respond to icmp echo request w/ correct checksum (2019-04-03)
****** DONE Correct icmp6 checksum
******* DONE Checksum is SET, but not correct!
**** DONE Test result (2019-04-03)
p4@ubuntu:~$ python ~/master-thesis/p4app/test.py -m  v6_static_mapping
PING 2001:db8:1::a00:1(2001:db8:1::a00:1) 56 data bytes
64 bytes from 2001:db8:1::a00:1: icmp_seq=1 ttl=64 time=14.7 ms

--- 2001:db8:1::a00:1 ping statistics ---
1 packets transmitted, 1 received, 0% packet loss, time 0ms
rtt min/avg/max/mdev = 14.750/14.750/14.750/0.000 ms
p4@ubuntu:~$
*** DONE Add / check default route for v4 hosts
*** DONE Check IPv4 -> IPv6 translation
p4@ubuntu:~$ python ~/master-thesis/p4app/test.py -m v4_static_mapping
PING 10.1.1.1 (10.1.1.1) 56(84) bytes of data.
64 bytes from 10.1.1.1: icmp_seq=1 ttl=64 time=12.5 ms

--- 10.1.1.1 ping statistics ---
1 packets transmitted, 1 received, 0% packet loss, time 0ms
rtt min/avg/max/mdev = 12.593/12.593/12.593/0.000 ms
p4@ubuntu:~$

** TODO Implement ipv6<->ipv4 udp translation
*** DONE udp: ipv6->ipv4

p4@ubuntu:~$ mx h3 "echo V4-OK | socat - UDP-LISTEN:2342"
/usr/bin/mx: line 25: [: too many arguments
V6-OK
p4@ubuntu:~$

p4@ubuntu:~$ mx h1 "echo V6-OK | socat - UDP6:[2001:db8:1::a00:1]:2342"
/usr/bin/mx: line 25: [: too many arguments
V4-OK
p4@ubuntu:~$
**** pcap/v6_udp-2019-04-11-0840-h1.pcap
**** pcap/v6_udp-2019-04-11-0840-h3.pcap
*** TODO udp: ipv4->ipv6
p4@ubuntu:~$ mx h3 "echo V4-OK | socat - UDP:10.1.1.1:2342"
/usr/bin/mx: line 25: [: too many arguments
V6-OK
p4@ubuntu:~$
p4@ubuntu:~$ mx h1 "echo V6-OK | socat - UDP6-LISTEN:2342"
/usr/bin/mx: line 25: [: too many arguments
V4-OK
**** proof
create mode 100644 pcap/v4_udp-2019-04-11-0855-h1.pcap
create mode 100644 pcap/v4_udp-2019-04-11-0855-h3.pcap

** DONE Implement ipv6<->ipv4 tcp translation
*** DONE tcp: v6 -> v4
p4@ubuntu:~$ mx h1 "echo V6-OK | socat - TCP6:[2001:db8:1::a00:1]:2342"
/usr/bin/mx: line 25: [: too many arguments
V4-OK
p4@ubuntu:~$
p4@ubuntu:~$ mx h3 "echo V4-OK | socat - TCP-LISTEN:2342"
/usr/bin/mx: line 25: [: too many arguments
V6-OK
p4@ubuntu:~$
**** Proof
create mode 100644 pcap/v6_tcp-2019-04-11-0846-h1.pcap
create mode 100644 pcap/v6_tcp-2019-04-11-0846-h3.pcap
*** DONE tcp: v4 -> v6
p4@ubuntu:~$ mx h3 "echo V4-OK | socat - TCP:10.1.1.1:2342"
/usr/bin/mx: line 25: [: too many arguments
V6-OK
p4@ubuntu:~$
p4@ubuntu:~$ mx h1 "echo V6-OK | socat - TCP6-LISTEN:2342"
/usr/bin/mx: line 25: [: too many arguments
V4-OK
p4@ubuntu:~$
**** Proof
pcap/v4_tcp-2019-04-11-0853-h1.pcap | Bin 0 -> 1174 bytes
pcap/v4_tcp-2019-04-11-0853-h3.pcap | Bin 0 -> 1070 bytes

** TODO Update p4c to avoid compiler bug
*** TODO Updating p4c
**** DONE Try1
p4@ubuntu:~/p4-learning/vm/bin$ sh update-p4c.sh
update-p4c.sh: 34: update-p4c.sh: Syntax error: "(" unexpected
p4@ubuntu:~/p4-learning/vm/bin$ git pull
Already up-to-date.
p4@ubuntu:~/p4-learning/vm/bin$ git describe --always
fb9d0ea
p4@ubuntu:~/p4-learning/vm/bin$

p4@ubuntu:~/p4-tools/p4c$ git checkout 1ab1c796677a3a2349df9619d82831a39a6e4437
p4@ubuntu:~/p4-tools/p4c/build$ cmake  ..
p4@ubuntu:~/p4-tools/p4c/build$ make -j8
**** DONE Need to upgrade RAM / c++ errors / killed
**** DONE Compile error from 1ab1c79
[ 33%] Building CXX object frontends/CMakeFiles/frontend.dir/unified_frontend_sources_4.cpp.o
[ 37%] Building CXX object frontends/CMakeFiles/frontend.dir/__/ir/ir-generated.cpp.o
[ 35%] Building CXX object frontends/CMakeFiles/frontend.dir/unified_frontend_sources_2.cpp.o
[ 43%] Built target midend
[ 45%] Linking CXX static library libfrontend.a
[ 56%] Built target frontend
Scanning dependencies of target bmv2backend
make[2]: *** No rule to make target '../control-plane/p4runtime/proto/p4/v1/p4data.proto', needed by 'control-plane/google/rpc/status.pb.cc'.  Stop.
CMakeFiles/Makefile2:1197: recipe for target 'control-plane/CMakeFiles/controlplane.dir/all' failed
make[1]: *** [control-plane/CMakeFiles/controlplane.dir/all] Error 2
make[1]: *** Waiting for unfinished jobs....
[ 58%] Building CXX object backends/bmv2/CMakeFiles/bmv2backend.dir/unified_bmv2_backend_common_srcs_1.cpp.o
[ 59%] Building CXX object backends/bmv2/CMakeFiles/bmv2backend.dir/unified_bmv2_backend_common_srcs_2.cpp.o
[ 61%] Linking CXX static library libbmv2backend.a
[ 61%] Built target bmv2backend
Makefile:138: recipe for target 'all' failed
make: *** [all] Error 2
p4@ubuntu:~/p4-tools/p4c/build$ cd ..
p4@ubuntu:~/p4-tools/p4c$ git describe  --always
1ab1c79
p4@ubuntu:~/p4-tools/p4c$
**** DONE Upgrading to latest master: 46609cd -> fails
p4@ubuntu:~/p4-tools/p4c$ git describe --always
46609cd

p4@ubuntu:~/p4-tools/p4c$ cd build/
p4@ubuntu:~/p4-tools/p4c/build$ make clean
frontends/CMakeFiles/frontend.dir/build.make:93: warning: overriding recipe for target 'frontends/parsers/v1/v1parser.output'
frontends/CMakeFiles/frontend.dir/build.make:74: warning: ignoring old recipe for target 'frontends/parsers/v1/v1parser.output'
p4@ubuntu:~/p4-tools/p4c/build$ cmake  .. && make -j8
[ 50%] Building CXX object frontends/CMakeFiles/frontend.dir/unified_frontend_sources_5.cpp.o
[ 51%] Building CXX object frontends/CMakeFiles/frontend.dir/unified_frontend_sources_6.cpp.o
[ 53%] Linking CXX static library libir.a
[ 53%] Built target ir
[ 54%] Building CXX object frontends/CMakeFiles/frontend.dir/unified_frontend_sources_7.cpp.o
[ 56%] Linking CXX static library libfrontend.a
[ 56%] Built target frontend
make[2]: *** No rule to make target '../control-plane/p4runtime/proto/p4/v1/p4data.proto', needed by 'control-plane/google/rpc/status.pb.cc'.  Stop.
CMakeFiles/Makefile2:1197: recipe for target 'control-plane/CMakeFiles/controlplane.dir/all' failed
make[1]: *** [control-plane/CMakeFiles/controlplane.dir/all] Error 2
make[1]: *** Waiting for unfinished jobs....
Scanning dependencies of target bmv2backend
[ 58%] Building CXX object backends/bmv2/CMakeFiles/bmv2backend.dir/unified_bmv2_backend_common_srcs_2.cpp.o
[ 59%] Building CXX object backends/bmv2/CMakeFiles/bmv2backend.dir/unified_bmv2_backend_common_srcs_1.cpp.o
[ 61%] Linking CXX static library libbmv2backend.a
[ 61%] Built target bmv2backend
Makefile:138: recipe for target 'all' failed
make: *** [all] Error 2
p4@ubuntu:~/p4-tools/p4c/build$
**** DONE Build on notebook succeeds 900557c5
[16:37] line:p4c% git describe --always
900557c5
**** TODO Build on VM with 900557c5 after removing build/
** TODO Get p4 VM / vagrant running
*** DONE install libvirtd-daemon
*** DONE install ebtables
*** DONE install dnsmasq
** TODO Get p4c & co. running on the notebook
*** DONE mininet via packages
*** DONE p4c
(virtualenv-with-site) [17:43] line:build% make install
[  0%] Built target update_includes
[  0%] Built target linkgraphs
[  0%] Built target linkbmv2
[  0%] Built target linkp4cebpf
[  0%] Built target linkp4test
[  1%] Built target p4c_driver
[  4%] Built target p4ctoolkit
[ 12%] Built target irgenerator
[ 14%] Generating IR class files
[ 14%] Built target genIR
[ 18%] Built target ir
[ 18%] Built target mkv1dirs
[ 18%] Built target mkp4dirs
[ 45%] Built target frontend
[ 51%] Built target midend
[ 51%] Built target mkP4configdir
[ 64%] Built target controlplane
[ 68%] Built target bmv2backend
[ 75%] Built target p4c-bm2-psa
[ 81%] Built target p4c-bm2-ss
[ 84%] Built target p4c-ebpf
[ 87%] Built target p4test
[ 90%] Built target p4c-graphs
[ 93%] Built target gtest
[100%] Built target gtestp4c
Install the project...
-- Install configuration: "RELEASE"
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include/p4d2model.p4
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include/v1model.p4
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include/core.p4
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include/psa.p4
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/bin/p4c
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/driver.py
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/util.py
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/config.py
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/__init__.py
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/main.py
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/p4c.bmv2.cfg
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4c_src/p4c.ebpf.cfg
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/bin/p4c-bm2-ss
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/bin/p4c-bm2-psa
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/bin/p4c-ebpf
-- Up-to-date: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/share/p4c/p4include/ebpf_model.p4
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/bin/p4test
-- Installing: /home/nico/vcs/master-thesis/support/p4c-installation/bin/p4c-graphs
(virtualenv-with-site) [0:42] line:build% ls /home/nico/vcs/master-thesis/support/p4c-installation/bin/
p4c  p4c-bm2-psa  p4c-bm2-ss  p4c-ebpf  p4c-graphs  p4test
(virtualenv-with-site) [0:42] line:build%
*** TODO install behavioral-model

*** TODO Debug / reread the virtualbox script from the lecture
*** TODO Get p4c installed / running
    https://github.com/p4lang/p4c
**** log
[16:31] line:p4c%     git submodule update --init --recursive

root@line:~# apt install bison \
>              build-essential \
>              cmake \
>              flex \
>              g++ \
>              libboost-dev \
>              libboost-graph-dev \
>              libboost-iostreams1.58-dev \
>              libfl-dev \
>              libgc-dev \
>              libgmp-dev \
>              pkg-config \
>              python-ipaddr \
>              python-pip \
>              python-setuptools \
>              tcpdump
Reading package lists... Done
Building dependency tree
Reading state information... Done
Package libboost-iostreams1.58-dev is not available, but is referred to by another package.
This may mean that the package is missing, has been obsoleted, or
is only available from another source

E: Package 'libboost-iostreams1.58-dev' has no installation candidate
root@line:~# apt install libpcap-dev              libelf-dev              llvm              clang              iproute2              net-tools

[16:33] line:p4c% . ~/vcs/master-thesis/support/virtualenv2/bin/activate
(virtualenv2) [16:35] line:p4c% pip install tenjin \
                     pyroute2 \
                     ply==3.8 \
                     scapy==2.4.0
**** Using newer version of libboost-iostreams1.58-dev
**** buidling
(virtualenv2) [16:36] line:p4c%     mkdir build && \
    cd build && \
    cmake .. '-DCMAKE_CXX_FLAGS:STRING=-O3'
**** missing protobuf
(virtualenv2) [16:36] line:p4c%     mkdir build && \
    cd build && \
    cmake .. '-DCMAKE_CXX_FLAGS:STRING=-O3'

    cd build && \
    cmake .. '-DCMAKE_CXX_FLAGS:STRING=-O3'-- The C compiler identification is GNU 8.3.0
-- The CXX compiler identification is GNU 8.3.0
-- Check for working C compiler: /usr/bin/cc
-- Check for working C compiler: /usr/bin/cc -- works
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting C compile features
-- Detecting C compile features - done
-- Check for working CXX compiler: /usr/bin/c++
-- Check for working CXX compiler: /usr/bin/c++ -- works
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting CXX compile features
-- Detecting CXX compile features - done
-- Found PythonInterp: /home/nico/vcs/master-thesis/support/virtualenv2/bin/python (found version "2.7.16")
-- Found FLEX: /usr/bin/flex (found version "2.6.4")
-- Found BISON: /usr/bin/bison (found suitable version "3.3.2", minimum required is "3.0.2")
CMake Error at /usr/share/cmake-3.13/Modules/FindPackageHandleStandardArgs.cmake:137 (message):
  Could NOT find Protobuf (missing: Protobuf_INCLUDE_DIR) (Required is at
  least version "3.0.0")
Call Stack (most recent call first):
  /usr/share/cmake-3.13/Modules/FindPackageHandleStandardArgs.cmake:378 (_FPHSA_FAILURE_MESSAGE)
  /usr/share/cmake-3.13/Modules/FindProtobuf.cmake:595 (FIND_PACKAGE_HANDLE_STANDARD_ARGS)
  CMakeLists.txt:81 (find_package)


-- Configuring incomplete, errors occurred!
See also "/home/nico/vcs/master-thesis/support/p4c/build/CMakeFiles/CMakeOutput.log".
See also "/home/nico/vcs/master-thesis/support/p4c/build/CMakeFiles/CMakeError.log".
(virtualenv2) [16:36] line:build% apt search protobuf

(virtualenv2) [16:38] line:build% sudo apt install python-protobuf protobuf-compiler

(virtualenv2) [16:38] line:build%   cmake .. '-DCMAKE_CXX_FLAGS:STRING=-O3'
-- Found Protobuf: /usr/lib/x86_64-linux-gnu/libprotobuf.a;-lpthread (found suitable version "3.6.1", minimum required is "3.0.0")
-- Boost version: 1.67.0
-- Found the following Boost libraries:
--   iostreams
--   regex
-- Found LibGc: /usr/lib/x86_64-linux-gnu/libgccpp.so (found suitable version "7.6.4", minimum required is "7.2.0")
-- Found Threads: TRUE
-- Found LibGmp: /usr/lib/x86_64-linux-gnu/libgmpxx.so
-- Looking for clock_gettime in rt
-- Looking for clock_gettime in rt - found
-- Looking for execinfo.h
-- Looking for execinfo.h - found
-- Looking for ucontext.h
-- Looking for ucontext.h - found
-- Looking for C++ include cxxabi.h
-- Looking for C++ include cxxabi.h - found
-- Looking for memchr
-- Looking for memchr - found
-- Looking for pipe2
-- Looking for pipe2 - found
-- Looking for GC_print_stats
-- Looking for GC_print_stats - found
-- Found PY_difflib: /usr/lib/python2.7/difflib.pyc
-- Found PY_shutil: /usr/lib/python2.7/shutil.pyc
-- Found PY_tempfile: /usr/lib/python2.7/tempfile.pyc
-- Found PY_subprocess: /usr/lib/python2.7/subprocess.pyc
-- Found PY_re: /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/re.pyc
-- Could NOT find Doxygen (missing: DOXYGEN_EXECUTABLE)
-- Program 'simple_switch_CLI' (https://github.com/p4lang/behavioral-model.git) not found;
Searched .
Will not run BMv2 tests. (missing: SIMPLE_SWITCH SIMPLE_SWITCH_CLI)
-- Program 'psa_switch_CLI' (https://github.com/p4lang/behavioral-model.git) not found;
Searched .
Will not run PSA BMv2 tests. (missing: PSA_SWITCH PSA_SWITCH_CLI)
-- Performing Test _HAVE_OPTION_Wall_
-- Performing Test _HAVE_OPTION_Wall_ - Success
-- Performing Test _HAVE_OPTION_Wextra_
-- Performing Test _HAVE_OPTION_Wextra_ - Success
-- Performing Test _HAVE_OPTION_Wnooverloadedvirtual_
-- Performing Test _HAVE_OPTION_Wnooverloadedvirtual_ - Success
-- Performing Test _HAVE_OPTION_Wnodeprecated_
-- Performing Test _HAVE_OPTION_Wnodeprecated_ - Success
-- Using the GNU gold linker.
-- Available extensions
CMake Warning at backends/bmv2/CMakeLists.txt:193 (MESSAGE):
  BMv2 simple switch is not available, not adding v1model BMv2 tests


CMake Warning at backends/bmv2/CMakeLists.txt:199 (MESSAGE):
  BMv2 PSA switch is not available, not adding PSA BMv2 tests


-- Found LLVM 7.0.1
-- Added 14 tests to 'ebpf-kernel' (0 xfails)
-- Added 14 tests to 'ebpf-bcc' (0 xfails)
-- Added 14 tests to 'ebpf' (0 xfails)
-- Added 161 tests to 'p4' (0 xfails)
-- Added 506 tests to 'p4' (4 xfails)
-- Added 204 tests to 'p14_to_16' (0 xfails)
-- CTest parallel: -j 8
-- Configuring done
-- Generating done
-- Build files have been written to: /home/nico/vcs/master-thesis/support/p4c/build

**** testing in build directory: works
/home/nico/vcs/master-thesis/support/p4c/build
**** Changing install path

CMAKE_INSTALL_PREFIX
cmake .. '-DCMAKE_CXX_FLAGS:STRING=-O3' -DCMAKE_INSTALL_PREFIX=/home/nico/vcs/master-thesis/support/p4c-installation

*** TODO Get p4utils running (?)
*** log of python, p4app, p4c installation
[16:16] line:support% virtualenv virtualenv2
Running virtualenv with interpreter /usr/bin/python2
New python executable in /home/nico/vcs/master-thesis/support/virtualenv2/bin/python2
Also creating executable in /home/nico/vcs/master-thesis/support/virtualenv2/bin/python
Installing setuptools, pkg_resources, pip, wheel...done.
[16:16] line:support%

[16:18] line:p4-utils-nsg% . ~/vcs/master-thesis/support/virtualenv2/bin/activate
(virtualenv2) [16:19] line:p4-utils-nsg% which pip
/home/nico/vcs/master-thesis/support/virtualenv2/bin/pip
(virtualenv2) [16:19] line:p4-utils-nsg%
**** pip install -e .
***** Missing python development headers
    copying psutil/tests/test_memory_leaks.py -> build/lib.linux-x86_64-2.7/psutil/tests
    running build_ext
    building 'psutil._psutil_linux' extension
    creating build/temp.linux-x86_64-2.7
    creating build/temp.linux-x86_64-2.7/psutil
    x86_64-linux-gnu-gcc -pthread -DNDEBUG -g -fwrapv -O2 -Wall -Wstrict-prototypes -fno-strict-aliasing -Wdate-time -D_FORTIFY_SOURCE=2 -g -fdebug-prefix-map=/build/python2.7-UboFgi/python2.7-2.7.16~rc1=. -fstack-protector-strong -Wformat -Werror=format-security -fPIC -DPSUTIL_POSIX=1 -DPSUTIL_VERSION=561 -DPSUTIL_LINUX=1 -I/usr/include/python2.7 -c psutil/_psutil_common.c -o build/temp.linux-x86_64-2.7/psutil/_psutil_common.o
    psutil/_psutil_common.c:9:10: fatal error: Python.h: No such file or directory
     #include <Python.h>
              ^~~~~~~~~~
    compilation terminated.
    error: command 'x86_64-linux-gnu-gcc' failed with exit status 1


root@line:~# apt install python2-dev
***** installing, but missing mininet.net
(virtualenv2) [16:21] line:p4-utils-nsg%  pip install -e "."
DEPRECATION: Python 2.7 will reach the end of its life on January 1st, 2020. Please upgrade your Python as Python 2.7 won't be maintained after that date. A future version of pip will drop support for Python 2.7.
Obtaining file:///home/nico/vcs/master-thesis/support/p4-utils-nsg
Requirement already satisfied: setuptools in /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/site-packages (from p4utils==0.2) (40.8.0)
Requirement already satisfied: networkx in /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/site-packages (from p4utils==0.2) (2.2)
Requirement already satisfied: ipaddress in /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/site-packages (from p4utils==0.2) (1.0.22)
Requirement already satisfied: scapy in /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/site-packages (from p4utils==0.2) (2.4.2)
Requirement already satisfied: psutil in /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/site-packages (from p4utils==0.2) (5.6.1)
Requirement already satisfied: decorator>=4.3.0 in /home/nico/vcs/master-thesis/support/virtualenv2/lib/python2.7/site-packages (from networkx->p4utils==0.2) (4.3.2)
Installing collected packages: p4utils
  Found existing installation: p4utils 0.2
    Not uninstalling p4utils at /home/nico/vcs/master-thesis/support/p4-utils-nsg, outside environment /home/nico/vcs/master-thesis/support/virtualenv2
    Can't uninstall 'p4utils'. No files were found to uninstall.
  Running setup.py develop for p4utils
Successfully installed p4utils
(virtualenv2) [16:21] line:p4-utils-nsg%
*** log Try2: using virtualenv that uses site packages for using mininet
[17:13] line:support% virtualenv --system-site-packages virtualenv-with-site
Running virtualenv with interpreter /usr/bin/python2
New python executable in /home/nico/vcs/master-thesis/support/virtualenv-with-site/bin/python2
Also creating executable in /home/nico/vcs/master-thesis/support/virtualenv-with-site/bin/python
Installing setuptools, pkg_resources, pip, wheel...done.
[17:23] line:support% . ./virtualenv-with-site/bin/activate
(virtualenv-with-site) [17:23] line:support%
(virtualenv-with-site) [17:23] line:p4-utils-nsg% pip install -e .
(virtualenv-with-site) [17:23] line:p4-utils-nsg% pip install -e .
DEPRECATION: Python 2.7 will reach the end of its life on January 1st, 2020. Please upgrade your Python as Python 2.7 won't be maintained after that date. A future version of pip will drop support for Python 2.7.
Obtaining file:///home/nico/vcs/master-thesis/support/p4-utils-nsg
Requirement already satisfied: setuptools in /home/nico/vcs/master-thesis/support/virtualenv-with-site/lib/python2.7/site-packages (from p4utils==0.2) (40.8.0)
Collecting networkx (from p4utils==0.2)
Requirement already satisfied: ipaddress in /usr/lib/python2.7/dist-packages (from p4utils==0.2) (1.0.17)
Requirement already satisfied: scapy in /usr/lib/python2.7/dist-packages (from p4utils==0.2) (2.4.0)
Collecting psutil (from p4utils==0.2)
Collecting decorator>=4.3.0 (from networkx->p4utils==0.2)
  Using cached https://files.pythonhosted.org/packages/f1/cd/7c8240007e9716b14679bc217a1baefa4432aa30394f7e2ec40a52b1a708/decorator-4.3.2-py2.py3-none-any.whl
Installing collected packages: decorator, networkx, psutil, p4utils
  Running setup.py develop for p4utils
Successfully installed decorator-4.3.2 networkx-2.2 p4utils psutil-5.6.1
(virtualenv-with-site) [17:23] line:p4-utils-nsg% which p4run
/home/nico/vcs/master-thesis/support/virtualenv-with-site/bin/p4run
(virtualenv-with-site) [17:24] line:p4-utils-nsg%

p4c --target bmv2 --arch v1model --std p4-16 "../p4src/static-mapping.p4" -o "/home/nico/vcs/master-thesis/p4src"
../p4src/static-mapping.p4(80): [--Wwarn=unused] warning: Table ndp_answer is not used; removing
    table ndp_answer {
          ^^^^^^^^^^
../p4src/static-mapping.p4(96): [--Wwarn=unused] warning: Table port2mcast is not used; removing
    table port2mcast {
          ^^^^^^^^^^
../p4src/static-mapping.p4(111): [--Wwarn=unused] warning: Table addr2mcast is not used; removing
    table addr2mcast {
          ^^^^^^^^^^
../p4src/static-mapping.p4(128): [--Wwarn=unused] warning: Table ndp is not used; removing
    table ndp {
          ^^^
Switch port mapping:
s1:  1:h1	2:h2	3:h3	4:h4	5:sw-cpu
*** Trying local vagrant VM
**** libvirtd missing user
root@line:~# libvirtd
2019-03-12 16:39:14.556+0000: 20235: info : libvirt version: 5.0.0, package: 1 (Guido Günther <agx@sigxcpu.org> Wed, 16 Jan 2019 10:31:33 +0100)
2019-03-12 16:39:14.556+0000: 20235: info : hostname: line
2019-03-12 16:39:14.556+0000: 20235: error : virGetUserID:1038 : invalid argument: Failed to parse user 'libvirt-qemu'
2019-03-12 16:39:14.556+0000: 20235: error : virStateInitialize:662 : Initialization of QEMU state driver failed: invalid argument: Failed to parse user 'libvirt-qemu'
2019-03-12 16:39:14.556+0000: 20235: error : daemonRunStateInit:799 : Driver state initialization failed
root@line:~# useradd -m libvirt-qemu
root@line:~#

root@line:~# strace -fF -e open libvirtd
strace: deprecated option -F ignored
strace: Process 20602 attached
strace: Process 20603 attached
strace: Process 20604 attached
strace: Process 20605 attached
strace: Process 20606 attached
strace: Process 20607 attached
strace: Process 20608 attached
strace: Process 20609 attached
strace: Process 20610 attached
strace: Process 20611 attached
strace: Process 20612 attached
strace: Process 20613 attached
strace: Process 20614 attached
strace: Process 20615 attached
strace: Process 20616 attached
strace: Process 20617 attached
strace: Process 20618 attached
[pid 20618] +++ exited with 0 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20618, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20619 attached
[pid 20619] +++ exited with 0 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20619, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20620 attached
strace: Process 20621 attached
strace: Process 20622 attached
[pid 20622] +++ exited with 0 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20622, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20623 attached
[pid 20623] +++ exited with 0 +++
[pid 20621] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20623, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20624 attached
[pid 20624] +++ exited with 0 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20624, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20625 attached
[pid 20625] +++ exited with 0 +++
[pid 20617] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20625, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20626 attached
[pid 20626] +++ exited with 0 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20626, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20627 attached
[pid 20627] +++ exited with 0 +++
[pid 20617] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20627, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20628 attached
[pid 20621] +++ exited with 0 +++
strace: Process 20629 attached
strace: Process 20630 attached
strace: Process 20631 attached
strace: Process 20632 attached
strace: Process 20633 attached
[pid 20631] +++ exited with 0 +++
[pid 20633] +++ exited with 1 +++
[pid 20630] +++ exited with 0 +++
[pid 20628] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20630, si_uid=1001, si_status=0, si_utime=0, si_stime=0} ---
[pid 20632] +++ exited with 1 +++
[pid 20629] +++ exited with 1 +++
[pid 20628] +++ exited with 1 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20628, si_uid=1001, si_status=1, si_utime=1, si_stime=0} ---
2019-03-12 16:40:53.098+0000: 20617: info : libvirt version: 5.0.0, package: 1 (Guido Günther <agx@sigxcpu.org> Wed, 16 Jan 2019 10:31:33 +0100)
2019-03-12 16:40:53.098+0000: 20617: info : hostname: line
2019-03-12 16:40:53.098+0000: 20617: error : virQEMUCapsNewForBinaryInternal:4681 : internal error: Failed to probe QEMU binary with QMP: qemu-system-i386: cannot create PID file: Cannot open pid file: Permission denied

2019-03-12 16:40:53.098+0000: 20617: warning : virQEMUCapsLogProbeFailure:4628 : Failed to probe capabilities for /usr/bin/qemu-system-i386: internal error: Failed to probe QEMU binary with QMP: qemu-system-i386: cannot create PID file: Cannot open pid file: Permission denied

strace: Process 20634 attached
strace: Process 20635 attached
strace: Process 20636 attached
strace: Process 20637 attached
strace: Process 20638 attached
strace: Process 20639 attached
[pid 20637] +++ exited with 0 +++
[pid 20639] +++ exited with 1 +++
[pid 20636] +++ exited with 0 +++
[pid 20634] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20636, si_uid=1001, si_status=0, si_utime=0, si_stime=0} ---
[pid 20638] +++ exited with 1 +++
[pid 20635] +++ exited with 1 +++
[pid 20634] +++ exited with 1 +++
[pid 20617] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20634, si_uid=1001, si_status=1, si_utime=1, si_stime=0} ---
2019-03-12 16:40:53.145+0000: 20617: error : virQEMUCapsNewForBinaryInternal:4681 : internal error: Failed to probe QEMU binary with QMP: qemu-system-x86_64: cannot create PID file: Cannot open pid file: Permission denied

2019-03-12 16:40:53.145+0000: 20617: warning : virQEMUCapsLogProbeFailure:4628 : Failed to probe capabilities for /usr/bin/qemu-system-x86_64: internal error: Failed to probe QEMU binary with QMP: qemu-system-x86_64: cannot create PID file: Cannot open pid file: Permission denied

strace: Process 20640 attached
[pid 20640] +++ exited with 0 +++
[pid 20617] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20640, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20641 attached
[pid 20641] +++ exited with 0 +++
[pid 20617] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20641, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
strace: Process 20642 attached
[pid 20642] +++ exited with 2 +++
[pid 20601] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20642, si_uid=0, si_status=2, si_utime=0, si_stime=0} ---
strace: Process 20643 attached
[pid 20643] +++ exited with 0 +++
[pid 20617] --- SIGCHLD {si_signo=SIGCHLD, si_code=CLD_EXITED, si_pid=20643, si_uid=0, si_status=0, si_utime=0, si_stime=0} ---
[pid 20617] +++ exited with 0 +++
[pid 20601] --- SIGWINCH {si_signo=SIGWINCH, si_code=SI_KERNEL} ---
^Cstrace: Process 20601 detached
strace: Process 20602 detached
strace: Process 20603 detached
strace: Process 20604 detached
strace: Process 20605 detached
strace: Process 20606 detached
strace: Process 20607 detached
strace: Process 20608 detached
strace: Process 20609 detached
strace: Process 20610 detached
strace: Process 20611 detached
strace: Process 20612 detached
strace: Process 20613 detached
strace: Process 20614 detached
strace: Process 20615 detached
strace: Process 20616 detached
strace: Process 20620 detached
*** Creating network
*** Adding hosts:
h1 h2 h3 h4
*** Adding switches:
Cannot find required executable simple_switch.
Please make sure that it is installed and available in your $PATH:
(/home/nico/vcs/master-thesis/support/virtualenv-with-site/bin:/usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin:/home/nico/vcs/master-thesis/support/p4c/build/)
(virtualenv-with-site) root@line:/home/nico/vcs/master-thesis/p4app#
** TODO Setup test VM [dual stack] for Jool:
** TODO Setup test VM [dual stack] for tayga:
** TODO Port to Hardware
*** NetPFGA documentation
**** Port mapping
| 1 | nf0 |
*** DONE Get access to tofino: no, NDA issues
*** DONE Get NetFPGA running
**** DONE Understand the simulations part -> not atm
**** DONE Install vivado
**** DONE Install SDNET

**** DONE fix license issue
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/testdata'
echo ok
ok
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/testdata'
sdnet ./src/switch_calc.sdnet -skipEval -busType axi -busWidth 256 -singlecontrolport -workDir nf_sume_sdnet_ip -altVivadoScripts
Xilinx SDNet Compiler version 2018.2, build 2342300

Cannot obtain license
make: *** [Makefile:67: compile_no_cpp_test] Error 1
nico@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc$

**** TODO Testing / compiling / uploading stuff to the NetPFGA --
     https://github.com/NetFPGA/P4-NetFPGA-public/wiki/Tutorial-Assignments
***** DONE try 1
      According to
 DO NOT USE THIS:: ==> https://github.com/NetFPGA/NetFPGA-SUME-public/wiki/NetFPGA-SUME-Reference-Learning-Switch

 root@loch:~/projects/P4-NetFPGA/tools/scripts# ./nf_test.py hw --major learning --minor sw
 Please set the environment variable 'SUME_FOLDER' to point to the local NetFPGA source
 Traceback (most recent call last):
   File "./nf_test.py", line 632, in <module>
     identifyWorkDir()
   File "./nf_test.py", line 418, in identifyWorkDir
     project = os.path.basename(os.path.abspath(os.environ['NF_DESIGN_DIR']))
   File "/usr/lib/python2.7/UserDict.py", line 40, in __getitem__
     raise KeyError(key)
 KeyError: 'NF_DESIGN_DIR'
 root@loch:~/projects/P4-NetFPGA/tools/scripts#

 Trying
 https://github.com/NetFPGA/P4-NetFPGA-public/wiki/Tutorial-Assignments

 root@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src# mv switch_calc.p4 switch_calc_orig.p4
 root@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src# ln -s switch_calc_solution.p4 switch_calc.p4
 root@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src#

 root@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc# make
 make -C src/ clean
 make[1]: Entering directory '/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 rm -f *.sdnet *.tbl .sdnet_switch_info.dat
 make[1]: Leaving directory '/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 make -C testdata/ clean
 make[1]: Entering directory '/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/testdata'
 rm -f *.pcap *.txt *.pyc *.axi config_writes.* *_reg_defines.py
 make[1]: Leaving directory '/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/testdata'
 rm -rf nf_sume_sdnet_ip/
 rm -f
 rm -f sw/config_tables.c
 make -C src/
 make[1]: Entering directory '/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 p4c-sdnet -o .sdnet --sdnet_info .sdnet_switch_info.dat _solution.p4
 make[1]: p4c-sdnet: Command not found
 make[1]: *** [Makefile:34: all] Error 127
 make[1]: Leaving directory '/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 make: *** [Makefile:60: frontend] Error 2
 root@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc#

 As nico:

 nico@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc$ make
 make -C src/ clean
 make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 rm -f *.sdnet *.tbl .sdnet_switch_info.dat
 make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 make -C testdata/ clean
 make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/testdata'
 rm -f *.pcap *.txt *.pyc *.axi config_writes.* *_reg_defines.py
 make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/testdata'
 rm -rf nf_sume_sdnet_ip/
 rm -f
 rm -f sw/config_tables.c
 make -C src/
 make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 p4c-sdnet -o switch_calc.sdnet --sdnet_info .sdnet_switch_info.dat switch_calc_solution.p4
 cpp: error: switch_calc_solution.p4: No such file or directory
 cpp: warning: ‘-x c’ after last input file has no effect
 cpp: fatal error: no input files
 compilation terminated.
 error: Preprocessor returned exit code 256; aborting compilation
 error: 1 errors encountered, aborting compilation
 make[1]: *** [Makefile:34: all] Error 1
 make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src'
 make: *** [Makefile:60: frontend] Error 2
 nico@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc$

 nico@loch:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/switch_calc/src$ cp switch_calc.p4 switch_calc_solution.p4

 $ cd $P4_PROJECT_DIR/nf_sume_sdnet_ip/SimpleSumeSwitch

 $ ./vivado_sim.bash.

***** DONE try 2: create an almost empty p4 project based on switch_calc
****** DONE frontend build: ok
****** DONE testdata: skipped
****** DONE compile_cpp_test: ok
****** DONE run_scripts: ok
****** TODO cpp_test: error
# Fix introduced for SDNet 2017.4
sed -i 's/xsim\.dir\/xsc\/dpi\.so/dpi\.so/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim.bash
sed -i 's/xsim\.dir\/xsc\/dpi\.so/dpi\.so/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
# Fix introduced for SDNet 2018.2
sed -i 's/glbl_sim/glbl/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
sed -i 's/SimpleSumeSwitch_tb_sim#work.glbl/SimpleSumeSwitch_tb/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
cp src/*.tbl nf_sume_sdnet_ip/SimpleSumeSwitch/
cp: cannot stat 'src/*.tbl': No such file or directory
make: *** [Makefile:23: cpp_test] Error 1
[23:12] loch:minip4%
******* DONE Removing cp of *tbl
******* DONE Removing pcap copy
******* TODO removing all cp's
***** DONE try 3: good until step 4; broken at the simulation
****** log 1
 [15:26] rainbow:~% echo $P4_PROJECT_DIR
 /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4
 [15:26] rainbow:~%
 [15:26] rainbow:~% cd $P4_PROJECT_DIR && make

 Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
 Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
 Compiling module work.S_SYNCER_for_S_SYNCER_for_TopDep...
 Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
 Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
 Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=1...
 Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
 Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
 Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
 Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
 Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
 Compiling module work.S_SYNCER_for_TopDeparser
 Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
 Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
 Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
 Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
 Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
 Compiling module work.S_SYNCER_for__OUT_
 Compiling module work.S_CONTROLLER_SimpleSumeSwitch
 Compiling module work.SimpleSumeSwitch
 Compiling module work.TB_System_Stim
 Compiling module work.Check
 Compiling module work.SimpleSumeSwitch_tb
 Compiling module work.glbl
 ERROR: [XSIM 43-3409] Failed to compile generated C file xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/obj/xsim_3.c.
 ERROR: [XSIM 43-3915] Encountered a fatal error. Cannot continue. Exiting...
 [15:29] rainbow:SimpleSumeSwitch% ./vivado_sim.bash
****** trying to find the error in the generated c code
[15:29] rainbow:SimpleSumeSwitch% find . -name xsim_3.c
./xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/obj/xsim_3.c
****** error seems to occur in xelab
***** DONE try 4: vivado 2018.2 instead of 2018.3
      Probably both ok - errors are the same
***** DONE new error: /usr/include/stdio.h:27:36: fatal error: bits/libc-header-start.h: No such file or directory
apt-get install gcc-multilib g++-multilib
***** DONE same error
Compiling module work.glbl
ERROR: [XSIM 43-3409] Failed to compile generated C file xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/obj/xsim_3.c.
ERROR: [XSIM 43-3915] Encountered a fatal error. Cannot continue. Exiting...
[17:47] rainbow:SimpleSumeSwitch%
***** DONE with verbosity / fixing ncurses dependency

ICR Memory Usage: 5072KB, 18432KB
/opt/Xilinx/Vivado/2018.2/data/../tps/llvm/3.1/lnx64.o/bin/clang  -fPIC -c -std=gnu89 -nobuiltininc -nostdinc++ -w  -Wl,--unres
olved-symbols=ignore-in-object-files -fbracket-depth=1048576 -I/opt/Xilinx/Vivado/2018.2/data/../tps/llvm/3.1/lnx64.o/bin/../li
b/clang/3.1/include -fPIC -m64  -I"/opt/Xilinx/Vivado/2018.2/data/xsim/include" "xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/ob
j/xsim_3.c" -O0 -sim -o "xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/obj/xsim_3.lnx64.o" -DXILINX_SIMULATOR
/opt/Xilinx/Vivado/2018.2/data/../tps/llvm/3.1/lnx64.o/bin/clang: error while loading shared libraries: libncurses.so.5: cannot
 open shared object file: No such file or directory
ERROR: [XSIM 43-3409] Failed to compile generated C file xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/obj/xsim_3.c.
ERROR: [XSIM 43-3915] Encountered a fatal error. Cannot continue. Exiting...
[20:00] rainbow:SimpleSumeSwitch%

root@rainbow:~# apt install libncurses5-dev


[20:02] rainbow:~% ldd /opt/Xilinx/Vivado/2018.2/data/../tps/llvm/3.1/lnx64.o/bin/clang
        linux-vdso.so.1 (0x00007ffda6bf6000)
        libz.so.1 => /lib/x86_64-linux-gnu/libz.so.1 (0x00007f8e23208000)
        libpthread.so.0 => /lib/x86_64-linux-gnu/libpthread.so.0 (0x00007f8e231e7000)
        libncurses.so.5 => not found
        librt.so.1 => /lib/x86_64-linux-gnu/librt.so.1 (0x00007f8e231dc000)
        libdl.so.2 => /lib/x86_64-linux-gnu/libdl.so.2 (0x00007f8e231d6000)
        libstdc++.so.6 => /lib/x86_64-linux-gnu/libstdc++.so.6 (0x00007f8e22ff5000)
        libm.so.6 => /lib/x86_64-linux-gnu/libm.so.6 (0x00007f8e22ea5000)
        libgcc_s.so.1 => /lib/x86_64-linux-gnu/libgcc_s.so.1 (0x00007f8e22e8b000)
        libc.so.6 => /lib/x86_64-linux-gnu/libc.so.6 (0x00007f8e22ca0000)
        /lib64/ld-linux-x86-64.so.2 (0x00007f8e2323f000)
[20:02] rainbow:~%

root@rainbow:~# apt install libncurses5

***** DONE Run step 4: ok fully works now with switch_calc_headrs and gen_testdata
****** command
cd $P4_PROJECT_DIR && make
****** DONE commented out the test data step to progress
****** TODO re-enable test data cp step => data required later
all: clean frontend compile_no_cpp_test run_scripts
	cp src/*.tbl ${SDNET_OUT_DIR}/${P4_SWITCH}/
	cp testdata/*.txt ${SDNET_OUT_DIR}/${P4_SWITCH}/
	cp testdata/*.axi ${SDNET_OUT_DIR}/${P4_SWITCH}/

# Fix introduced for SDNet 2018.2
sed -i 's/glbl_sim/glbl/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
sed -i 's/SimpleSumeSwitch_tb_sim#work.glbl/SimpleSumeSwitch_tb/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
cp src/*.tbl nf_sume_sdnet_ip/SimpleSumeSwitch/
cp testdata/*.txt nf_sume_sdnet_ip/SimpleSumeSwitch/
cp: cannot stat 'testdata/*.txt': No such file or directory
make: *** [Makefile:17: all] Error 1
[15:46] rainbow:minip4%

In testdata/Makefile:

all:
	echo ok

all2:
	./gen_testdata.py
	${SUME_SDNET}/bin/pcap2axi --output Packet_in.axi --bus_width 256 src.pcap
	${SUME_SDNET}/bin/pcap2axi --output Packet_expect.axi --bus_width 256 dst.pcap

Changing back to all:

make -C testdata/
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata'
./gen_testdata.py
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/pcap2axi --output Packet_in.axi --bus_width 256 src.pcap
Traceback (most recent call last):
  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/pcap2axi", line 108, in <module>
    write_to_file(args.file_pcap, args.output)
  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/pcap2axi", line 88, in write_to_file
    for pkt in rdpcap(file_in):
  File "/usr/lib/python2.7/dist-packages/scapy/utils.py", line 728, in rdpcap
    with PcapReader(filename) as fdesc:
  File "/usr/lib/python2.7/dist-packages/scapy/utils.py", line 751, in __call__
    filename, fdesc, magic = cls.open(filename)
  File "/usr/lib/python2.7/dist-packages/scapy/utils.py", line 778, in open
    fdesc = open(filename, "rb")
IOError: [Errno 2] No such file or directory: 'src.pcap'
make[1]: *** [Makefile:5: all] Error 1
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata'
make: *** [Makefile:32: frontend] Error 2
[15:47] rainbow:minip4%
****** TODO debug gen_testdata.py
***** DONE Run step 5: ok
****** command
#+BEGIN_EXAMPLE
cd $P4_PROJECT_DIR/nf_sume_sdnet_ip/SimpleSumeSwitch && ./vivado_sim.bash
#+END_EXAMPLE
***** DONE Run step 6: ok => config_writes
****** command
#+BEGIN_CENTER
cd $P4_PROJECT_DIR && make config_writes
#+END_CENTER
***** DONE Run step 7: ok - install sume library core
****** command
#+BEGIN_CENTER
cd $P4_PROJECT_DIR && make uninstall_sdnet && make install_sdnet
#+END_CENTER
****** log
 # set_property value_format {long} [ipx::get_user_parameter SDNET_ADDR_WIDTH [ipx::current_core]]
 # ipx::add_subcore xilinx.com:ip:axis_data_fifo:1.1 [ipx::get_file_groups xilinx_anylanguagesynthesis -of_objects [ipx::current_core]]
 # ipx::add_subcore xilinx.com:ip:axis_data_fifo:1.1 [ipx::get_file_groups xilinx_anylanguagebehavioralsimulation -of_objects [ipx::current_core]]
 # ipx::add_bus_parameter FREQ_HZ [ipx::get_bus_interfaces m_axis -of_objects [ipx::current_core]]
 # ipx::add_bus_parameter FREQ_HZ [ipx::get_bus_interfaces s_axis -of_objects [ipx::current_core]]
 # update_ip_catalog -rebuild
 INFO: [IP_Flow 19-234] Refreshing IP repositories
 INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/lib/hw'.
 WARNING: [IP_Flow 19-3656] If you move the project, the path for repository '/home/nico/projects/P4-NetFPGA/lib/hw' may become invalid. A better location for the repository would be in a path adjacent to the project. (Current project location is '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj'.)
 # ipx::infer_user_parameters [ipx::current_core]
 # ipx::check_integrity [ipx::current_core]
 INFO: [IP_Flow 19-861] XGUI layout file basename "xgui/nf_sume_sdnet_v1_0.tcl" does not have the current IP <name>_v<version> format. If the IP name or version was changed recently, recreate this file to update the file format.
 INFO: [IP_Flow 19-2181] Payment Required is not set for this core.
 INFO: [IP_Flow 19-2187] The Product Guide file is missing.
 INFO: [Ipptcl 7-1486] check_integrity: Integrity check passed.
 # ipx::save_core [ipx::current_core]
 # update_ip_catalog
 # close_project
 INFO: [Common 17-206] Exiting Vivado at Sat May 18 15:18:13 2019...
 make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip'
 [15:18] rainbow:minip4%  cd $P4_PROJECT_DIR && make uninstall_sdnet && make install_sdnet

***** DONE run step 8: just copies a python script
****** run command
#+BEGIN_CENTER
cd $NF_DESIGN_DIR/test/sim_switch_default && make
#+END_CENTER
****** log
 [15:18] rainbow:minip4% cd $NF_DESIGN_DIR/test/sim_switch_default && make
 rm -f config_writes.py*
 rm -f *.pyc
 cp /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata/config_writes.py ./
 [15:18] rainbow:sim_switch_default%
***** DONE run step 9: ok sume simulation: fails with various errors, python and cp failures
****** DONE run command
#+BEGIN_CENTER
cd $SUME_FOLDER && ./tools/scripts/nf_test.py sim --major switch --minor default
#+END_CENTER

****** DONE python indent bug
# update_compile_order -fileset sim_1
update_compile_order: Time (s): cpu = 00:00:17 ; elapsed = 00:00:09 . Memory (MB): peak = 1995.594 ; gain = 0.016 ; free physic
al = 21975 ; free virtual = 33161
loading libsume..
Traceback (most recent call last):
  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_de
fault/run.py", line 42, in <module>
    import config_writes
  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_de
fault/config_writes.py", line 7

                        ^
IndentationError: expected an indented block
    while executing
"exec python $::env(NF_DESIGN_DIR)/test/${test_name}/run.py"
    invoked from within
"set output [exec python $::env(NF_DESIGN_DIR)/test/${test_name}/run.py]"
    (file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_s
ume_switch_sim.tcl" line 177)
INFO: [Common 17-206] Exiting Vivado at Sat May 18 15:21:21 2019...

-> inserting pass in def config_tables()
****** DONE post python cp error: different error after fixing python
=== Work directory is /tmp/nico/test/simple_sume_switch
=== Setting up test in /tmp/nico/test/simple_sume_switch/sim_switch_default
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_0_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_0_stim.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_0_expected.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_1_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_1_stim.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_1_expected.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_2_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_2_stim.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_2_expected.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_3_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_3_stim.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_3_expected.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/dma_0_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/dma_0_expected.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/reg_stim.log': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/reg_expect.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/reg_stim.axi': No such file or directory
=== Running test /tmp/nico/test/simple_sume_switch/sim_switch_default ... using cmd ['/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/run.py', '--sim', 'xsim']
[15:21] rainbow:P4-NetFPGA%
****** DONE "add_wave failed" (post python fix) -> go back to step 4
# add_wave $nf_sume_sdnet_ip/out_src_port
# add_wave $nf_sume_sdnet_ip/out_dst_port
# set const_reg_ip /top_tb/top_sim/nf_datapath_0/nf_sume_sdnet_wrapper_1/inst/SimpleSumeSwitch_inst/const_reg_rw_0/
# add_wave_divider {const reg extern signals}
# add_wave $const_reg_ip
ERROR: [Wavedata 42-471] Note: Nothing was found for the following items: /top_tb/top_sim/nf_datapath_0/nf_sume_sdnet_wrapper_1/inst/SimpleSumeSwitch_inst/const_reg_rw_0/
ERROR: [Common 17-39] 'add_wave' failed due to earlier errors.

    while executing
"add_wave $const_reg_ip "
    (file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_sim.tcl" line 328)
INFO: [Common 17-206] Exiting Vivado at Sat May 18 15:31:59 2019...
make: *** [Makefile:121: sim] Error 1
make: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test'
512
=== Work directory is /tmp/nico/test/simple_sume_switch
=== Setting up test in /tmp/nico/test/simple_sume_switch/sim_switch_default
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_0_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_1_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_2_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_3_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/dma_0_log.axi': No such file or directory
=== Running test /tmp/nico/test/simple_sume_switch/sim_switch_default ... using cmd ['/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/run.py', '--sim', 'xsim']
[15:31] rainbow:P4-NetFPGA%
***** DONE run step 10: compiling the bitstream [takes hours]
****** command
#+BEGIN_CENTER
cd $NF_DESIGN_DIR && make

# or

cd $NF_DESIGN_DIR && make 2>&1 | tee compilelog

#+END_CENTER
****** log
 Ignoring previous errors and continuing with this step => does not
 work, ends with:

 #+BEGIN_CENTER
 Opening simple_sume_switch XPR project

 # open_project project/$design.xpr
 Scanning sources...
 Finished scanning sources
 INFO: [IP_Flow 19-234] Refreshing IP repositories
 INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/ip_repo'.
 INFO: [IP_Flow 19-2313] Loaded Vivado IP repository '/opt/Xilinx/Vivado/2018.2/data/ip'.
 # puts "\nOpening $design Implementation design\n"

 Opening simple_sume_switch Implementation design

 # open_run impl_1
 ERROR: [Common 17-69] Command failed: Run 'impl_1' has not been launched. Unable to open
 Vivado%
 #+END_CENTER
****** DONE try 2: Run 'impl_1' has not been launched. Unable to open
#+BEGIN_CENTER

export simple_sume_switch project to SDK

 ****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source tcl/export_hardware.tcl
# set design [lindex $argv 0]
# puts "\nOpening $design XPR project\n"

Opening simple_sume_switch XPR project

# open_project project/$design.xpr
Scanning sources...
Finished scanning sources
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/ip_repo'.
INFO: [IP_Flow 19-2313] Loaded Vivado IP repository '/opt/Xilinx/Vivado/2018.2/data/ip'.
# puts "\nOpening $design Implementation design\n"

Opening simple_sume_switch Implementation design

# open_run impl_1
ERROR: [Common 17-69] Command failed: Run 'impl_1' has not been launched. Unable to open
Vivado%
#+END_CENTER
****** DONE try3: debug the REAL failing command
******* command
 #+BEGIN_CENTER
 vivado -mode batch -source tcl/simple_sume_switch.tcl
 #+END_CENTER
******* log
#+BEGIN_CENTER
ERROR: [BD 41-171] The modes of the interface pins 'cfg_interrupt'(Slave) and 'pcie3_cfg_interrupt'(Slave) are incompatible. They cannot be connected.
ERROR: [BD 5-3] Error: running connect_bd_intf_net.
ERROR: [Common 17-39] 'connect_bd_intf_net' failed due to earlier errors.

    while executing
"connect_bd_intf_net -intf_net nf_riffa_dma_1_pcie3_cfg_interrupt [get_bd_intf_pins nf_riffa_dma_1/cfg_interrupt] [get_bd_intf_pins pcie3_7x_1/pcie3_cf..."
    (procedure "create_hier_cell_dma_sub" line 141)
    invoked from within
"create_hier_cell_dma_sub [current_bd_instance .] dma_sub"
    (procedure "create_root_design" line 68)
    invoked from within
"create_root_design """
    (file "./tcl/control_sub.tcl" line 729)

    while executing
"source ./tcl/control_sub.tcl"
    (file "tcl/simple_sume_switch.tcl" line 89)

.... after bugfixing:

Creating bitmap...
Creating bitstream...
Bitstream compression saved 132634496 bits.
Writing bitstream ../bitfiles/simple_sume_switch.bit...
INFO: [Vivado 12-1842] Bitgen Completed Successfully.
INFO: [Common 17-83] Releasing license: Implementation
100 Infos, 51 Warnings, 1 Critical Warnings and 0 Errors encountered.
write_bitstream completed successfully
write_bitstream: Time (s): cpu = 00:02:39 ; elapsed = 00:03:20 . Memory (MB): peak = 4301.938 ; gain = 944.953 ; free physical
= 23157 ; free virtual = 31451
# exit
INFO: [Common 17-206] Exiting Vivado at Mon May 20 13:07:53 2019...
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
[13:07] rainbow:simple_sume_switch%
#+END_CENTER
******* TODO clarifying "simple_sume_switch.tcl"
******** DONE What is it?
Seems to be some kind of batch system for vivado
******** DONE Who or what created it?
Seems to be manually / from the project / not generated
******** DONE What is it trying to do?
Assuming connecting "things" on the "board".
******** DONE Why is it incompatible?
******** DONE Trying to resolve the error 1: commenting out line 538
# connect_bd_intf_net -intf_net nf_riffa_dma_1_pcie3_cfg_interrupt
 [get_bd_intf_pins nf_riffa_dma_1/cfg_interrupt] [get_bd_intf_pins
 pcie3_7x_1/pcie3_cfg_interrupt]

****** DONE try4 going back to step 10 -> fails
#+BEGIN_CENTER
ume_switch/hw/project/simple_sume_switch.runs/control_sub_m00_data_fifo_0_synth_1/runme.log
control_sub_s00_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_s00_data_fifo_0_synth_1/runme.log
control_sub_auto_cc_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_auto_cc_0_synth_1/runme.log
synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/synth_1/runme.log
[Fri May 24 11:55:57 2019] Launched impl_1...
Run output will be captured here: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/impl_1/runme.log
launch_runs: Time (s): cpu = 00:00:34 ; elapsed = 00:01:10 . Memory (MB): peak = 2538.609 ; gain = 1199.879 ; free physical = 28377 ; free virtual = 34012
# wait_on_run impl_1
[Fri May 24 11:55:57 2019] Waiting for impl_1 to finish...
[Fri May 24 12:39:07 2019] impl_1 finished
wait_on_run: Time (s): cpu = 00:26:26 ; elapsed = 00:43:10 . Memory (MB): peak = 2538.609 ; gain = 0.000 ; free physical = 28208 ; free virtual = 34003
# open_run impl_1
ERROR: [Common 17-69] Command failed: Run 'impl_1' has not been launched. Unable to open
Vivado% q
#+END_CENTER

****** DONE try5: error: No IP matching VLNV 'NetFPGA:NetFPGA:nf_sume_sdnet:*' was found
#+BEGIN_CENTER
[11:52] rainbow:hw%  vivado -mode batch -source tcl/simple_sume_switch.tcl
...

### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd>
# create_ip -name nf_sume_sdnet -vendor NetFPGA -library NetFPGA -module_name nf_sume_sdnet_ip
ERROR: [Coretcl 2-1134] No IP matching VLNV 'NetFPGA:NetFPGA:nf_sume_sdnet:*' was found. Please check your repository configuration.
INFO: [Common 17-206] Exiting Vivado at Sat May 25 11:52:01 2019...

#+END_CENTER

****** DONE try6: go back to clean netpfga-live, diff all sources
#+BEGIN_CENTER


[13:44] rainbow:~% diff -ru ~/P4-NetFPGA-live-clean/tools ~/projects/P4-NetFPGA/tools
Only in /home/nico/projects/P4-NetFPGA/tools/scripts/NFTest: testcheck.pyc
diff -ru /home/nico/P4-NetFPGA-live-clean/tools/settings.sh /home/nico/projects/P4-NetFPGA/tools/settings.sh
--- /home/nico/P4-NetFPGA-live-clean/tools/settings.sh  2019-05-25 11:55:45.655636066 +0200
+++ /home/nico/projects/P4-NetFPGA/tools/settings.sh    2019-05-13 11:49:02.122265641 +0200
@@ -28,7 +28,8 @@
 # @NETFPGA_LICENSE_HEADER_END@
 #

-export P4_PROJECT_NAME=switch_calc
+export P4_PROJECT_NAME=switch_calc
+export P4_PROJECT_NAME=minip4
 export NF_PROJECT_NAME=simple_sume_switch
 export SUME_FOLDER=${HOME}/projects/P4-NetFPGA
 export SUME_SDNET=${SUME_FOLDER}/contrib-projects/sume-sdnet-switch
@@ -47,4 +48,3 @@
 export DRIVER_FOLDER=${SUME_FOLDER}/lib/sw/std/driver/${DRIVER_NAME}
 export APPS_FOLDER=${SUME_FOLDER}/lib/sw/std/apps/${DRIVER_NAME}
 export HWTESTLIB_FOLDER=${SUME_FOLDER}/lib/sw/std/hwtestlib
-
[13:44] rainbow:~%

#+END_CENTER

****** DONE try7: restart from beginning in minip4 alongside try6
       - steps 1...8 ok
       - step 9: fails to cp axi files
       - step 9: before that a python error
****** DONE try8: fix python error in config_writes.py: script is generated
#+BEGIN_CENTER
# set_property compxlib.xsim_compiled_library_dir {} [current_project]                                                 [0/1819]
# set_property top_lib xil_defaultlib [get_filesets sim_1]
# update_compile_order -fileset sim_1
update_compile_order: Time (s): cpu = 00:00:17 ; elapsed = 00:00:09 . Memory (MB): peak = 2003.578 ; gain = 8.004 ; free physical = 27661 ; free virtual = 33990
loading libsume..
Traceback (most recent call last):
  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/run.py", line 42, in <module>
    import config_writes
  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/config_writes.py", line 7

                        ^
IndentationError: expected an indented block
    while executing
"exec python $::env(NF_DESIGN_DIR)/test/${test_name}/run.py"
    invoked from within
"set output [exec python $::env(NF_DESIGN_DIR)/test/${test_name}/run.py]"
    (file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_sim.tcl" line 177)
INFO: [Common 17-206] Exiting Vivado at Sat May 25 13:45:13 2019...
make: *** [Makefile:121: sim] Error 1
make: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test'
512
=== Work directory is /tmp/nico/test/simple_sume_switch
=== Setting up test in /tmp/nico/test/simple_sume_switch/sim_switch_default
#+END_CENTER

config_writes.py
#+BEGIN_CENTER
[13:50] rainbow:~% find ~/P4-NetFPGA-live-clean -name config_writes.py
[13:50] rainbow:~%

#+END_CENTER
******* File does not EXIST in original repo -> might be created in step6?
"Generate the scripts that can be used in the NetFPGA SUME simulations to configure the table entries.

$ cd $P4_PROJECT_DIR && make config_writes
"

#+BEGIN_CENTER!
[13:50] rainbow:~% find ~/projects/P4-NetFPGA -name config_writes.py
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata/config_writes.py
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/config_writes.py
[13:53] rainbow:~%

[13:53] rainbow:~% grep -r config_writes.py /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/vivado.log:  File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/config_writes.py", line 7
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/Makefile: cp ${P4_PROJECT_DIR}/testdata/config_writes.py ./
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/Makefile: rm -f config_writes.py*
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_ctrlWrites/Makefile:      cp ${P4_PROJECT_DIR}/testdata/config_writes.py ./
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_ctrlWrites/Makefile:      rm -f config_writes.py*
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/Makefile:     ${SUME_SDNET}/bin/gen_config_writes.py ${SDNET_OUT_DIR}/${P4_SWITCH}/config_writes.txt ${P4_SWITCH_BASE_ADDR} testdata
[13:56] rainbow:~%

#+END_CENTER

Likely:

/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/Makefile:     ${SUME_SDNET}/bin/gen_config_writes.py ${SDNET_OUT_DIR}/${P4_SWITCH}/config_writes.txt ${P4_SWITCH_BASE_ADDR} testdata

/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch
[14:01] rainbow:sume-sdnet-switch% ls bin
conv_p414_cmds            gen_P4_SWITCH_externs.py  libtcam_templates.pyc       nf_sim_tools.pyc
extern_data.py            gen_P4_SWITCH_regs.py     make_config_tables.py       p4_px_tables.py
extern_data.pyc           libcam_templates.py       make_new_p4_proj.py         pcap2axi
gen_config_fsm_writes.py  libcam_templates.pyc      make_regs_addressable.py    sss_sume_metadata.py
gen_config_writes.py      liblpm_templates.py       modify_P4_SWITCH_tb.py      sss_sume_metadata.pyc
gen_P4_SWITCH_API.py      liblpm_templates.pyc      nf_sim_compare_axi_logs.py
gen_P4_SWITCH_CLI.py      libtcam_templates.py      nf_sim_tools.py
[14:01] rainbow:sume-sdnet-switch%

sim_config = 'config_writes.py'
hw_config = 'config_writes.sh'

****** DONE try9: debug the script that generates the script that generates the error
#+BEGIN_CENTER
[14:01] rainbow:sume-sdnet-switch% pwd
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch
[14:01] rainbow:sume-sdnet-switch% ls bin
conv_p414_cmds            gen_P4_SWITCH_externs.py  libtcam_templates.pyc       nf_sim_tools.pyc
extern_data.py            gen_P4_SWITCH_regs.py     make_config_tables.py       p4_px_tables.py
extern_data.pyc           libcam_templates.py       make_new_p4_proj.py         pcap2axi
gen_config_fsm_writes.py  libcam_templates.pyc      make_regs_addressable.py    sss_sume_metadata.py
gen_config_writes.py      liblpm_templates.py       modify_P4_SWITCH_tb.py      sss_sume_metadata.pyc
gen_P4_SWITCH_API.py      liblpm_templates.pyc      nf_sim_compare_axi_logs.py
gen_P4_SWITCH_CLI.py      libtcam_templates.py      nf_sim_tools.py

#+END_CENTER

Find the input file to find the script call directory
#+BEGIN_CENTER
[14:04] rainbow:sume-sdnet-switch% find ~/projects/P4-NetFPGA -name config_writes.txt
/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt
[14:08] rainbow:sume-sdnet-switch%

#+END_CENTER

Input data in nf_sume_sdnet_ip is:

#+BEGIN_CENTER
<addr, data>: (00000020, 00000001)
<addr, data>: (00000020, 00000000)

#+END_CENTER

Original call in the Makefile:

#+BEGIN_CENTER
[14:10] rainbow:minip4% make config_writes
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/gen_config_writes.py nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt 0x44020000 testdata
[14:10] rainbow:minip4%
#+END_CENTER

Understading gen_config_writes.py:

#+BEGIN_CENTER
def main():
    parser = argparse.ArgumentParser()
    parser.add_argument('filename', type=str, help="the config_writes.txt file")
    parser.add_argument('baseaddr', type=str, help="the base address of the P4_SWITCH")
    parser.add_argument('outdir', type=str, help="the name of the output directory")
    args = parser.parse_args()

    dic = parse_config_writes(args.filename)
    new_dic = remove_init_addresses(dic)
    write_sim_config(new_dic, int(args.baseaddr, 0), args.outdir)
    write_hw_config(new_dic, int(args.baseaddr, 0), args.outdir)

#+END_CENTER

read arguments, create a dictionary by removing init addresses (why?
which?), create the two output files, one of them being
config_writes.py that does not have any lines.

#+BEGIN_CENTER
def parse_config_writes(filename):
    regex = r"<addr, data>: \(([abcdefABCDEF\d]*), ([abcdefABCDEF\d]*)\)"
    dic = collections.OrderedDict()
    i = 0
    with open(filename) as f:
        for line in f:
            searchObj = re.match(regex, line)
            if searchObj is not None:
                dic[i] = (searchObj.group(1), searchObj.group(2))
            else:
                print >> sys.stderr, "ERROR: encountered unexpected line in file: \n", line
                sys.exit(1)
            i += 1
    return dic
#+END_CENTER

Looks for all matching lines, errors out if wrong lines are in there.

#+BEGIN_CENTER
def remove_init_addresses(dic):
    result = collections.OrderedDict()
    for (index, tup) in dic.iteritems():
        if tup[0][-2:] != "20":
            result[index] =  tup
    return result
#+END_CENTER

Adding debug:

#+BEGIN_CENTER
def main():
    parser = argparse.ArgumentParser()
    parser.add_argument('filename', type=str, help="the config_writes.txt file")
    parser.add_argument('baseaddr', type=str, help="the base address of the P4_SWITCH")
    parser.add_argument('outdir', type=str, help="the name of the output directory")
    args = parser.parse_args()

    dic = parse_config_writes(args.filename)
    print("orig dic: {}".format(dic))
    new_dic = remove_init_addresses(dic)
    print("new dic: {}".format(new_dic))
    write_sim_config(new_dic, int(args.baseaddr, 0), args.outdir)
    write_hw_config(new_dic, int(args.baseaddr, 0), args.outdir)

#+END_CENTER

Output:

#+BEGIN_CENTER
nfig_writes.txt 0x44020000 testdata
[14:10] rainbow:minip4% make config_writes
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/gen_config_writes.py nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt 0x44020000 testdata
orig dic: OrderedDict([(0, ('00000020', '00000001')), (1, ('00000020', '00000000'))])
new dic: OrderedDict()
[14:15] rainbow:minip4%

#+END_CENTER

-> Problem seems to be that no addresses are left. Why?

****** DONE try10: find out, why nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt has too less content
******* DONE find out what generates config_writes.txt
Seems to be step 5:

#+BEGIN_CENTER
[14:22] rainbow:SimpleSumeSwitch% pwd
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch
[14:23] rainbow:SimpleSumeSwitch% ls -lh config_writes.txt
-rw-rw-r-- 1 nico nico 140 May 25 14:21 config_writes.txt
[14:23] rainbow:SimpleSumeSwitch% date
Sat 25 May 2019 02:23:41 PM CEST
[14:23] rainbow:SimpleSumeSwitch%
#+END_CENTER
******* DONE Debug vivado_sim.bash -> run w/ x11 output, also vivado_sim_waveform.bash
Open GUI, pressing "play" button, getting different / new errors
#+BEGIN_CENTER
[SW] CAM_Init() - done
[SW] CAM_EnableDevice() - start
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_write_control()- start
SV_write_control()- done
[SW] CAM_EnableDevice() - done
[2420698]  INFO: finished packet stimulus file
[2735572] ERROR: tuple mismatch for packet 1
expected < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >
actual   < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000000010000 >
$finish called at time : 2735572 ps : File
"/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v"
Line 120

#+END_CENTER

Error message created in
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v

Same error on shell only version:

#+BEGIN_CENTER
projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_memory.sv
[SW] CAM_Init() - start
[SW] CAM_Init() - done
[SW] CAM_EnableDevice() - start
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_write_control()- start
SV_write_control()- done
[SW] CAM_EnableDevice() - done
[2420698]  INFO: finished packet stimulus file
[2735572] ERROR: tuple mismatch for packet 1
expected < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >
actual   < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000000010000 >
$finish called at time : 2735572 ps : File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v" Line 120
exit
INFO: [Common 17-206] Exiting xsim at Sat May 25 14:38:05 2019...
[14:38] rainbow:SimpleSumeSwitch% echo $?
0
[14:38] rainbow:SimpleSumeSwitch%

#+END_CENTER

Analysing Makefile in testdata + scripts
******** get_testdata.py: generates some pcap with some packets

Need to find out
import sss_sdnet_tuples
sss_sdnet_tuples.clear_tuple_files()

Result of this script is src.pcap and dst.pcap.

Is the lookup table related to the devices?

NUM_KEYS = 4
lookup_table = {
    0: 0x00000001,
    1: 0x00000010,
    2: 0x00000100,
    3: 0x00001000
}

Where are in/out ports?!

Modifying / adjusting P4 code to mirror input packets

******** switch_calc_headers creates some headers
some specific packet,  uses bind_layers

****** DONE try11: fixing gen_testdata, adding p4 code for mirroring
Failure again at step 5:

#+BEGIN_CENTER
me_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for__OUT_.lahsy4kevbbz5f1pl25cndeyi9crlj_812.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for__OUT_/lahsy4kevbbz5f1pl25cndeyi9crlj_812/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_1120  File: /home/nico/master-thesis/netpfga/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_memory.sv
[SW] CAM_Init() - start
[SW] CAM_Init() - done
[SW] CAM_EnableDevice() - start
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_write_control()- start
SV_write_control()- done
[SW] CAM_EnableDevice() - done
[2260762]  INFO: finished packet stimulus file
[2735572] ERROR: tuple mismatch for packet 1
expected < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >
actual   < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000000010000 >
$finish called at time : 2735572 ps : File "/home/nico/master-thesis/netpfga/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v" Line 120
exit
INFO: [Common 17-206] Exiting xsim at Sun May 26 11:09:04 2019...
[11:09] rainbow:SimpleSumeSwitch%

#+END_CENTER

After setting egress port, vivado_sim.bash looks good

#+BEGIN_CENTER
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_write_control()- start
SV_write_control()- done
[SW] CAM_EnableDevice() - done
[2260762]  INFO: finished packet stimulus file
[2735572]  INFO: packet 1 tuple OK < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >
[2735572]  INFO: packet 1  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000090082222222208081111111108)
[2738904]  INFO: packet 1  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[6074236]  INFO: stopping simulation after 1000 idle cycles
[6074236]  INFO: all expected data successfully received
[6074236]  INFO: TEST PASSED
$finish called at time : 6074236 ps : File "/home/nico/master-thesis/netpfga/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/SimpleSumeSwitch_tb.sv" Line 207
exit
INFO: [Common 17-206] Exiting xsim at Sun May 26 11:14:34 2019...
[11:14] rainbow:SimpleSumeSwitch%

#+END_CENTER

Started compiling the bitstream at around 1120
Ended at Sun 26 May 2019 01:09:05 PM CEST

***** run step 11: checking design -- skipped
***** DONE run step 12: ok
****** code
#+BEGIN_CENTER
cd $NF_DESIGN_DIR/bitfiles && \
mv simple_sume_switch.bit ${P4_PROJECT_NAME}.bit && \
cp $P4_PROJECT_DIR/testdata/config_writes.sh ./
#+END_CENTER
***** DONE run step 13:
****** command
#+BEGIN_CENTER
cd $NF_DESIGN_DIR/bitfiles/ && sudo bash ./program_switch.sh

[13:18] rainbow:bitfiles% sudo bash
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles# . ~nico/master-thesis/netpfga/bashinit
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles# bash program_switch.sh
#+END_CENTER
****** DONE try1: paths not setup for root
[14:54] rainbow:bitfiles% cd $NF_DESIGN_DIR/bitfiles/ && sudo bash ./program_switch.sh
./program_switch.sh: line 34: /tools/program_switch.sh: No such file or directory
[14:56] rainbow:bitfiles% ls
config_writes.sh  minip4.bit  program_switch.sh  README
[14:56] rainbow:bitfiles%
****** DONE try2: setup paths as root: various other errors
#+BEGIN_CENTER
root@rainbow:~# cd $NF_DESIGN_DIR/bitfiles/ &&  bash ./program_switch.sh
rmmod: ERROR: Module sume_riffa is not currently loaded
rlwrap: warning: your $TERM is 'screen' but rlwrap couldn't find it in the terminfo database. Expect some problems.
RUN loading image file.
switch_calc.bit
attempting to launch hw_server
 ****** Xilinx hw_server v2018.2
  **** Build date : Jun 14 2018-20:18:37
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

INFO: hw_server application started
INFO: Use Ctrl-C to exit hw_server application

INFO: To connect to this hw_server instance use url: TCP:127.0.0.1:3121


couldn't open "switch_calc.bit": no such file or directory
    invoked from within
"::tcf::eval -progress ::xsdb::print_progress {::tcf::cache_enter tcfchan#0 {tcf_cache_eval {process_tcf_actions_cache_client ::tcfclient#0::arg}}}"
    (procedure "::tcf::cache_eval_with_progress" line 2)
    invoked from within
"::tcf::cache_eval_with_progress [dict get $arg chan]  [list process_tcf_actions_cache_client $argvar] $progress"
    (procedure "process_tcf_actions" line 1)
    invoked from within
"process_tcf_actions $arg ::xsdb::print_progress"
    (procedure "fpga" line 430)
    invoked from within
"fpga -f $bitimage"
    (file "/root/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl" line 33)
Check programming FPGA or Reboot machine !
rmmod: ERROR: Module sume_riffa is not currently loaded
nf0: ERROR while getting interface flags: No such device
nf1: ERROR while getting interface flags: No such device
nf2: ERROR while getting interface flags: No such device
nf3: ERROR while getting interface flags: No such device

#+END_CENTER
****** DONE try3: adjusting/analysing "./program_switch.sh"
Calls another script
#+BEGIN_CENTER
# Program the switch with the bit file and then configure the tables
${SUME_SDNET}/tools/program_switch.sh switch_calc.bit config_writes.sh
#+END_CENTER
****** DONE try4: analyse ANOTHER program_switch.sh
#+BEGIN_CENTER
root@rainbow:~/projects/P4-NetFPGA# find . -name program_switch.sh
./contrib-projects/sume-sdnet-switch/projects/int/simple_sume_switch/bitfiles/program_switch.sh
./contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/bitfiles/program_switch.sh
./contrib-projects/sume-sdnet-switch/projects/switch_calc/simple_sume_switch/bitfiles/program_switch.sh
./contrib-projects/sume-sdnet-switch/projects/learning_switch/simple_sume_switch/bitfiles/program_switch.sh
./contrib-projects/sume-sdnet-switch/projects/tcp_monitor/simple_sume_switch/bitfiles/program_switch.sh
./contrib-projects/sume-sdnet-switch/tools/program_switch.sh
./contrib-projects/sume-sdnet-switch/templates/sss_p4_proj/simple_sume_switch/bitfiles/program_switch.sh
root@rainbow:~/projects/P4-NetFPGA#

#+END_CENTER

Add set -x debugging, see real error

#+BEGIN_CENTER

#+END_CENTER
****** DONE try 5: reboot && retry
#+BEGIN_CENTER
[9:24] rainbow:~% sudo -i
root@rainbow:~# lsmod | grep riffa
root@rainbow:~# modprobe sume_riffa
modprobe: FATAL: Module sume_riffa not found in directory /lib/modules/5.0.0-15-generic
root@rainbow:~#
#+END_CENTER
-> not changing



******* DONE Going back to setup steps
[10:11] rainbow:tcam_v1_1_0% cd $SUME_FOLDER/lib/hw/xilinx/cores/tcam_v1_1_0/ && make update && make
cd $SUME_FOLDER/lib/hw/xilinx/cores/cam_v1_1_0/ && make update && make
cd $SUME_SDNET/sw/sume && make
cd $SUME_FOLDER && make

-> all good so far

cd $DRIVER_FOLDER
make all
sudo make install
sudo modprobe sume_riffa



#+BEGIN_CENTER
[11:44] rainbow:sume_riffa_v1_0_0% sudo make install
make -C /lib/modules/5.0.0-15-generic/build M=/home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0 modules
make[1]: Entering directory '/usr/src/linux-headers-5.0.0-15-generic'
  Building modules, stage 2.
  MODPOST 1 modules
make[1]: Leaving directory '/usr/src/linux-headers-5.0.0-15-generic'
install -o root -g root -m 0755 -d /lib/modules/5.0.0-15-generic/extra/sume_riffa/
install -o root -g root -m 0755 sume_riffa.ko /lib/modules/5.0.0-15-generic/extra/sume_riffa/
depmod -a 5.0.0-15-generic
[11:44] rainbow:sume_riffa_v1_0_0%

[11:44] rainbow:sume_riffa_v1_0_0% lsmod | grep sume_riffa
sume_riffa             28672  0
[11:45] rainbow:sume_riffa_v1_0_0%

#+END_CENTER

****** DONE try 6: after successful compile, missing switch_calc.bitcoin
#+BEGIN_CENTER
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles# bash program_switch.sh
++ which vivado
+ xilinx_tool_path=/opt/Xilinx/Vivado/2018.2/bin/vivado
+ bitimage=switch_calc.bit
+ configWrites=config_writes.sh
+ '[' -z switch_calc.bit ']'
+ '[' -z config_writes.sh ']'
+ '[' /opt/Xilinx/Vivado/2018.2/bin/vivado == '' ']'
+ rmmod sume_riffa
+ xsct /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl -tclargs switch_calc.bit
rlwrap: warning: your $TERM is 'screen' but rlwrap couldn't find it in the terminfo database. Expect some problems.
RUN loading image file.
switch_calc.bit
attempting to launch hw_server

 ****** Xilinx hw_server v2018.2
  **** Build date : Jun 14 2018-20:18:37
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

INFO: hw_server application started
INFO: Use Ctrl-C to exit hw_server application

INFO: To connect to this hw_server instance use url: TCP:127.0.0.1:3121


couldn't open "switch_calc.bit": no such file or directory
    invoked from within
"::tcf::eval -progress ::xsdb::print_progress {::tcf::cache_enter tcfchan#0 {tcf_cache_eval {process_tcf_actions_cache_client ::tcfclient#0::arg}}}"
    (procedure "::tcf::cache_eval_with_progress" line 2)
    invoked from within
"::tcf::cache_eval_with_progress [dict get $arg chan]  [list process_tcf_actions_cache_client $argvar] $progress"
    (procedure "process_tcf_actions" line 1)
    invoked from within
"process_tcf_actions $arg ::xsdb::print_progress"
    (procedure "fpga" line 430)
    invoked from within
"fpga -f $bitimage"
    (file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl" line 33)
+ bash /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/pci_rescan_run.sh
Check programming FPGA or Reboot machine !
+ rmmod sume_riffa
rmmod: ERROR: Module sume_riffa is not currently loaded
+ modprobe sume_riffa
+ ifconfig nf0 up
nf0: ERROR while getting interface flags: No such device
+ ifconfig nf1 up
nf1: ERROR while getting interface flags: No such device
+ ifconfig nf2 up
nf2: ERROR while getting interface flags: No such device
+ ifconfig nf3 up
nf3: ERROR while getting interface flags: No such device
+ bash config_writes.sh
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles#

#+END_CENTER

Debugging  why the bitfile is missing -> WRONG name!
Analysing program_switch.sh


#+BEGIN_CENTER
[13:22] rainbow:bitfiles% ls
config_writes.sh  minip4.bit  program_switch.sh  README
[13:24] rainbow:bitfiles%

#+END_CENTER

switch_calc.bit HARDCODED incorrectly in the script

#+BEGIN_CENTER
# Program the switch with the bit file and then configure the tables
${SUME_SDNET}/tools/program_switch.sh minip4.bit config_writes.sh

#+END_CENTER

Output of programming

#+BEGIN_CENTER
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles# bash program_switch.sh
++ which vivado
+ xilinx_tool_path=/opt/Xilinx/Vivado/2018.2/bin/vivado
+ bitimage=minip4.bit
+ configWrites=config_writes.sh
+ '[' -z minip4.bit ']'
+ '[' -z config_writes.sh ']'
+ '[' /opt/Xilinx/Vivado/2018.2/bin/vivado == '' ']'
+ rmmod sume_riffa
+ xsct /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl -tclargs minip4.bit
rlwrap: warning: your $TERM is 'screen' but rlwrap couldn't find it in the terminfo database. Expect some problems.
RUN loading image file.
minip4.bit
attempting to launch hw_server

 ****** Xilinx hw_server v2018.2
  **** Build date : Jun 14 2018-20:18:37
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

INFO: hw_server application started
INFO: Use Ctrl-C to exit hw_server application

INFO: To connect to this hw_server instance use url: TCP:127.0.0.1:3121

100%   11MB   1.7MB/s  00:06
+ bash /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/pci_rescan_run.sh
Check programming FPGA or Reboot machine !
+ rmmod sume_riffa
rmmod: ERROR: Module sume_riffa is not currently loaded
+ modprobe sume_riffa
+ ifconfig nf0 up
nf0: ERROR while getting interface flags: No such device
+ ifconfig nf1 up
nf1: ERROR while getting interface flags: No such device
+ ifconfig nf2 up
nf2: ERROR while getting interface flags: No such device
+ ifconfig nf3 up
nf3: ERROR while getting interface flags: No such device
+ bash config_writes.sh
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles#

#+END_CENTER

After reboot:
#+BEGIN_CENTER
[13:27] rainbow:~% lspci
00:00.0 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15d0
00:00.2 IOMMU: Advanced Micro Devices, Inc. [AMD] Device 15d1
00:01.0 Host bridge: Advanced Micro Devices, Inc. [AMD] Family 17h (Models 00h-0fh) PCIe Dummy Host Bridge
00:01.1 PCI bridge: Advanced Micro Devices, Inc. [AMD] Device 15d3
00:01.2 PCI bridge: Advanced Micro Devices, Inc. [AMD] Device 15d3
00:01.6 PCI bridge: Advanced Micro Devices, Inc. [AMD] Device 15d3
00:08.0 Host bridge: Advanced Micro Devices, Inc. [AMD] Family 17h (Models 00h-0fh) PCIe Dummy Host Bridge
00:08.1 PCI bridge: Advanced Micro Devices, Inc. [AMD] Device 15db
00:08.2 PCI bridge: Advanced Micro Devices, Inc. [AMD] Device 15dc
00:14.0 SMBus: Advanced Micro Devices, Inc. [AMD] FCH SMBus Controller (rev 61)
00:14.3 ISA bridge: Advanced Micro Devices, Inc. [AMD] FCH LPC Bridge (rev 51)
00:18.0 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15e8
00:18.1 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15e9
00:18.2 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15ea
00:18.3 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15eb
00:18.4 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15ec
00:18.5 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15ed
00:18.6 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15ee
00:18.7 Host bridge: Advanced Micro Devices, Inc. [AMD] Device 15ef
10:00.0 Memory controller: Xilinx Corporation Device 7028
15:00.0 USB controller: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset USB 3.1 xHCI Controller (rev 02)
15:00.1 SATA controller: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset SATA Controller (rev 02)
15:00.2 PCI bridge: Advanced Micro Devices, Inc. [AMD] Device 43b2 (rev 02)
1d:00.0 PCI bridge: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset PCIe Port (rev 02)
1d:01.0 PCI bridge: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset PCIe Port (rev 02)
1d:04.0 PCI bridge: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset PCIe Port (rev 02)
1d:05.0 PCI bridge: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset PCIe Port (rev 02)
1d:06.0 PCI bridge: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset PCIe Port (rev 02)
1d:07.0 PCI bridge: Advanced Micro Devices, Inc. [AMD] 300 Series Chipset PCIe Port (rev 02)
24:00.0 Network controller: Intel Corporation Dual Band Wireless-AC 3168NGW [Stone Peak] (rev 10)
25:00.0 Ethernet controller: Intel Corporation I211 Gigabit Network Connection (rev 03)
38:00.0 VGA compatible controller: Advanced Micro Devices, Inc. [AMD/ATI] Raven Ridge [Radeon Vega Series / Radeon Vega Mobile Series] (rev c8)
38:00.1 Audio device: Advanced Micro Devices, Inc. [AMD/ATI] Device 15de
38:00.2 Encryption controller: Advanced Micro Devices, Inc. [AMD] Device 15df
38:00.3 USB controller: Advanced Micro Devices, Inc. [AMD] Device 15e0
38:00.4 USB controller: Advanced Micro Devices, Inc. [AMD] Device 15e1
38:00.6 Audio device: Advanced Micro Devices, Inc. [AMD] Device 15e3
39:00.0 SATA controller: Advanced Micro Devices, Inc. [AMD] FCH SATA Controller [AHCI mode] (rev 61)
[13:27] rainbow:~%

root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles# lsmod | grep sume_riffa
sume_riffa             28672  0
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles#
[  187.401378] sume_riffa: loading out-of-tree module taints kernel.
[  187.401449] sume_riffa: module verification failed: signature and/or required key missing - tainting kernel
[  187.402281] NetFPGA SUME (RIFFA DMA) version $Revision: 1.34 $
[  187.402341] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: enabling device (0000 -> 0002)
[  187.402563] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] # of channels: 2
[  187.402565] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] bus interface width: 128
[  187.402567] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] bus master enabled: 1
[  187.402568] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] negotiated link width: 8
[  187.402569] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] negotiated rate width: 2500 MTs
[  187.402571] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] max downstream payload: 512 B
[  187.402572] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] max upstream payload: 128 B
[  187.402599] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 0 Ethernet address 02:53:55:4d:45:00
[  187.402604] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 1 Ethernet address 02:53:55:4d:45:01
[  187.402609] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 2 Ethernet address 02:53:55:4d:45:02
[  187.402613] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 3 Ethernet address 02:53:55:4d:45:03
[  187.427036] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 enp16s0: renamed from nf0
[  187.441436] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename7: renamed from nf3
[  187.465095] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 nf1: up
[  187.465218] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename6: renamed from nf2
[  187.493947] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 enp16s0: up
[  187.504797] amd_iommu_report_page_fault: 28 callbacks suppressed
[  187.504801] AMD-Vi: Event logged [IO_PAGE_FAULT device=10:00.7 domain=0x0000 address=0xffff4000 flags=0x0050]
[  188.421105] IPv6: ADDRCONF(NETDEV_CHANGE): nf1: link becomes ready
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles#

root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles# ip l
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
2: enp37s0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq state UP mode DEFAULT group default qlen 1000
    link/ether 70:85:c2:ad:62:79 brd ff:ff:ff:ff:ff:ff
3: wlp36s0: <NO-CARRIER,BROADCAST,MULTICAST,UP> mtu 1500 qdisc mq state DOWN mode DORMANT group default qlen 1000
    link/ether dc:8b:28:47:5c:f7 brd ff:ff:ff:ff:ff:ff
4: enp16s0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:00 brd ff:ff:ff:ff:ff:ff
5: nf1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:01 brd ff:ff:ff:ff:ff:ff
6: rename6: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:02 brd ff:ff:ff:ff:ff:ff
7: rename7: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:03 brd ff:ff:ff:ff:ff:ff
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles#

#+END_CENTER

***** DONE Step 14: test the card / switch
****** try1: adding ips, using tcpdump
******* testing enp16s0
  #+BEGIN_CENTER
 root@rainbow:~# tcpdump -ni enp16s0
 tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
 listening on enp16s0, link-type EN10MB (Ethernet), capture size 262144 bytes
 13:33:53.952947 IP6 fe80::53:55ff:fe4d:4500 > ff02::2: ICMP6, router solicitation, length 16
 13:33:55.404587 LLDP, length 216: rainbow.place6.ungleich.ch
 13:34:02.242610 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
 13:34:03.263792 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
 13:34:04.287910 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
 13:34:07.429549 IP 0.0.0.0.68 > 255.255.255.255.67: BOOTP/DHCP, Request from 02:53:55:4d:45:00, length 288
 13:34:25.415196 LLDP, length 216: rainbow.place6.ungleich.ch
 13:34:55.418304 LLDP, length 216: rainbow.place6.ungleich.ch
 13:35:12.381120 IP 0.0.0.0.68 > 255.255.255.255.67: BOOTP/DHCP, Request from 02:53:55:4d:45:00, length 288
 13:35:25.420868 LLDP, length 216: rainbow.place6.ungleich.ch
 13:35:55.423875 LLDP, length 216: rainbow.place6.ungleich.ch
 13:36:17.384654 IP 0.0.0.0.68 > 255.255.255.255.67: BOOTP/DHCP, Request from 02:53:55:4d:45:00, length 288
 13:36:25.427542 LLDP, length 216: rainbow.place6.ungleich.ch
 13:36:55.431733 LLDP, length 216: rainbow.place6.ungleich.ch
 13:37:20.483400 IP 0.0.0.0.68 > 255.255.255.255.67: BOOTP/DHCP, Request from 02:53:55:4d:45:00, length 288
 13:37:25.435735 LLDP, length 216: rainbow.place6.ungleich.ch
 13:37:54.556948 IP6 fe80::53:55ff:fe4d:4500 > ff02::2: ICMP6, router solicitation, length 16
 13:37:55.438238 LLDP, length 216: rainbow.place6.ungleich.ch
 13:38:25.384418 IP 0.0.0.0.68 > 255.255.255.255.67: BOOTP/DHCP, Request from 02:53:55:4d:45:00, length 288
 13:38:25.442805 LLDP, length 216: rainbow.place6.ungleich.ch

  #+END_CENTER
******* Testing nf1
#+BEGIN_CENTER
root@rainbow:/etc/network# ip addr add 2001:db8:1::1/64 dev nf1
root@rainbow:/etc/network#

root@rainbow:~# tcpdump -ni nf1
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on nf1, link-type EN10MB (Ethernet), capture size 262144 bytes
13:39:11.947770 IP6 fe80::53:55ff:fe4d:4501 > ff02::16: HBH ICMP6, multicast listener report v2, 3 group record(s), length 68
13:39:12.011981 IP6 :: > ff02::1:ff00:1: ICMP6, neighbor solicitation, who has 2001:db8:1::1, length 32
13:39:12.799761 IP6 fe80::53:55ff:fe4d:4501 > ff02::16: HBH ICMP6, multicast listener report v2, 3 group record(s), length 68
13:39:14.064981 IP6 2001:db8:1::1.5353 > ff02::fb.5353: 0*- [0q] 2/0/0 (Cache flush) PTR rainbow.local., (Cache flush) AAAA 2001:db8:1::1 (139)
13:39:16.251534 IP6 2001:db8:1::1.5353 > ff02::fb.5353: 0*- [0q] 2/0/0 (Cache flush) PTR rainbow.local., (Cache flush) AAAA 2001:db8:1::1 (139)
13:39:25.449875 LLDP, length 212: rainbow.place6.ungleich.ch


#+END_CENTER

Rebooting again


#+BEGIN_CENTER
root@rainbow:~# modprobe sume_riffa
root@rainbow:~# dmesg | tail -n 20
[   88.460898] NetFPGA SUME (RIFFA DMA) version $Revision: 1.34 $
[   88.461136] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] # of channels: 2
[   88.461138] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] bus interface width: 128
[   88.461140] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] bus master enabled: 1
[   88.461141] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] negotiated link width: 8
[   88.461143] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] negotiated rate width: 2500 MTs
[   88.461144] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] max downstream payload: 512 B
[   88.461145] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] max upstream payload: 128 B
[   88.461168] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 0 Ethernet address 02:53:55:4d:45:00
[   88.461173] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 1 Ethernet address 02:53:55:4d:45:01
[   88.461177] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 2 Ethernet address 02:53:55:4d:45:02
[   88.461182] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 3 Ethernet address 02:53:55:4d:45:03
[   88.481731] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 enp16s0: renamed from nf3
[   88.502173] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename6: renamed from nf2
[   88.526514] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename4: renamed from nf0
[   88.542069] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 enp16s0: up
[   88.543090] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename5: renamed from nf1
[   89.497027] IPv6: ADDRCONF(NETDEV_CHANGE): enp16s0: link becomes ready
[   89.497964] amd_iommu_report_page_fault: 28 callbacks suppressed
[   89.497967] AMD-Vi: Event logged [IO_PAGE_FAULT device=10:00.7 domain=0x0000 address=0xffff4000 flags=0x0050]
root@rainbow:~#

#+END_CENTER
***** 2019-05-26, netfpga integration

#+BEGIN_CENTER
[10:56] rainbow:projects% mv minip4 ~/master-thesis/netpfga/
[10:56] rainbow:projects% ln -s ~/master-thesis/netpfga/minip4
[10:56] rainbow:projects%

root@rainbow:~# ip l s enp16s0 up
root@rainbow:~# tcpdump -ni enp16s0
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on enp16s0, link-type EN10MB (Ethernet), capture size 262144 bytes

[   88.460460] sume_riffa: loading out-of-tree module taints kernel.
[   88.460534] sume_riffa: module verification failed: signature and/or required key missing - tainting kernel
[   88.460898] NetFPGA SUME (RIFFA DMA) version $Revision: 1.34 $
[   88.461136] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] # of channels: 2
[   88.461138] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] bus interface width: 128
[   88.461140] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] bus master enabled: 1
[   88.461141] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] negotiated link width: 8
[   88.461143] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] negotiated rate width: 2500 MTs
[   88.461144] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] max downstream payload: 512 B
[   88.461145] NetFPGA SUME (RIFFA DMA) 0000:10:00.0: [riffa] max upstream payload: 128 B
[   88.461168] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 0 Ethernet address 02:53:55:4d:45:00
[   88.461173] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 1 Ethernet address 02:53:55:4d:45:01
[   88.461177] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 2 Ethernet address 02:53:55:4d:45:02
[   88.461182] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 (unnamed net_device) (uninitialized): Port 3 Ethernet address 02:53:55:4d:45:03
[   88.481731] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 enp16s0: renamed from nf3
[   88.502173] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename6: renamed from nf2
[   88.526514] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename4: renamed from nf0
[   88.542069] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 enp16s0: up
[   88.543090] NetFPGA SUME (RIFFA DMA) 0000:10:00.0 rename5: renamed from nf1
[   89.497027] IPv6: ADDRCONF(NETDEV_CHANGE): enp16s0: link becomes ready
[   89.497964] amd_iommu_report_page_fault: 28 callbacks suppressed
[   89.497967] AMD-Vi: Event logged [IO_PAGE_FAULT device=10:00.7 domain=0x0000 address=0xffff4000 flags=0x0050]
[  124.875633] device enp16s0 entered promiscuous mode
root@rainbow:~#


root@rainbow:~# ip addr add 2001:db8::1/64 dev enp16s0

13:45:04.211832 IP6 :: > ff02::1:ff00:1: ICMP6, neighbor solicitation, who has 2001:db8::1, length 32
13:45:05.555657 IP6 2001:db8::1.5353 > ff02::fb.5353: 0*- [0q] 2/0/0 (Cache flush) PTR rainbow.local., (Cache flush) AAAA 2001:db8::1 (139)
13:45:07.718554 IP6 2001:db8::1.5353 > ff02::fb.5353: 0*- [0q] 2/0/0 (Cache flush) PTR rainbow.local., (Cache flush) AAAA 2001:db8::1 (139)
13:45:23.556081 LLDP, length 216: rainbow.place6.ungleich.ch
#+END_CENTER

-> no replies

Testing with the supplied tool

#+BEGIN_CENTER
root@rainbow:~/master-thesis/netpfga/minip4/sw/hw_test_tool# python switch_calc_tester.py
SIOCSIFADDR: No such device
eth1: ERROR while getting interface flags: No such device
SIOCSIFNETMASK: No such device
tcpdump: eth1: No such device exists
(SIOCGIFHWADDR: No such device)
The HW testing tool for the switch_calc design
 type help to see all commands
testing>

#+END_CENTER

Broken again. Debug manually.

#+BEGIN_CENTER


[13:49] rainbow:~% python
Python 2.7.16 (default, Apr  6 2019, 01:42:57)
[GCC 8.3.0] on linux2
Type "help", "copyright", "credits" or "license" for more information.
>>> from scapy.all import *
>>> MAC1 = "08:11:11:11:11:08"
>>> MAC2 = "08:22:22:22:22:08"
>>> pkt = Ether(dst=MAC2, src=MAC1)
>>> srp1(pkt, iface="enp16s0")
Traceback (most recent call last):
  File "<stdin>", line 1, in <module>
  File "/usr/lib/python2.7/dist-packages/scapy/sendrecv.py", line 434, in srp1
    ans, _ = srp(*args, **kargs)
  File "/usr/lib/python2.7/dist-packages/scapy/sendrecv.py", line 416, in srp
    s = conf.L2socket(promisc=promisc, iface=iface, filter=filter, nofilter=nofilter, type=type)
  File "/usr/lib/python2.7/dist-packages/scapy/arch/linux.py", line 502, in __init__
    self.ins = socket.socket(socket.AF_PACKET, socket.SOCK_RAW, socket.htons(type))
  File "/usr/lib/python2.7/socket.py", line 191, in __init__
    _sock = _realsocket(family, type, proto)
socket.error: [Errno 1] Operation not permitted
>>>

#+END_CENTER

Try padding to 64 bytes

#+BEGIN_CENTER
>>> len(pkt)
14
>>> 64-14
50
>>> RAW(50*"A")
Traceback (most recent call last):
  File "<stdin>", line 1, in <module>
NameError: name 'RAW' is not defined
>>> Raw(50*"A")
<Raw  load='AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA' |>
>>> pkg2 = pkt / Raw(50*"A")
>>>
>>> pkg2 = pkt / Raw(50*"A")
>>> srp1(pkg2, iface="enp16s0")
Begin emission:
Finished sending 1 packets.


tcpdump:


#+END_CENTER

**** DONE Understand a bit of xilinx/netfpga/vivado ~ somewhat
     - https://www.xilinx.com/support/documentation/sw_manuals/xilinx2014_4/ug900-vivado-logic-simulation.pdf
The xvhdl and xvlog commands parse VHDL and Verilog files, respectively. Descriptions
for each option are available in Table 5-2, page 102.

This command parses the VHDL source file(s) and stores the parsed dump into a HDL library
on disk.
***** xelab
xelab
The xelab command, for given top-level units, does the following:
• Loads children design units using language binding rules or the –L <library>
command line specified HDL libraries
• Performs a static elaboration of the design (sets parameters, generics, puts generate
statements into effect, and so forth)
• Generates executable code
• Links the generated executable code with the simulation kernel library to create an
executable simulation snapshot
You then use the produced executable simulation snapshot name as an option to the xsim
command along with other options to effect HDL simulation
***** Summary of xilinx toolchain
VHDL->[via xvhdl]-> HDL
Verilog->[via xvlog]->HDL

***** Understand SimpleSumeSwitch
SimpleSumeSwitch(
    TopParser(),
    TopPipe(),
    TopDeparser()
) main;
**** Understand the different switch models (?)
*** TODO Find out whether delta based checksumming is feasible [in P4]
**** DONE Analysing scapy
     CLOSED: [2019-06-23 Sun 14:18]
#+BEGIN_CENTER
[13:51] line:~% dpkg -L python3-scapy | grep inet
/usr/lib/python3/dist-packages/scapy/layers/inet.py
/usr/lib/python3/dist-packages/scapy/layers/inet6.py

        if self.chksum is None:
            ck = checksum(p)
            p = p[:10]+chb(ck>>8)+chb(ck&0xff)+p[12:]
        return p+pay

[13:55] line:~% grep checksum -r /usr/lib/python3/dist-packages/scapy/ | grep def
/usr/lib/python3/dist-packages/scapy/contrib/isis.py:    def checksum_info(self, hdrlen):
/usr/lib/python3/dist-packages/scapy/contrib/isis.py:    def checksum_info(self, hdrlen):
/usr/lib/python3/dist-packages/scapy/contrib/ospf.py:def ospf_lsa_checksum(lsa):
/usr/lib/python3/dist-packages/scapy/utils.py:    def checksum(pkt):
/usr/lib/python3/dist-packages/scapy/utils.py:    def checksum(pkt):
/usr/lib/python3/dist-packages/scapy/utils.py:def fletcher16_checksum(binbuf):
/usr/lib/python3/dist-packages/scapy/layers/sctp.py:def sctp_checksum(buf):
[13:55] line:~%



if struct.pack("H",1) == b"\x00\x01": # big endian
    def checksum(pkt):
        if len(pkt) % 2 == 1:
            pkt += b"\0"
        s = sum(array.array("H", pkt))
        s = (s >> 16) + (s & 0xffff)
        s += s >> 16
        s = ~s
        return s & 0xffff
else:
    def checksum(pkt):
        if len(pkt) % 2 == 1:
            pkt += b"\0"
        s = sum(array.array("H", pkt))
        s = (s >> 16) + (s & 0xffff)
        s += s >> 16
        s = ~s
        return (((s>>8)&0xff)|s<<8) & 0xffff


#+END_CENTER
**** TODO Trying to create a delta diff: AAAA vs. BBAA
#+BEGIN_CENTER
[14:17] line:bin% python3 checksum_from_scapy.py AAAA
b'AAAA'
32125
[14:18] line:bin% python3 checksum_from_scapy.py BBAA
b'BBAA'
31868
[14:18] line:bin% python3 checksum_from_scapy.py AA
b'AA'
48830
[14:20] line:bin% python3 checksum_from_scapy.py BB
b'BB'
48573
>>> bin(48830)
'0b1011111010111110'
>>> bin(48573)
'0b1011110110111101'
>>>

>>> array.array("H", "AAAA".encode("utf-8"))
array('H', [16705, 16705])
>>> array.array("H", "AA".encode("utf-8"))
array('H', [16705])

-> bit concat on 16:
AA:
>>> 0b100000101000001
16705

Order in 16 bit tuples does not matter:

[14:24] line:bin% python3 checksum_from_scapy.py AABB
b'AABB'
sum=33667
31868
[14:28] line:bin% python3 checksum_from_scapy.py BBAA
b'BBAA'
sum=33667
31868

[14:28] line:bin% python3 checksum_from_scapy.py BBCCAA
b'BBCCAA'
sum=50886
14649
[14:28] line:bin% python3 checksum_from_scapy.py BBAACC
b'BBAACC'
sum=50886
14649

Sum on shorts does not stay in short area:

>>> sum(array.array("H", [48830, 48573]))
97403
>>> sum(array.array("H", "AAAA".encode("utf-8")))
33410
>>> sum(array.array("H", "AABB".encode("utf-8")))
33667
>>> sum(array.array("H", "AABBCC".encode("utf-8")))
50886
>>> sum(array.array("H", "AABBCCDD".encode("utf-8")))
68362

Adding with overflow control works:

>>> s = 97403
>>> s = (s >> 16) + (s & 0xffff)
>>> s
31868
>>> s += s >> 16
>>> s
31868

[14:29] line:bin% python3 checksum_from_scapy.py AABB
b'AABB'
sum=33667
31868


#+END_CENTER
*** TODO Get ANY p4 program to successfully run on netpfga
**** TODO mirroring ethernet
***** no packets seen on source interface
**** TODO sending data to switch port 1
***** DONE figuring out which is port 1: nf0
expected
actual

    applyPkt(pkt, 'nf0', pktCnt)
    expPkt(pkt,   'nf2')
#  0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >
#  0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000010010000 >

    applyPkt(pkt, 'nf0', pktCnt)
    expPkt(pkt,   'nf3')

 < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000040010000 >
 < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >

***** DONE Testing packets: does not arrive on nf0 with ping6
4: nf0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 02:53:55:4d:45:00 brd ff:ff:ff:ff:ff:ff
    inet6 fe80::53:55ff:fe4d:4500/64 scope link
       valid_lft forever preferred_lft forever
5: nf1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 02:53:55:4d:45:01 brd ff:ff:ff:ff:ff:ff
    inet6 2001:db8::1/64 scope global
       valid_lft forever preferred_lft forever
    inet6 fe80::53:55ff:fe4d:4501/64 scope link
       valid_lft forever preferred_lft forever
6: nf2: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN group default qlen 1000
    link/ether 02:53:55:4d:45:02 brd ff:ff:ff:ff:ff:ff
7: nf3: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN group default qlen 1000
    link/ether 02:53:55:4d:45:03 brd ff:ff:ff:ff:ff:ff

root@rainbow:~# tcpdump -ni nf0
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on nf0, link-type EN10MB (Ethernet), capture size 262144 bytes

[19:27] rainbow:~% sudo -i
root@rainbow:~# tcpdump -ni nf1
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on nf1, link-type EN10MB (Ethernet), capture size 262144 bytes
19:28:36.720431 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
19:28:37.725181 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
19:28:38.749195 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32

***** TODO Testing packets with send_packet.py: nothing arrives
root@rainbow:/home/nico/master-thesis/bin# python send_packet.py nf1
.
Sent 1 packets.
root@rainbow:/home/nico/master-thesis/bin# python send_packet.py nf0
.
Sent 1 packets.
root@rainbow:/home/nico/master-thesis/bin#

-> only shows up on the interface that we send, not on nf0 if sending
   on nf1
***** TODO Trying to add explicit table entry
#+BEGIN_CENTER
>> table_cam_add_entry lookup_table send_to_port1 ff:ff:ff:ff:ff:ff =>
CAM_Init_ValidateContext() - done
WROTE 0x44020050 = 0xffffffff
WROTE 0x44020054 = 0xffff
WROTE 0x44020080 = 0x0003
python: ioctl: Unknown error 512
[20:27] rainbow:CLI%
#+END_CENTER
***** TODO Trying to read a table entry
#+BEGIN_CENTER
>> table_cam_read_entry lookup_table 0
CAM_Init_ValidateContext() - done
WROTE 0x44020050 = 0x0000
WROTE 0x44020054 = 0x0000
python: ioctl: Unknown error 512
[20:31] rainbow:CLI% python P4_SWITCH_CLI.py
loading libsume..
loading libsume..
loading libcam..
The SimpleSumeSwitch interactive command line tool
 type help to see all commands
>>  table_cam_read_entry lookup_table 1
CAM_Init_ValidateContext() - done
WROTE 0x44020050 = 0x0001
WROTE 0x44020054 = 0x0000
python: ioctl: Unknown error 512
[20:31] rainbow:CLI% python P4_SWITCH_CLI.py
loading libsume..
loading libsume..
loading libcam..
The SimpleSumeSwitch interactive command line tool
 type help to see all commands
>> table_cam_read_entry lookup_table p.ethernet.dstAddr
ERROR: failed to convert p.ethernet.dstAddr of type <type 'str'> to an integer

#+END_CENTER

*** TODO Create either HDL or PX for supporting payload checksum
    https://github.com/NetFPGA/P4-NetFPGA-public/issues/13
    https://github.com/NetFPGA/P4-NetFPGA-public/issues/13#issuecomment-490431016
**** TODO Explore HDL
**** TODO Explore PX
*** TODO Integrate nat64 code into netfpga
**** figure out how to do ANY checksums
** Diff / Delta based checksums
*** create test case / test theory
**** TODO try first v6/v6
**** using python/struct
***** find right byte orders
**** using python/scapy
#+BEGIN_CENTER

#+END_CENTER
**** using p4

**** using p4/netpfga
** NAT64/NAT46 Features in jool and tayga
*** TODO Static 1:1 NAT46: translate from IPv4 to IPv6 with a table
**** TODO TCP
**** TODO UDP
**** TODO ICMP <-> ICMPv6
*** TODO Stateless Prefix based NAT64: IPv6 to IPv4 translation prefix based
**** Allows IPv6 hosts to reach the IPv4 Internet
*** See time table above
** Additional features queue (to be discussed)
*** TODO Offset based translation (v4->v6) -> same as range (?)
*** TODO IP address learning (v6/v4) for real life switch? How do hosts find it?
** Netpfga cabling
| eth2 <--> nf0 |
| eth1 <--> nf3 |
* Thesis documentation
** Introduction
*** Related work
**** RFC6052
     - Defining well known prefix 64:ff9b::/96
     - Defining embedding depending on prefix: /32../104 in 8 bit
       steps
     - Longer than /96: suffix support

** Motivation
   TBD
** Translation mechanisms
   - v4 to v6 / vice versa
   - Stateful / stateless
   - static / dynamic
*** Explicit Address Mappings Table (EAMT)
    Range based mapping tables
    See https://www.jool.mx/en/eamt.html,
    https://tools.ietf.org/html/rfc7757
*** Stateful NAT46
    - Not needed
    - IP address based translation is enough
** Current state of the art tayga/jool
    TBD
*** Tayga
    - Single threaded
    - Multi threaded work started due to initiative of ungleich /
      Chrisrock [IPv6.chat]
*** Jool
     - EAMT bidirectional only (!)

IPtables interaction

```

user@T:~# # Create a Jool iptables instance named "example."
user@T:~# # Also, establish that the IPv6 representation of any IPv4 address should be
user@T:~# # `2001:db8::<IPv4 address>`. (See sections below for examples.)
user@T:~# jool_siit instance add "example" --iptables  --pool6 2001:db8::/96
user@T:~#
user@T:~# # Tell iptables which traffic should be handled by our newly-created instance:
user@T:~#
user@T:~# # IPv6: only packets from 2001:db8::198.51.100.8/125 to 2001:db8::192.0.2
user@T:~# ip6tables -t mangle -A PREROUTING \
>		-s 2001:db8::198.51.100.8/125 -d 2001:db8::192.0.2.0/120 \
>		-j JOOL_SIIT --instance "example"
user@T:~# # IPv4: Only packets from 192.0.2 to 198.51.100.8/29
user@T:~# iptables  -t mangle -A PREROUTING \
>		-s 192.0.2.0/24 -d 198.51.100.8/29 \
>		-j JOOL_SIIT --instance "example"
```
5656
*** Cisco (?)
** TODO P4 based implementation
*** General

    - IPv6 subnet 2001:db8::/32
    - IPv6 hosts are in 2001:db8:6::/64
    - IPv6 default router (::/0) is 2001:db8:6::42/64
    - IPv4 mapped Internet "NAT64 prefix" 2001:db8:4444::/96 (should
      go into a table)
    - IPv4 hosts are in 10.0.4.0/24
    - IPv6 in IPv4 mapped hosts are in 10.0.6.0/24
    - IPv4 default router = 10.0.0.42
*** TODO IPv4 embedding

RFC6052

#+BEGIN_SRC

    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |PL| 0-------------32--40--48--56--64--72--80--88--96--104---------|
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |32|     prefix    |v4(32)         | u | suffix                    |
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |40|     prefix        |v4(24)     | u |(8)| suffix                |
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |48|     prefix            |v4(16) | u | (16)  | suffix            |
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |56|     prefix                |(8)| u |  v4(24)   | suffix        |
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |64|     prefix                    | u |   v4(32)      | suffix    |
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
    |96|     prefix                                    |    v4(32)     |
    +--+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+


#+END_SRC

Bits 64..71 have to be 0 -- ref rfc4291 - host identifier - why?
Section 2.5.1 of rfc4291 "required to be unique within a subnet prefix"
Modified EUI-64 format.
Compare EUI-64: first 8 bits of mac address

inverting u bit from rfc 4291

#+BEGIN_QUOTE
the "u" bit is set to one (1)
   to indicate universal scope, and it is set to zero (0) to indicate
   local scope.

#+END_QUOTE


#+BEGIN_SRC

          0       0 0       1 1       2
         |0       7 8       5 6       3|
         +----+----+----+----+----+----+
         |cccc|ccug|cccc|cccc|cccc|cccc|
         +----+----+----+----+----+----+


#+END_SRC

*** Neighbor discover protocol
**** Initial log
     - Matching on prefix & ingress port, setting multicast

Being forwarded:

p4@ubuntu:~/master-thesis$ mx h1 tcpdump -ni h1-eth0
sudo: unable to resolve host ubuntu
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on h1-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
^C14:59:22.871803 IP6 2001:db8:62::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8:62::2, length 32
14:59:23.863913 IP6 2001:db8:62::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8:62::2, length 32
14:59:24.864033 IP6 2001:db8:62::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8:62::2, length 32

3 packets captured
3 packets received by filter
0 packets dropped by kernel

But no answer yet!


root@ubuntu:~/master-thesis/p4app# ip a
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN group default qlen 1
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    inet 127.0.0.1/8 scope host lo
       valid_lft forever preferred_lft forever
    inet6 ::1/128 scope host
       valid_lft forever preferred_lft forever
2: h1-eth0@if123: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 9500 qdisc netem state UP group default qlen 1000
    link/ether 00:00:0a:00:00:01 brd ff:ff:ff:ff:ff:ff link-netnsid 0
    inet6 2001:db8:62::2/64 scope global
       valid_lft forever preferred_lft forever
    inet6 2001:db8:61::1/64 scope global
       valid_lft forever preferred_lft forever
    inet6 fe80::200:aff:fe00:1/64 scope link
       valid_lft forever preferred_lft forever
root@ubuntu:~/master-thesis/p4app#

Link local communication does not work:

root@ubuntu:~/master-thesis/p4app# ping6 -c1 fe80::200:aff:fe00:2%h1-eth0
PING fe80::200:aff:fe00:2%h1-eth0(fe80::200:aff:fe00:2) 56 data bytes
From fe80::200:aff:fe00:1 icmp_seq=1 Destination unreachable: Address unreachable

--- fe80::200:aff:fe00:2%h1-eth0 ping statistics ---
1 packets transmitted, 0 received, +1 errors, 100% packet loss, time 0ms

root@ubuntu:~/master-thesis/p4app#

Packet is received on the other host, but not answered. Why?

Real trace from my network:

18:48:17.008524 IP6 2a0a:e5c1:111:111:eb7:ffdb:e245:f712 > ff02::1:ffb7:e225: ICMP6, neighbor solicitation, who has 2a0a:e5c1:111:111:1016:3c5a:38b7:e225, length 32
18:48:18.015016 IP6 2a0a:e5c1:111:111:eb7:ffdb:e245:f712 > ff02::1:ffb7:e225: ICMP6, neighbor solicitation, who has 2a0a:e5c1:111:111:1016:3c5a:38b7:e225, length 32
18:48:18.031165 IP6 2a0a:e5c1:111:111:1016:3c5a:38b7:e225 > 2a0a:e5c1:111:111:eb7:ffdb:e245:f712: ICMP6, neighbor advertisement, tgt is 2a0a:e5c1:111:111:1016:3c5a:38b7:e225, length 32
18:48:18.031236 IP6 2a0a:e5c1:111:111:eb7:ffdb:e245:f712 > 2a0a:e5c1:111:111:1016:3c5a:38b7:e225: ICMP6, echo request, seq 1, length 64
18:48:18.031267 IP6 2a0a:e5c1:111:111:eb7:ffdb:e245:f712 > 2a0a:e5c1:111:111:1016:3c5a:38b7:e225: ICMP6, echo request, seq 2, length 64
18:48:18.131709 IP6 2a0a:e5c1:111:111:1016:3c5a:38b7:e225 > 2a0a:e5c1:111:111:eb7:ffdb:e245:f712: ICMP6, echo reply, seq 1, length 64
18:48:18.131732 IP6 2a0a:e5c1:111:111:1016:3c5a:38b7:e225 > 2a0a:e5c1:111:111:eb7:ffdb:e245:f712: ICMP6, echo reply, seq 2, length 64


root@ubuntu:~/master-thesis/p4app# cat /proc/sys/net/ipv6/conf/*/disable_ipv6
1
1
0
0
root@ubuntu:~/master-thesis/p4app#
root@ubuntu:~/master-thesis/p4app# ls -1 /proc/sys/net/ipv6/conf/*/disable_ipv6
/proc/sys/net/ipv6/conf/all/disable_ipv6
/proc/sys/net/ipv6/conf/default/disable_ipv6
/proc/sys/net/ipv6/conf/h1-eth0/disable_ipv6
/proc/sys/net/ipv6/conf/lo/disable_ipv6
root@ubuntu:~/master-thesis/p4app#

Works on mininet

mininet> h2 bash
root@line:~# ip a
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN group default qlen 1
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
    inet 127.0.0.1/8 scope host lo
       valid_lft forever preferred_lft forever
    inet6 ::1/128 scope host
       valid_lft forever preferred_lft forever
2: h2-eth0@if93: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc noqueue state UP group default qlen 1000
    link/ether 32:0e:1e:bf:3c:4b brd ff:ff:ff:ff:ff:ff link-netnsid 0
    inet 10.0.0.2/8 brd 10.255.255.255 scope global h2-eth0
       valid_lft forever preferred_lft forever
    inet6 fe80::300e:1eff:febf:3c4b/64 scope link
       valid_lft forever preferred_lft forever
root@line:~# ip addr add 2001:db8:61::42/64 dev h2-eth0
root@line:~# ^Dexit
mininet> h1 bash
root@line:~# ip addr add 2001:db8:61::42/64^[[D^[[D^?^?^?^?^?^?^?^?^?^?^?^C^C
root@line:~# ^Dexit
mininet> h1 ip addr add 2001:db8:61::2/64 dev h1-eth0
mininet> h2 ping6 -c2 2001:db8:61::2
PING 2001:db8:61::2(2001:db8:61::2) 56 data bytes
64 bytes from 2001:db8:61::2: icmp_seq=1 ttl=64 time=0.230 ms
64 bytes from 2001:db8:61::2: icmp_seq=2 ttl=64 time=0.138 ms

--- 2001:db8:61::2 ping statistics ---
2 packets transmitted, 2 received, 0% packet loss, time 1018ms
rtt min/avg/max/mdev = 0.138/0.184/0.230/0.046 ms
mininet>


mininet on VM also works

mininet>  h1 ip addr add 2001:db8:61::1/64 dev h1-eth0
mininet> h2 ip addr add 2001:db8:61::2/64 dev h2-eth0
mininet> h2 ping6 -c2 2001:db8:61::2
PING 2001:db8:61::2(2001:db8:61::2) 56 data bytes
64 bytes from 2001:db8:61::2: icmp_seq=1 ttl=64 time=0.053 ms
64 bytes from 2001:db8:61::2: icmp_seq=2 ttl=64 time=0.082 ms

--- 2001:db8:61::2 ping statistics ---
2 packets transmitted, 2 received, 0% packet loss, time 999ms
rtt min/avg/max/mdev = 0.053/0.067/0.082/0.016 ms
mininet>

WORKING trace on mininet on the VM

19:38:49.852088 IP6 2001:db8:61::2 > ff02::1:ff00:1: ICMP6, neighbor solicitation, who has 2001:db8:61::1, length 32
19:38:49.852144 IP6 2001:db8:61::1 > 2001:db8:61::2: ICMP6, neighbor advertisement, tgt is 2001:db8:61::1, length 32
19:38:49.852163 IP6 2001:db8:61::2 > 2001:db8:61::1: ICMP6, echo request, seq 1, length 64
19:38:49.852176 IP6 2001:db8:61::1 > 2001:db8:61::2: ICMP6, echo reply, seq 1, length 64


checking ipv6 in p4-utils

p4@ubuntu:~/p4-utils$ grep -ri ipv6 .
./p4utils/mininetlib/p4_mininet.py:        # disable IPv6
./p4utils/mininetlib/p4_mininet.py:        self.cmd("sysctl -w net.ipv6.conf.all.disable_ipv6=1")
./p4utils/mininetlib/p4_mininet.py:        self.cmd("sysctl -w net.ipv6.conf.default.disable_ipv6=1")
./p4utils/mininetlib/p4_mininet.py:        self.cmd("sysctl -w net.ipv6.conf.lo.disable_ipv6=1")
./p4utils/mininetlib/p4net.py:        #remove Ipv6 for all the interfaces
./p4utils/mininetlib/p4net.py:            cmd2 = "sysctl net.ipv6.conf.{0}.disable_ipv6=1"
./p4utils/mininetlib/p4net.py:            #remove ipv6
Binary file ./p4utils/mininetlib/p4_mininet.pyc matches
Binary file ./p4utils/mininetlib/p4net.pyc matches
Binary file ./p4utils/utils/runtime_API.pyc matches
./p4utils/utils/runtime_API.py:class UIn_BadIPv6Error(UIn_Error):
./p4utils/utils/runtime_API.py:def ipv6Addr_to_bytes(addr):
./p4utils/utils/runtime_API.py:    from ipaddr import IPv6Address
./p4utils/utils/runtime_API.py:        ip = IPv6Address(addr)
./p4utils/utils/runtime_API.py:        raise UIn_BadIPv6Error()
./p4utils/utils/runtime_API.py:        raise UIn_BadIPv6Error()
./p4utils/utils/runtime_API.py:            return ipv6Addr_to_bytes(input_str)
./p4utils/utils/runtime_API.py:        except UIn_BadIPv6Error:
./p4utils/utils/runtime_API.py:            raise UIn_BadParamError("Invalid IPv6 address")
p4@ubuntu:~/p4-utils$


Messages we see in the controller on startup

DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=56 nh=Hop-by-Hop Option Header hlim=1 src=:: dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x6d6d reserved=0 records_number=2 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:1 sources=[  ] auxdata='' |<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:2 |>>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:01:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=36 nh=Hop-by-Hop Option Header hlim=1 src=fe80::201:aff:fe00:2 dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x6604 reserved=0 records_number=1 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:2 |>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=36 nh=Hop-by-Hop Option Header hlim=1 src=fe80::200:aff:fe00:1 dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x6607 reserved=0 records_number=1 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:1 |>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72e res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=56 nh=Hop-by-Hop Option Header hlim=1 src=:: dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x6d6d reserved=0 records_number=2 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:1 sources=[  ] auxdata='' |<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:2 |>>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=36 nh=Hop-by-Hop Option Header hlim=1 src=fe80::200:aff:fe00:1 dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x6607 reserved=0 records_number=1 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:1 |>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=56 nh=Hop-by-Hop Option Header hlim=1 src=fe80::200:aff:fe00:2 dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x63ea reserved=0 records_number=2 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:1 sources=[  ] auxdata='' |<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:2 |>>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:2 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72d res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:02 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:16 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=56 nh=Hop-by-Hop Option Header hlim=1 src=fe80::200:aff:fe00:2 dst=ff02::16 |<IPv6ExtHdrHopByHop  nh=ICMPv6 len=0 autopad=On options=[<RouterAlert  otype=Router Alert [00: skip, 0: Don't change en-route] optlen=2 value=Datagram contains a MLD message |>, <PadN  otype=PadN [00: skip, 0: Don't change en-route] optlen=0 |>] |<ICMPv6MLReport2  type=MLD Report Version 2 res=0 cksum=0x63ea reserved=0 records_number=2 records=[<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:1 sources=[  ] auxdata='' |<ICMPv6MLDMultAddrRec  rtype=4 auxdata_len=0 sources_number=0 dst=ff02::1:ff00:2 |>>] |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72e res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:2 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72d res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:02 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72e res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:02 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:2 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72d res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:02 |>>>>

**** Ignored ICMPv6 packets
We are not using router advertisements, so we ignore RS packets
DEBUG:main:INCOMING: <Ether  dst=33:33:00:00:00:02 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=16 nh=ICMPv6 hlim=255 src=fe80::200:aff:fe00:1 dst=ff02::2 |<ICMPv6ND_RS  type=Router Solicitation code=0 cksum=0xf72e res=0 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>

**** Double table entries due to collision
      - NDP: last 24 bit
      - Switch has same ending address in different networks -> equal
        last 24 bit
      - results in trying to add multicast address multiple times

Adding entry to exact match table v6_addresses
match key:           EXACT-ff:02:00:00:00:00:00:00:00:00:00:01:ff:00:00:42
action:              controller_reply
runtime data:        00:01
Invalid table operation (DUPLICATE_ENTRY)
Adding entry to exact match table v6_addresses
match key:           EXACT-ff:02:00:00:00:00:00:00:00:00:00:01:ff:00:00:43
action:              controller_reply
runtime data:        00:01
Invalid table operation (DUPLICATE_ENTRY)
Adding entry to exact match table v6_addresses
match key:           EXACT-20:01:0d:b8:00:00:00:01:00:00:00:00:00:00:00:43
action:              icmp6_echo_reply
runtime data:
Entry has been added with handle 5

**** General approach
     - Need to react on our multicast group
     - But also need to forward to other ports that subscribed to
       that multicast group!
*** Static mappings
     - likely need table(s)
     - need tcp & udp translation
*** ICMPv6
**** General / Intro
Different lengths possible

[20:35] line:~% ping -6 -s 20 ::1
PING ::1(::1) 20 data bytes
28 bytes from ::1: icmp_seq=1 ttl=64 time=0.045 ms
28 bytes from ::1: icmp_seq=2 ttl=64 time=0.064 ms
^C
--- ::1 ping statistics ---
2 packets transmitted, 2 received, 0% packet loss, time 1018ms
rtt min/avg/max/mdev = 0.045/0.054/0.064/0.012 ms
[20:36] line:~% ping -6 -s 80 ::1
PING ::1(::1) 80 data bytes
88 bytes from ::1: icmp_seq=1 ttl=64 time=0.053 ms
88 bytes from ::1: icmp_seq=2 ttl=64 time=0.095 ms
^C
--- ::1 ping statistics ---
2 packets transmitted, 2 received, 0% packet loss, time 1001ms
rtt min/avg/max/mdev = 0.053/0.074/0.095/0.021 ms
[20:36] line:~%

Different checksum in most packets.

root@ubuntu:~/master-thesis# ip -6 neigh show
root@ubuntu:~/master-thesis# ip -6 neigh add 2001:db8:61::42 dev h1-eth0 lladdr 00:00:0a:00:00:42
root@ubuntu:~/master-thesis# ip -6 neigh show
2001:db8:61::42 dev h1-eth0 lladdr 00:00:0a:00:00:42 PERMANENT
root@ubuntu:~/master-thesis#

root@ubuntu:~/master-thesis# tcpdump -ni h1-eth0
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on h1-eth0, link-type EN10MB (Ethernet), capture size 262144 bytes
^C20:22:43.944152 IP6 2001:db8:61::1 > 2001:db8:61::42: ICMP6, echo request, seq 1, length 64
20:22:43.945992 IP6 2001:db8:61::1 > 2001:db8:61::42: ICMP6, echo request, seq 1, length 64
20:22:44.952453 IP6 2001:db8:61::1 > 2001:db8:61::42: ICMP6, echo request, seq 2, length 64
20:22:44.953995 IP6 2001:db8:61::1 > 2001:db8:61::42: ICMP6, echo request, seq 2, length 64

4 packets captured
4 packets received by filter
0 packets dropped by kernel
root@ubuntu:~/master-thesis#
**** When pinging we see
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8:61::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd343 res=0 tgt=2001:db8:61::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8:61::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd343 res=0 tgt=2001:db8:61::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>
DEBUG:main:INCOMING: <Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8:61::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0xd343 res=0 tgt=2001:db8:61::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>>

**** Hosts
***** Left side: IPv6
***** Right side: IPv4
**** Included in the header

**** DONE Supported feature: NDP NA/NS
- For resolving mac address
- Initially controller
- Ported into switch
**** DONE Supported feature: icmp6 echo reply
p4@ubuntu:~/master-thesis/p4app$ python test.py  --method ping6_switch
PING 2001:db8::42(2001:db8::42) 56 data bytes
64 bytes from 2001:db8::42: icmp_seq=1 ttl=64 time=3.05 ms

--- 2001:db8::42 ping statistics ---
1 packets transmitted, 1 received, 0% packet loss, time 0ms
rtt min/avg/max/mdev = 3.055/3.055/3.055/0.000 ms
p4@ubuntu:~/master-thesis/p4app$

*** Requirements
*** Static NAT64
Asymmetric maps: v6->v4 can match whole IPv4 Internet (/96)
But v4->v6 can only map sub range!
Using /24s (for convience) in IPv4
*** Development mode/loop
Code - commit - push - pull -
restart switch - check whether all tables are present (missing .apply())
restart controller - check whether tables are applied correctly (type conversion problems) -
start tcpdump - start test program - stop tcpdump - add
pcap to git repo - git add-commit-push - git pull - start wireshark -
debug packets - analyse code - goto 1
*** Setting up a system for working on P4 on devuan
**** Scripts in the wild
     https://github.com/nsg-ethz/p4-learning/blob/master/vm/bin/update-p4c.sh
     https://github.com/jafingerhut/p4-guide/blob/master/bin/install-p4dev-p4runtime.sh
     https://github.com/nsg-ethz/p4-learning/tree/master/vm/bin
**** mininet
**** bmv2
[21:24] line:~% sudo apt install libthrift-dev
[21:26] line:~% sudo apt install thrift-compiler
libnanomsg-dev libjudy-dev

*** TODO Session / dynamice mappings
**** General
     - Have 1..n session IPv4 addresses
     - Handle outgoing IPv6: create new session
     - Handle in
***** TODO Case IPv6 initiator
      - Mapping whole IPv4 Internet in /96 prefix
      - Session information for mapping reply
      - Timeout handling in controller
****** TODO IPv6 udp -> IPv4
       - Got 4-5 tuple ([proto], src ip, src port, dst ip, dst port)
       - Does not / never signal end
       - Needs timeout for cleaning up
****** TODO IPv6 tcp -> IPv4
       - Similar to udp
       - react on FIN/RST (?) -- could be an addition
****** TODO IPv6 icmp6 -> IPv4
       - usual protocol specific changes
       - Session??
       - src ip, dst ip, code ?

***** TODO Case IPv4 initiator
      - Needs upper level protol
**** TODO General network matching
***** DONE Create table(s)
***** DONE Fill it up from the controller: general network
***** TODO Create controller session handler
****** Controller Logic
       - controller selects "outgoing" IPv4 address range => base for sessions
       - IPv4 addresses can be "random" (in our test case), but need
         to be unique
       - switch does not need to know about the "range", only about
         sessions
       - on session create, controller selects "random" ip (ring?)
       - on session create, controller selects "random port" (next in range?)
       - on session create controller adds choice into 2 tables:
         incoming, outgoing

***** DONE Feed back to controller: implemented in switch
***** DONE Create ipv6 session in the controller
***** Create ipv4 session in the controller
***** TODO Ensure translation code works
>>> ipaddress.IPv6Network("2001:db8:100::/96")[int(ipaddress.IPv4Address("10.0.0.1"))]
IPv6Address('2001:db8:100::a00:1')

****** DONE Status: syn sent, neighbor solicitation working, nothing received on other side

INFO:main:unhandled reassambled=<Ether  dst=33:33:ff:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=0 plen=32 nh=ICMPv6 hlim=255 src=2001:db8::1 dst=ff02::1:ff00:42 |<ICMPv6ND_NS  type=Neighbor Solicitation code=0 cksum=0x13a7 res=0 tgt=2001:db8::42 |<ICMPv6NDOptSrcLLAddr  type=1 len=1 lladdr=00:00:0a:00:00:01 |>>>> from table TABLE_NAT64_SESSION
INFO:main:unhandled reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=667225 plen=40 nh=TCP hlim=64 src=2001:db8::1 dst=2001:db8:100::a00:1 |<TCP  sport=36458 dport=2342 seq=1287954527 ack=0 dataofs=10 reserved=0 flags=S window=28320 chksum=0xdfd6 urgptr=0 options=[('MSS', 9440), ('SAckOK', ''), ('Timestamp', (795131854, 0)), ('NOP', None), ('WScale', 9)] |>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=667225 plen=40 nh=TCP hlim=64 src=2001:db8::1 dst=2001:db8:100::a00:1 |<TCP  sport=36458 dport=2342 seq=1287954527 ack=0 dataofs=10 reserved=0 flags=S window=28320 chksum=0xdedc urgptr=0 options=[('MSS', 9440), ('SAckOK', ''), ('Timestamp', (795132104, 0)), ('NOP', None), ('WScale', 9)] |>>> from table TABLE_V6_NETWORKS
INFO:main:unhandled reassambled=<Ether  dst=00:00:0a:00:00:42 src=00:00:0a:00:00:01 type=0x86dd |<IPv6  version=6 tc=0 fl=765494 plen=40 nh=TCP hlim=64 src=2001:db8::1 dst=2001:db8:100::a00:1 |<TCP  sport=36458 dport=2342 seq=1287954527 ack=0 dataofs=10 reserved=0 flags=S window=28320 chksum=0xdce7 urgptr=0 options=[('MSS', 9440), ('SAckOK', ''), ('Timestamp', (795132605, 0)), ('NOP', None), ('WScale', 9)] |>>> from table TABLE_V6_NETWORKS

****** DONE action nat64_tcp_session_create is called
**** TODO tcp session
**** TODO udp session
**** TODO tcp session
** TODO Hardware port
*** Installation issues
Installing vivado would stall/sleep/hang forverer due to missing
system library, no error output.
*** Build process
- Very fragile, many pieces, unclear which step is required for creating
what.
- Fails at every step
- Dependencies in over 80k lines of code (Makefile, python, shell)
- Unclear error messages
  Some step did something and another step fails due do something that
  was generated by a step that is not clear what it is supposed to do
- one step huge output, hundreds to thousands of lines, errors
  somewher in between => exceeding tmux buffers
- some steps take VERY long correctly
- some steps stopped in an infinite loop => hard to distinguish
- non fatal/fatal errors cannot be distinguished
grep: ../../../RELEASE_NOTES: No such file or directory

** TODO Comparison with existing tools (Performance, Features)
*** Features
| What?               | Description                              | State in P4       | References                                                                      |
|---------------------+------------------------------------------+-------------------+---------------------------------------------------------------------------------|
| Jool EAMT           | Mapping with tables, multiple entries    | Supported         | https://www.jool.mx/en/eamt.html, https://www.jool.mx/en/run-eam.html, RFC 7757 |
| Jool SIIT           | Mapping IPv6 to range of IPv4, one entry | Supported by EAMT |                                                                                 |
| Jool Stateful NAT64 |                                          |                   | https://www.jool.mx/en/intro-xlat.html#stateful-nat64                           |
|                     |                                          |                   | https://www.jool.mx/en/run-nat64.html                                           |
|                     |                                          |                   |                                                                                 |
** P4 Possible Improvements / Current Challenges / Limitations
*** DONE cannot read key from table
**** log
Key and mask for matching destination is in table. We need this
 information in the action. However this information is not exposed, so
 we need to specify another parameter with the same information as in
 the key(s).

 Log from slack: (2019-03-14)

 nico [1:55 PM]
 If I use LPM for matching, can I easily get the network address from P4 or do I have to use a bitmask myself? In the latter case it is not exactly clear how to get the mask from the table

 Nate Foster [1:58 PM]
 You want to retrieve the address in the packet? In a table?
 And do you want to do the retrieving from the data plane or the control plane? (edited)

 nico [2:00 PM]
 If I have a match in a table that matches on LPM, it can be any IP address in a network
 For calculating the NAT64/NAT46 translation, I will need the base address, i.e. network address to do subtractions/additions
 So it is fully data plane, what I would like to do
 I'll commit sample code to show the use case more clearly
 https://gitlab.ethz.ch/nicosc/master-thesis/blob/master/p4src/static-mapping.p4#L73
 GitLab
 p4src/static-mapping.p4 · master · nicosc / master-thesis
 gitlab.ethz.ch
 So the action nat64_static() is used in the table v6_networks.
 In v6_networks I use a match on `hdr.ipv6.dst_addr: lpm;`
 What I would like to be able is to get the network address ; I can do that manually, if I have the mask
 I can also re-inject this parameter by another action argument, but I'd assume that I can somewhere read this out from the table / match

 Nate Foster [2:15 PM]
 To make sure I understand, in the data plane, you want to retrieve the address in the lpm pattern? (edited)

 nico [2:16 PM]
 I want to retrieve the key

 Nate Foster [2:16 PM]
 Wait. The value `hdr.ipv6.dst_addr` is the thing used in the match.
 So you have that.
 What you don’t have is the IPv6 address and mask put into the table by the control plane.
 I assume you want the latter, right?

 nico [2:17 PM]
 For example, if my matching key is 2001:db8::/32 and the real address is 2001:db8::f00, then I would like to retrieve 2001:db8:: and 32 from the table
 exactly :slightly_smiling_face:
 I can "fix" this by adding another argument, but it feels somewhat wrong to do that
 Because the table already knows this information

 Nate Foster [2:26 PM]
 I can’t think of a way other than the action parameter hack.

 nico [2:26 PM]
 Oh, ok
 Is it because the information is "lost in hardware"?

 Nate Foster [2:31 PM]
 No you’re right that most implementations have the value in memory. And one can imagine a different table API that allowed one to retrieve it in the data plane.
 But unless I am missing something obvious, P4 hides it…

**** Result
Need to duplicate information

*** DONE ICMP6: checksum over payload
     - variable length, up to 65k
Exists!
*** DONE Synchronisation with the controller
    - Double data type definition -> might differ
    - TYPE_CPU for ethernet
    - Port ingress offset (9 vs. 16 bit)

*** p4c expression bug 2019-03-30
Hit in master-thesis 0.4-28-g881643e

#+BEGIN_SRC
Warning: you requested the nanomsg event logger, but bmv2 was compiled without -DBMELOG, and the event logger cannot be activated
Calling target program-options parser
[14:01:44.334] [bmv2] [D] [thread 23356] Set default default entry for table 'MyIngress.icmp6': MyIngress.controller_debug_table_id - 2,
[14:01:44.341] [bmv2] [D] [thread 23356] Set default default entry for table 'MyIngress.nat64': MyIngress.controller_debug_table_id - 1,
[14:01:44.344] [bmv2] [D] [thread 23356] Set default default entry for table 'tbl_act': act -
[14:01:44.345] [bmv2] [D] [thread 23356] Set default default entry for table 'tbl_act_0': act_0 -
[14:01:44.345] [bmv2] [D] [thread 23356] Set default default entry for table 'tbl_nat64_icmp6_generic': MyIngress.nat64_icmp6_generic -
[14:01:44.345] [bmv2] [D] [thread 23356] Set default default entry for table 'tbl_act_1': act_1 -
[14:01:44.345] [bmv2] [D] [thread 23356] Set default default entry for table 'tbl_act_2': act_2 -
[14:01:44.345] [bmv2] [D] [thread 23356] Set default default entry for table 'MyIngress.v4_networks': MyIngress.controller_debug_table_id - 5,
[14:01:44.345] [bmv2] [D] [thread 23356] Set default default entry for table 'MyIngress.v6_networks': MyIngress.controller_debug_table_id - 3,
[14:01:44.346] [bmv2] [D] [thread 23356] Set default default entry for table 'tbl_act_3': act_3 -
Invalid entry type 'expression' in field list
bad json:
{
   "type" : "expression",
   "value" : {
      "type" : "expression",
      "value" : {
         "left" : null,
         "op" : "d2b",
         "right" : {
            "type" : "field",
            "value" : [ "scalars", "metadata.chk_icmp6_na_ns" ]
         }
      }
   }
}


#+END_SRC

*** DONE Only one LPM key supported in tables (2019-03-23)
Priority support in ternary possible. Means rewriting for
developers. Could possibly be supported by switching to ternary mode
internally.

#+BEGIN_SRC
../p4src/static-mapping.p4(121): error: MyIngress.nat64, Multiple LPM keys in table
    table nat64 {
          ^^^^^
Compilation Error
#+END_SRC

Code:
#+BEGIN_SRC
    table nat64 {
        key = {
            hdr.ipv6.src_addr: lpm;
            hdr.ipv6.dst_addr: lpm;
        }
        actions = {
            controller_debug;
            nat64_static;
            NoAction;
        }
        size = NAT64_TABLE_SIZE;
        default_action = controller_debug;
    }
#+END_SRC

*** No table meta information for default actions (asked 2019-03-25)
Is there any meta information for "from which table was the action
called" available? My use case is having a debug action that sends
packets to the controller and I use it as a default_action in various
tables; however know I don't know anymore from which table the action
was called. Is there any kind of meta information which table called
me available?

I could work around this by using if(! .. .hit) { my_action(table_id)
}, but it would not work with using default_action = ...

*** DONE No switch in actions, No conditional execution in actions
**** 3 possible solutions
     - multi table (state as of 2019-03-28)
     - switch/if in actions: with shadow tables
     - switch/if in apply block

**** log
Imho, compiler should be able to unroll these to some degree.

#+BEGIN_SRC
../p4src/static-mapping.p4(60): error: SwitchStatement: switch statements not allowed in actions
        switch(hdr.icmp6.type) {
        ^^^^^^
#+END_SRC

#+BEGIN_SRC
../p4src/static-mapping.p4(57): error: MethodCallStatement: Conditional execution in actions is not supported on this target
        hdr.icmp.setValid();
        ^^^^^^^^^^^^^^^^^^^
../p4src/static-mapping.p4(70): error: MethodCallStatement: Conditional execution in actions is not supported on this target
        hdr.icmp6.setInvalid();
        ^^^^^^^^^^^^^^^^^^^^^^
../p4src/static-mapping.p4(73): error: MethodCallStatement: Conditional execution in actions is not supported on this target
        hdr.icmp6_na_ns.setInvalid();
        ^^^^^^^^^^^^^^^^^^^^^^^^^^^^
../p4src/static-mapping.p4(74): error: MethodCallStatement: Conditional execution in actions is not supported on this target
        hdr.icmp6_option_link_layer_addr.setInvalid();
        ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
Compilation Error
p4@ubuntu:~/master-thesis/p4app$
#+END_SRC

Code:

#+BEGIN_SRC
        if(hdr.ipv6.next_header == PROTO_ICMP6) {
            nat64_icmp6();
        }
#+END_SRC

*** TODO Modules, OS
Not addressed so far: how to create re-usable code fragments that can
be plugged in easily. There could be a hypothetical "P4OS" that
manages code fragments. This might include, but not limited to
downloading (signed?) source code, managing dependencies similar to
Linux package management, handling updates, etc.
*** TODO Code sharing (controller, switch)
Many constants double defined. Easy to make errors.

*** Checksum handling: v6->v4 adding, not checking
Currently checksums are NOT checked. For translation v6->v4 this means
we add a checksum without ever checking v4 checksum before.

** Implementation description and limitations
*** Implementation description [move todos here]
**** TODO Support (non-) fragmentation
     - if DF bit is not set in ipv4
**** TODO Supporting [different] MTUs
     - sizes of headers are different
     - packet might not fit into same mtu anymore
     - send back "ICMP Packet  Too Big messages to the sender." RFC7915
**** TODO pmtud support
     - mss change
#+BEGIN_QUOTE
translator MUST send a
   Packet Too Big error message or fragment the packet when the packet
   size exceeds the MTU of the next-hop interface.
#+END_QUOTE

https://tools.ietf.org/html/rfc7915

*** Limitations
**** IPv4 embedding (RFC6052, RFC4291)
Supported is similar to the  "IPv4-Compatible IPv6 Address" as defined by
rfc4291 section 2.5.5.1. Longer prefixes can be specified, but
effectively last part used. Not ensuring 16 0 bits. Deprecated
according to RFC4291.

Also section 2.5.5.2 "IPv4-Mapped IPv6 Address"

     - Only correctly support /96 prefix
     - Other modes also embed in last 32 bits
     - However supports any prefix length >= 96


Mac addresses: bit 0 = unicast (0)/multicast(1),
bit 1 = local (1)/global (0) - site wiki/mac

U/L bit is universal/local, bit 2; inverting: local = 0, global = 1

**** No fragmentation support (yet)
In line with RFC7915
#+BEGIN_QUOTE
Fragmented ICMP/ICMPv6 packets will not be translated by IP/ICMP    translators.
#+END_QUOTE
**** No session handling (yet)
 1:1 mappings. No (automatic) session.
**** IPv4 / IPv6 embedding
 Currently offset based - probably not following the RFC!
**** No DNS64
 has already been solved in a different domain - could even do
 transparent / in network modification
**** Incomplete NDP
     Very limited option support
**** NAT64 mappings not source network dependent
 Only the destination network is matched for deciding on NAT64, as
 priority based double LPM is not supported. This limits a prefix to be
 used only in one network.
**** TODO No resolution of hardware addresses
      - hardcoded ip --> mac addresses
 Correct version:
 Resolve mac address in controller, buffer packet, replay packet /
 handle packet.
 Only has to be set, when packets originate from the switch/controller.

**** TODO No support of IPv4 options
     - header is assumed to be always 20 octets


**** TODO Security issue: not checking checksums before
     - Could be implemented

** Log various
*** 2019-06-06
No device seen after loading modules after reboot - netfpga.
Trying to reprogram

#+BEGIN_CENTER
+ xsct /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl -tclargs minip4.bit
rlwrap: warning: your $TERM is 'screen' but rlwrap couldn't find it in the terminfo database. Expect some problems.
RUN loading image file.
minip4.bit
attempting to launch hw_server

 ****** Xilinx hw_server v2018.2
  **** Build date : Jun 14 2018-20:18:37
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

INFO: hw_server application started
INFO: Use Ctrl-C to exit hw_server application

INFO: To connect to this hw_server instance use url: TCP:127.0.0.1:3121

100%   11MB   1.7MB/s  00:06

+ bash /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/pci_rescan_run.sh
Check programming FPGA or Reboot machine !
+ rmmod sume_riffa
rmmod: ERROR: Module sume_riffa is not currently loaded
+ modprobe sume_riffa
+ ifconfig nf0 up
nf0: ERROR while getting interface flags: No such device
+ ifconfig nf1 up
nf1: ERROR while getting interface flags: No such device
+ ifconfig nf2 up
nf2: ERROR while getting interface flags: No such device
+ ifconfig nf3 up
nf3: ERROR while getting interface flags: No such device
+ bash config_writes.sh
root@rainbow:~/master-thesis/netpfga/minip4/simple_sume_switch/bitfiles#

#+END_CENTER
Full run, messages are the same:

#+BEGIN_CENTER
+ xsct /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl -tclargs minip4.bit
rlwrap: warning: your $TERM is 'screen' but rlwrap couldn't find it in the terminfo database. Expect some problems.
RUN loading image file.
minip4.bit
attempting to launch hw_server

 ****** Xilinx hw_server v2018.2
  **** Build date : Jun 14 2018-20:18:37
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

INFO: hw_server application started
INFO: Use Ctrl-C to exit hw_server application

INFO: To connect to this hw_server instance use url: TCP:127.0.0.1:3121

100%   10MB   1.7MB/s  00:06
+ bash /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/pci_rescan_run.sh
Check programming FPGA or Reboot machine !
+ rmmod sume_riffa
rmmod: ERROR: Module sume_riffa is not currently loaded
+ modprobe sume_riffa
+ ifconfig nf0 up
nf0: ERROR while getting interface flags: No such device
+ ifconfig nf1 up
nf1: ERROR while getting interface flags: No such device
+ ifconfig nf2 up
nf2: ERROR while getting interface flags: No such device
+ ifconfig nf3 up
nf3: ERROR while getting interface flags: No such device
+ bash config_writes.sh
[0:33] rainbow:minip4% sudo reboot

#+END_CENTER
*** 2019-06-07: exec format error
Trying to load kernel module now gives an error:

#+BEGIN_CENTER
[7:05] rainbow:netpfga% . ./bashinit
[7:05] rainbow:netpfga% bash  build-load-drivers.sh
+ cd /home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0
+ make all
make -C /lib/modules/5.0.0-16-generic/build M=/home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0 modules
make[1]: Entering directory '/usr/src/linux-headers-5.0.0-16-generic'
  Building modules, stage 2.
  MODPOST 1 modules
make[1]: Leaving directory '/usr/src/linux-headers-5.0.0-16-generic'
+ sudo make install
make -C /lib/modules/5.0.0-16-generic/build M=/home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0 modules
make[1]: Entering directory '/usr/src/linux-headers-5.0.0-16-generic'
  Building modules, stage 2.
  MODPOST 1 modules
make[1]: Leaving directory '/usr/src/linux-headers-5.0.0-16-generic'
install -o root -g root -m 0755 -d /lib/modules/5.0.0-16-generic/extra/sume_riffa/
install -o root -g root -m 0755 sume_riffa.ko /lib/modules/5.0.0-16-generic/extra/sume_riffa/
depmod -a 5.0.0-16-generic
+ sudo modprobe sume_riffa
modprobe: ERROR: could not insert 'sume_riffa': Exec format error
[7:06] rainbow:netpfga%

#+END_CENTER

dmesg:

#+BEGIN_CENTER
[  257.356321] sume_riffa: version magic '5.0.0-15-generic SMP mod_unload ' should be '5.0.0-16-generic SMP mod_unload '

#+END_CENTER

Rebuilding module:

#+BEGIN_CENTER
[7:08] rainbow:sume_riffa_v1_0_0% make clean
make -C /lib/modules/5.0.0-16-generic/build M=/home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0 clean
make[1]: Entering directory '/usr/src/linux-headers-5.0.0-16-generic'
  CLEAN   /home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0/.tmp_versions
  CLEAN   /home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0/Module.symvers
make[1]: Leaving directory '/usr/src/linux-headers-5.0.0-16-generic'
[7:08] rainbow:sume_riffa_v1_0_0% make all
make -C /lib/modules/5.0.0-16-generic/build M=/home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0 modules
make[1]: Entering directory '/usr/src/linux-headers-5.0.0-16-generic'
  CC [M]  /home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0/sume_riffa.o
  Building modules, stage 2.
  MODPOST 1 modules
  CC      /home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0/sume_riffa.mod.o
  LD [M]  /home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0/sume_riffa.ko
make[1]: Leaving directory '/usr/src/linux-headers-5.0.0-16-generic'
[7:08] rainbow:sume_riffa_v1_0_0% sudo make install
sudo modprobe sume_riffa

make -C /lib/modules/5.0.0-16-generic/build M=/home/nico/projects/P4-NetFPGA/lib/sw/std/driver/sume_riffa_v1_0_0 modules
make[1]: Entering directory '/usr/src/linux-headers-5.0.0-16-generic'
  Building modules, stage 2.
  MODPOST 1 modules
make[1]: Leaving directory '/usr/src/linux-headers-5.0.0-16-generic'
install -o root -g root -m 0755 -d /lib/modules/5.0.0-16-generic/extra/sume_riffa/
install -o root -g root -m 0755 sume_riffa.ko /lib/modules/5.0.0-16-generic/extra/sume_riffa/
depmod -a 5.0.0-16-generic
[7:08] rainbow:sume_riffa_v1_0_0%

#+END_CENTER

The devices are back:

#+BEGIN_CENTER
[7:08] rainbow:sume_riffa_v1_0_0% ip l
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN mode DEFAULT group default qlen 1000
    link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
2: eth0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc mq state UP mode DEFAULT group default qlen 1000
    link/ether 70:85:c2:ad:62:79 brd ff:ff:ff:ff:ff:ff
3: wlan0: <NO-CARRIER,BROADCAST,MULTICAST,UP> mtu 1500 qdisc mq state DOWN mode DORMANT group default qlen 1000
    link/ether dc:8b:28:47:5c:f7 brd ff:ff:ff:ff:ff:ff
4: nf0: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:00 brd ff:ff:ff:ff:ff:ff
5: nf1: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:01 brd ff:ff:ff:ff:ff:ff
6: nf2: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:02 brd ff:ff:ff:ff:ff:ff
7: nf3: <BROADCAST,MULTICAST> mtu 1500 qdisc noop state DOWN mode DEFAULT group default qlen 1000
    link/ether 02:53:55:4d:45:03 brd ff:ff:ff:ff:ff:ff
[7:09] rainbow:sume_riffa_v1_0_0%

#+END_CENTER
*** 2019-06-08: adding table entries

mac = 02:53:55:42:45:01 (from send_packet.py)

#+BEGIN_CENTER
>> list_cam_tables
------------
lookup_table :
------------
{u'action_ids': {u'TopPipe.do_nothing': 2,
                 u'TopPipe.send_to_port1': 3,
                 u'TopPipe.swap_eth_addresses': 1},
 u'annotations': {u'Xilinx_ExternallyConnected': [u'0'],
                  u'Xilinx_LookupEngineType': [u'EM'],
                  u'name': [u'TopPipe.lookup_table']},
 u'match_type': u'EM',
 u'p4_name': u'lookup_table',
 u'px_class': u'LookupEngine',
 u'px_name': u'lookup_table',
 u'px_type_name': u'lookup_table_t',
 u'request_fields': [{u'p4_name': u'p.ethernet.dstAddr',
                      u'px_name': u'lookup_request_key',
                      u'size': 48,
                      u'type': u'bits'}],
 u'response_fields': [{u'px_name': u'hit', u'size': 1, u'type': u'bits'},
                      {u'px_name': u'action_run',
                       u'size': 2,
                       u'type': u'bits'}]}
>>

root@rainbow:~# ip l s nf0 up

>> table_cam_add_entry
ERROR:
table_cam_add_entry <table_name> <action_name> <keys> => <action_data>
DESCRIPTION: Add an entry to the specified table
PARAMS:
    <table_name> : name of the table to add an entry to
    <action_name> : name of the action to use in the entry (must be listed in the table's actions list)
    <keys> : space separated list of keys to use as the entry key (must correspond to table's keys in the order defined in the P4 program)
    <action_data> : space separated list of values to provide as input to the action

['']

>> table_cam_add_entry lookup_table send_to_port1 ff:ff:ff:ff:ff:ff
ERROR:
table_cam_add_entry <table_name> <action_name> <keys> => <action_data>
DESCRIPTION: Add an entry to the specified table
PARAMS:
    <table_name> : name of the table to add an entry to
    <action_name> : name of the action to use in the entry (must be listed in the table's actions list)
    <keys> : space separated list of keys to use as the entry key (must correspond to table's keys in the order defined in the P4 program)
    <action_data> : space separated list of values to provide as input to the action

['lookup_table send_to_port1 ff:ff:ff:ff:ff:ff']
[20:09] rainbow:CLI% python P4_SWITCH_CLI.py
loading libsume..
loading libsume..
loading libcam..
The SimpleSumeSwitch interactive command line tool
 type help to see all commands
>> table_cam_add_entry lookup_table send_to_port1 => ff:ff:ff:ff:ff:ff
ERROR:
table_cam_add_entry <table_name> <action_name> <keys> => <action_data>
DESCRIPTION: Add an entry to the specified table
PARAMS:
    <table_name> : name of the table to add an entry to
    <action_name> : name of the action to use in the entry (must be listed in the table's actions list)
    <keys> : space separated list of keys to use as the entry key (must correspond to table's keys in the order defined in the P4 program)
    <action_data> : space separated list of values to provide as input to the action

[20:10] rainbow:CLI%


table_cam_add_entry lookup_table send_to_port1 ff:ff:ff:ff:ff:ff => ""

>> table_cam_add_entry lookup_table send_to_port1 ff:ff:ff:ff:ff:ff =>
CAM_Init_ValidateContext() - done
WROTE 0x44020050 = 0xffffffff
WROTE 0x44020054 = 0xffff
WROTE 0x44020080 = 0x0003
python: ioctl: Unknown error 512
[20:27] rainbow:CLI%

#+END_CENTER

*** 2019-06-10: testing with INT (hint from Hendrik)
**** 15:54 compile & upload done
**** 16:36 ...testing
***** replaced ethX with nfX
 #+BEGIN_CENTER
root@rainbow:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/int/sw/hw_test_tool# ./rcv_int.py
root@rainbow:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/int/sw/hw_test_tool# ./int_tester.py
tcpdump: listening on nf1, link-type EN10MB (Ethernet), capture size 262144 bytes
The HW testing tool for the INT design
 type help to see all commands
testing> help

Documented commands (type help <topic>):
========================================
help  run_test

Undocumented commands:
======================
EOF  exit

testing> run_test 0b11001
.
Sent 1 packets.
Sent pkt:
------------------------------------------------------------------------------------------
|  ETHERNET  | ins_cnt:3          max_hop:10         total_hop:0          bitmask:11001      |
------------------------------------------------------------------------------------------

testing>


 #+END_CENTER
***** DONE Receiver does not see any packet
      CLOSED: [2019-06-10 Mon 16:37]
***** DONE testing with tcpdump and ETH_DST = "ff:ff:ff:ff:ff:ff"
      CLOSED: [2019-06-10 Mon 17:34]
Sending on nf1, listenng on nf3, all interfaces up

#+BEGIN_CENTER
root@rainbow:~# tcpdump -ni nf3
tcpdump: verbose output suppressed, use -v or -vv for full protocol decode
listening on nf3, link-type EN10MB (Ethernet), capture size 262144
bytes

root@rainbow:~/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/int/sw/hw_test_tool# ./int_tester.py
tcpdump: listening on nf1, link-type EN10MB (Ethernet), capture size 262144 bytes
The HW testing tool for the INT design
 type help to see all commands
testing> run_test 0b11001
.
Sent 1 packets.
Sent pkt:
------------------------------------------------------------------------------------------
|  ETHERNET  | ins_cnt:3          max_hop:10         total_hop:0          bitmask:11001      |
------------------------------------------------------------------------------------------

testing> run_test 0b11001
.
Sent 1 packets.
Sent pkt:
------------------------------------------------------------------------------------------
|  ETHERNET  | ins_cnt:3          max_hop:10         total_hop:0          bitmask:11001      |
------------------------------------------------------------------------------------------

testing>

#+END_CENTER

-> no packet received on nf3, even though commands.txt contains
mapping
*** 2019-06-10: trying to output on all ports -> unclear test data
Test data in gen_testdata.py expects order. If we output to 0b1010101
(=85), then the packet should arrive on all ports. Order unknown.

*** 2019-06-11: rebooted -> card is missing from lspci
reprogramming. why is it missing?

#+BEGIN_CENTER
[18:25] rainbow:bitfiles% sudo bash -c ". $HOME/master-thesis/netpfga/bashinit && $(pwd -P)/program_switch.sh"
++ which vivado
+ xilinx_tool_path=/opt/Xilinx/Vivado/2018.2/bin/vivado
+ bitimage=int.bit
+ configWrites=config_writes.sh
+ '[' -z int.bit ']'
+ '[' -z config_writes.sh ']'
+ '[' /opt/Xilinx/Vivado/2018.2/bin/vivado == '' ']'
+ rmmod sume_riffa
rmmod: ERROR: Module sume_riffa is not currently loaded
+ xsct /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/run_xsct.tcl -tclargs int.bit
rlwrap: warning: your $TERM is 'screen' but rlwrap couldn't find it in the terminfo database. Expect some problems.
RUN loading image file.
int.bit
attempting to launch hw_server

****** Xilinx hw_server v2018.2
  **** Build date : Jun 14 2018-20:18:37
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

INFO: hw_server application started
INFO: Use Ctrl-C to exit hw_server application

INFO: To connect to this hw_server instance use url: TCP:127.0.0.1:3121

100%   13MB   1.7MB/s  00:08

+ bash /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/tools/pci_rescan_run.sh
Check programming FPGA or Reboot machine !
+ rmmod sume_riffa
rmmod: ERROR: Module sume_riffa is not currently loaded
+ modprobe sume_riffa
+ ifconfig nf0 up
nf0: ERROR while getting interface flags: No such device
+ ifconfig nf1 up
nf1: ERROR while getting interface flags: No such device
+ ifconfig nf2 up
nf2: ERROR while getting interface flags: No such device
+ ifconfig nf3 up
nf3: ERROR while getting interface flags: No such device
+ bash config_writes.sh
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device
rwaxi: ioctl: No such device

#+END_CENTER

After reprogram AND reboot:

10:00.0 Memory controller: Xilinx Corporation Device 7028

*** 2019-06-12: try broadcasting
#+BEGIN_CENTER
[SW] CAM_EnableDevice() - done
[2274090]  INFO: finished packet stimulus file
[2735572] ERROR: tuple mismatch for packet 1
expected < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001040000 >
actual   < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000055040000 >
$finish called at time : 2735572 ps : File "/home/nico/master-thesis/netpfga/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v" Line 120
exit

#+END_CENTER

-> mismatch when using expPkt on all ports
-> trying to use bcast fails due to programming errors
-> using bcast in the map -> breaks config_writes.py

Using bcast, following output :

#+BEGIN_CENTER
SV_write_control()- done
[SW] CAM_EnableDevice() - done
[2274090]  INFO: finished packet stimulus file
[2735572]  INFO: packet 1 tuple OK < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000055040000 >
[2735572]  INFO: packet 1  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000090012222222208022222222208)
[2738904]  INFO: packet 1  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[2745568]  INFO: packet 2 tuple OK < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000055100000 >
[2745568]  INFO: packet 2  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000090012222222208022222222208)
[2748900]  INFO: packet 2  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[2755564]  INFO: packet 3 tuple OK < tuple_out_digest_data, tuple_out_sume_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000055400000 >
[2755564]  INFO: packet 3  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000090012222222208022222222208)
[2758896]  INFO: packet 3  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[6094228]  INFO: stopping simulation after 1000 idle cycles
[6094228]  INFO: all expected data successfully received
[6094228]  INFO: TEST PASSED
$finish called at time : 6094228 ps : File "/home/nico/master-thesis/netpfga/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/SimpleSumeSwitch_tb.sv" Line 207
exit

#+END_CENTER

-> nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt isn't generated correctly

*** 2019-06-13: try downgrading kernel: requires outdated libssl that is not there in 18.x
#+BEGIN_CENTER
root@rainbow:/home/nico# mkdir ubuntu
root@rainbow:/home/nico# mv linux-* ubuntu/
root@rainbow:/home/nico# cd ubuntu/
root@rainbow:/home/nico/ubuntu# ls
linux-headers-4.10.0-32-generic_4.10.0-32.36~16.04.1_amd64.deb  linux-image-4.10.0-32-generic_4.10.0-32.36~16.04.1_amd64.deb
root@rainbow:/home/nico/ubuntu#

..
run-parts: executing /etc/kernel/postinst.d/zz-update-grub 4.10.0-32-generic /boot/vmlinuz-4.10.0-32-generic
Sourcing file `/etc/default/grub'
Sourcing file `/etc/default/grub.d/50-curtin-settings.cfg'
Sourcing file `/etc/default/grub.d/init-select.cfg'
Generating grub configuration file ...
Found linux image: /boot/vmlinuz-5.0.0-16-generic
Found initrd image: /boot/initrd.img-5.0.0-16-generic
Found linux image: /boot/vmlinuz-5.0.0-15-generic
Found initrd image: /boot/initrd.img-5.0.0-15-generic
Found linux image: /boot/vmlinuz-4.10.0-32-generic
Found initrd image: /boot/initrd.img-4.10.0-32-generic
done
Errors were encountered while processing:
 linux-headers-4.10.0-32-generic
root@rainbow:/home/nico/ubuntu#

#+END_CENTER
*** 2019-06-13: reminder: no ubuntu 16.04 originally due to broken packages
*** 2019-06-13: re-installing ubuntu 16.04 fails w/ disk detection issues
- trying 2 different computers
- trying 2 different disks
- erased partition table

Only worked after creating a sample partition
*** 2019-06-13: reinstall sdnet: next button doesn't work on ubuntu 16.04
java traceback when trying to install sdnet
#+BEGIN_CENTER
Exception in thread "AWT-EventQueue-0" java.lang.IllegalArgumentException: Window must not be zero
	at java.desktop/sun.awt.X11.XAtom.checkWindow(Unknown Source)
	at java.desktop/sun.awt.X11.XAtom.getAtomData(Unknown Source)
	at java.desktop/sun.awt.X11.XToolkit.getWorkArea(Unknown Source)
	at java.desktop/sun.awt.X11.XToolkit.getInsets(Unknown Source)
	at java.desktop/sun.awt.X11.XToolkit.getScreenInsets(Unknown Source)
	at java.desktop/java.awt.Window.init(Unknown Source)
	at java.desktop/java.awt.Window.<init>(Unknown Source)
	at java.desktop/java.awt.Window.<init>(Unknown Source)
	at java.desktop/java.awt.Dialog.<init>(Unknown Source)
	at java.desktop/java.awt.Dialog.<init>(Unknown Source)
	at java.desktop/javax.swing.JDialog.<init>(Unknown Source)
	at java.desktop/javax.swing.JOptionPane.createDialog(Unknown Source)
	at java.desktop/javax.swing.JOptionPane.createDialog(Unknown Source)
	at j.a.c(Unknown Source)
	at j.a.a(Unknown Source)
	at j.a.a(Unknown Source)
	at j.a.c(Unknown Source)
	at com.xilinx.installer.gui.panel.destination.b.a(Unknown Source)
	at com.xilinx.installer.gui.panel.destination.DestinationPanel.z(Unknown Source)
	at com.xilinx.installer.gui.E.a(Unknown Source)
	at com.xilinx.installer.gui.InstallerGUI.l(Unknown Source)
	at com.xilinx.installer.gui.i.actionPerformed(Unknown Source)
	at java.desktop/javax.swing.AbstractButton.fireActionPerformed(Unknown Source)
	at java.desktop/javax.swing.AbstractButton$Handler.actionPerformed(Unknown Source)
	at java.desktop/javax.swing.DefaultButtonModel.fireActionPerformed(Unknown Source)
	at java.desktop/javax.swing.DefaultButtonModel.setPressed(Unknown Source)
	at java.desktop/javax.swing.plaf.basic.BasicButtonListener.mouseReleased(Unknown Source)
	at java.desktop/java.awt.Component.processMouseEvent(Unknown Source)
	at java.desktop/javax.swing.JComponent.processMouseEvent(Unknown Source)
	at java.desktop/java.awt.Component.processEvent(Unknown Source)
	at java.desktop/java.awt.Container.processEvent(Unknown Source)
	at java.desktop/java.awt.Component.dispatchEventImpl(Unknown Source)
	at java.desktop/java.awt.Container.dispatchEventImpl(Unknown Source)
	at java.desktop/java.awt.Component.dispatchEvent(Unknown Source)
	at java.desktop/java.awt.LightweightDispatcher.retargetMouseEvent(Unknown Source)
	at java.desktop/java.awt.LightweightDispatcher.processMouseEvent(Unknown Source)
	at java.desktop/java.awt.LightweightDispatcher.dispatchEvent(Unknown Source)
	at java.desktop/java.awt.Container.dispatchEventImpl(Unknown Source)
	at java.desktop/java.awt.Window.dispatchEventImpl(Unknown Source)
	at java.desktop/java.awt.Component.dispatchEvent(Unknown Source)
	at java.desktop/java.awt.EventQueue.dispatchEventImpl(Unknown Source)
	at java.desktop/java.awt.EventQueue.access$500(Unknown Source)
	at java.desktop/java.awt.EventQueue$3.run(Unknown Source)
	at java.desktop/java.awt.EventQueue$3.run(Unknown Source)
	at java.base/java.security.AccessController.doPrivileged(Native Method)
	at java.base/java.security.ProtectionDomain$JavaSecurityAccessImpl.doIntersectionPrivilege(Unknown Source)
	at java.base/java.security.ProtectionDomain$JavaSecurityAccessImpl.doIntersectionPrivilege(Unknown Source)
	at java.desktop/java.awt.EventQueue$4.run(Unknown Source)
	at java.desktop/java.awt.EventQueue$4.run(Unknown Source)
	at java.base/java.security.AccessController.doPrivileged(Native Method)
	at java.base/java.security.ProtectionDomain$JavaSecurityAccessImpl.doIntersectionPrivilege(Unknown Source)
	at java.desktop/java.awt.EventQueue.dispatchEvent(Unknown Source)
	at java.desktop/java.awt.EventDispatchThread.pumpOneEventForFilters(Unknown Source)
	at java.desktop/java.awt.EventDispatchThread.pumpEventsForFilter(Unknown Source)
	at java.desktop/java.awt.EventDispatchThread.pumpEventsForHierarchy(Unknown Source)
	at java.desktop/java.awt.EventDispatchThread.pumpEvents(Unknown Source)
	at java.desktop/java.awt.EventDispatchThread.pumpEvents(Unknown Source)
	at java.desktop/java.awt.EventDispatchThread.run(Unknown Source)


#+END_CENTER

Reason was a hidden window.
***
*** 2019-06-13: try using external card for packets
*** 2019-06-14: test adding table entry with ubuntu 16.04, kernel 4.15.0-51-generic
#+BEGIN_CENTER
[12:05] rainbow16:CLI% ./P4_SWITCH_CLI.py
loading libsume..
loading libsume..
loading libcam..
The SimpleSumeSwitch interactive command line tool
 type help to see all commands
>> table_cam_add_entry lookup_table send_to_port1 ff:ff:ff:ff:ff:ff =>
CAM_Init_ValidateContext() - done
WROTE 0x44020050 = 0xffffffff
WROTE 0x44020054 = 0xffff
WROTE 0x44020080 = 0x0003
python: ioctl: Unknown error 512
[12:05] rainbow16:CLI%

#+END_CENTER
*** 2019-06-14: try finding pre compiled bitfiles that can be tested
*** 2019-06-14: re-verify hardware
Using
https://github.com/NetFPGA/NetFPGA-SUME-public/wiki/Acceptance-Test-Project

#+BEGIN_CENTER
[13:33] rainbow16:acceptance_test% make cores

for lib in ./std/cores/nf_sume_10g_interface_shared_logic ./std/cores/nf_axis_gen_chk ./std/cores/nf_sume_10g_interface ./digilent/cores/d_clkfreq_detector ./digilent/cores/nf_sume_gpio_test ./digilent/cores/d_sdctrl ; do\
        make -C ip_repo/$lib clean; \
        make -C ip_repo/$lib; \
done;
make[1]: Entering directory '/home/nico/NetFPGA-SUME-live/projects/acceptance_test/ip_repo/std/cores/nf_sume_10g_interface_shared_logic'
rm -rf generated_ip
for i in nf_sume_10g_pcs_pma_ff_synchronizer_rst2.v nf_sume_10g_pcs_pma_gt_common.v; do \
        rm hdl/$i -fv; \
done;
rm -rf vivado*
rm -rf .Xil
rm -rf nf_sume_10g_interface_shared_logic_project
rm -rf component.xml
rm -rf xgui
make[1]: Leaving directory '/home/nico/NetFPGA-SUME-live/projects/acceptance_test/ip_repo/std/cores/nf_sume_10g_interface_shared_logic'
make[1]: Entering directory '/home/nico/NetFPGA-SUME-live/projects/acceptance_test/ip_repo/std/cores/nf_sume_10g_interface_shared_logic'
WARNING: Ignoring invalid XILINX_PATH location /opt/Xilinx/Vivado/2016.4.
Resolution: An invalid XILINX_PATH location has been detected. To resolve this issue:

1. Verify the value of XILINX_PATH is accurate by viewing the value the variable via 'set XILINX_PATH' for Windows or 'echo $XILINX_PATH' for Linux, and update it as needed.

2. To unset the variable using on Windows using 'set XILINX_PATH=' or remove it from Advanced System Settings\Environment Variables. On Linux 'unsetenv XILINX_PATH'


 ****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

WARNING: [Common 17-1271] The MYVIVADO environment variable specifies an invalid location '/opt/Xilinx/Vivado/2016.4'
source ../tcl/nf_sume_pcs_pma_compile.tcl
# set ip_name {nf_sume_10g_pcs_pma}
# create_project -in_memory -part xc7vx690tffg1761-3
# create_ip -name ten_gig_eth_pcs_pma -vendor xilinx.com -library ip -module_name ${ip_name}
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1704] No user IP repositories specified

#+END_CENTER

#+BEGIN_CENTER
[14:39] rainbow16:acceptance_test% make test
python sw/host/script/NfSumeTest.py
Traceback (most recent call last):
  File "sw/host/script/NfSumeTest.py", line 45, in <module>
    import wx
ImportError: No module named wx
Makefile:55: recipe for target 'test' failed
make: *** [test] Error 1
[14:40] rainbow16:acceptance_test%

...
[14:39] rainbow16:acceptance_test% make test
python sw/host/script/NfSumeTest.py
Traceback (most recent call last):
  File "sw/host/script/NfSumeTest.py", line 45, in <module>
    import wx
ImportError: No module named wx
Makefile:55: recipe for target 'test' failed
make: *** [test] Error 1
[14:40] rainbow16:acceptance_test%

[14:40] rainbow16:acceptance_test% make test
python sw/host/script/NfSumeTest.py
Traceback (most recent call last):
  File "sw/host/script/NfSumeTest.py", line 52, in <module>
    import serial
ImportError: No module named serial
Makefile:55: recipe for target 'test' failed
make: *** [test] Error 1
[14:41] rainbow16:acceptance_test%


root@rainbow16:~# apt install python-serial

#+END_CENTER

Trying to run make test -> various path erros -> trying sudo bash

#+BEGIN_CENTER


root@rainbow16:~/NetFPGA-SUME-live/projects/acceptance_test# . ~nico/master-thesis/netpfga/bashinit
#+END_CENTER

*** 2019-06-15: downloading / uploading reference switch
    - http://www.cl.cam.ac.uk/research/srg/netos/projects/netfpga/bitfiles/NetFPGA-SUME-live/1.3.0/reference_switch/reference_switch.bit
    - https://www.cl.cam.ac.uk/research/srg/netos/projects/netfpga/bitfiles/NetFPGA-SUME-live/1.3.0/

*** 2019-06-15: Testing with external host: seems like my minip4 switch actually works!

#+BEGIN_CENTER
22:18:39.824461 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
22:18:40.848171 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
22:18:40.848292 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
22:18:41.872171 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
22:18:41.872286 IP6 2001:db8::1 > ff02::1:ff00:2: ICMP6, neighbor solicitation, who has 2001:db8::2, length 32
22:18:58.848012 IP6 2001:db8::1.5353 > ff02::fb.5353: 0 [2q] PTR (QM)? _ipps._tcp.local. PTR (QM)? _ipp._tcp.local. (45)
22:18:58.848058 IP6 2001:db8::1.5353 > ff02::fb.5353: 0 [2q] PTR (QM)? _ipps._tcp.local. PTR (QM)? _ipp._tcp.local. (45)
22:20:02.849843 IP6 2001:db8::1.5353 > ff02::fb.5353: 0 [2q] PTR (QM)? _ipps._tcp.local. PTR (QM)? _ipp._tcp.local. (45)
22:20:02.849894 IP6 2001:db8::1.5353 > ff02::fb.5353: 0 [2q] PTR (QM)? _ipps._tcp.local. PTR (QM)? _ipp._tcp.local. (45)
22:22:10.850831 IP6 2001:db8::1.5353 > ff02::fb.5353: 0 [2q] PTR (QM)? _ipps._tcp.local. PTR (QM)? _ipp._tcp.local. (45)
22:22:10.850950 IP6 2001:db8::1.5353 > ff02::fb.5353: 0 [2q] PTR (QM)? _ipps._tcp.local. PTR (QM)? _ipp._tcp.local. (45)

#+END_CENTER

Problem:
- So basically riffa_sume doesn't do the right thing[tm]

Message from myself:

#+BEGIN_CENTER
It seems I was really mistaken for the last weeks
If I am not totally mistaken, the following is happening with the netpfga:
I was testing sending and receiving packets on the same computer; so I sent a packet on nfX and expected an answer on nf0, which is how I wanted to verify that the card works
So I ran tcpdump on nf0, send a packet  with ping6 and scapy on nf{0,1,2,3} (edited)
I have never seen the switch emitting ANY packet back with tcpdump
Now with the card connected to another host, sending neighbor solicitation, I see duplicated packets on the other host - so it seems that it might have worked all the time, just that tcpdump on nfX on the host which contains the card does not show the packets
#+END_CENTER


The testscript now generates 2 packets:

#+BEGIN_CENTER
root@naked:~# cat foo.py
#!/usr/bin/python3

import sys
from scapy.all import *

if __name__ == '__main__':
    iface = sys.argv[1]

    e = Ether(src="02:53:55:42:45:01",
              dst='ff:ff:ff:ff:ff:ff')

    i = IPv6(src = "2001:db8:42::1",
             dst = "2001:db8::2")

    t = TCP(dport=80, sport=random.randint(49152,65535))

    d = "A"

    pkg = e / i / t / d

    sendp(pkg, iface=iface, verbose=True)

root@naked:~#

22:27:34.542877 IP6 2001:db8:42::1.63186 > 2001:db8::2.80: Flags [S], seq 0:1, win 8192, length 1: HTTP
22:27:34.542982 IP6 2001:db8:42::1.63186 > 2001:db8::2.80: Flags [S], seq 0:1, win 8192, length 1: HTTP

#+END_CENTER

*** 2019-06-17: Testing hardware: test tool seems not to work
    - Compiling tests -> ok
    - Select test -> ok
    - Run test -> nothing happens, tests gets unchecked


#+BEGIN_CENTER

---------------------------------------------
[ddr3B]: Running Auto Test
---------------------------------------------
Traceback (most recent call last):
  File "/usr/lib/python2.7/dist-packages/wx-3.0-gtk2/wx/_core.py", line 16765, in <lambda>
    lambda event: event.callable(*event.args, **event.kw) )
  File "sw/host/script/NfSumeTest.py", line 848, in UpdateProgress
    self.progressDlg.Update(self.curProgress, str(localLine))
  File "/usr/lib/python2.7/dist-packages/wx-3.0-gtk2/wx/_core.py", line 16710, in __getattr__
    raise PyDeadObjectError(self.attrStr % self._name)
wx._core.PyDeadObjectError: The C++ part of the NfSumeProgress object has been deleted, attribute access no longer allowed.
Exception in thread Thread-18:
Traceback (most recent call last):
  File "/usr/lib/python2.7/threading.py", line 801, in __bootstrap_inner
    self.run()
  File "sw/host/script/NfSumeTest.py", line 947, in run
    self.target(*self.data)
  File "sw/host/script/NfSumeTest.py", line 355, in StartAutoTest
    self.TestInterface(testName)
  File "sw/host/script/NfSumeTest.py", line 465, in TestInterface
    self.ProgramFpga('../../../bitfiles/' + self.nfSumeTestConfiguration[testName]['bitstream'])
  File "sw/host/script/NfSumeTest.py", line 586, in ProgramFpga
    self.getFpgaIndex()
  File "sw/host/script/NfSumeTest.py", line 574, in getFpgaIndex
    p = Popen(['djtgcfg', 'init', '-d', 'NetSUME'], stdout=PIPE, bufsize = 1)
  File "/usr/lib/python2.7/subprocess.py", line 711, in __init__
    errread, errwrite)
  File "/usr/lib/python2.7/subprocess.py", line 1343, in _execute_child
    raise child_exception
OSError: [Errno 2] No such file or directory

#+END_CENTER

Might come from:

#+BEGIN_CENTER
 zsh: command not found: djtgcfg
[10:32] rainbow16:~% find /opt -name djtgcfg

#+END_CENTER

-> does not exist anywhere

#+BEGIN_CENTER
[10:34] rainbow16:NetFPGA-SUME-live% grep -r djtgcfg .
./projects/acceptance_test/sw/host/script/NfSumeTest.py:        p = Popen(['djtgcfg', 'init', '-d', 'NetSUME'], stdout=PIPE, bufsize = 1)
./projects/acceptance_test/sw/host/script/NfSumeTest.py:        #p = Popen(['djtgcfg', 'prog', '-d', 'NetSUME', '-i', self.fpgaIndex, '-f',
./tools/scripts/load_bitfile.py:    p = Popen(['djtgcfg', 'init', '-d', 'NetSUME'], stdout=PIPE, bufsize = 1)

#+END_CENTER

Likely requires "Installation of Digilent Adept Tools"

 https://reference.digilentinc.com/reference/software/adept/start

(website does not load as of 2019-06-17, 10:39)!

Install deb that supports the hardware test:

#+BEGIN_CENTER
10-ipv6-privacy.conf  Desktop  digilent.adept.runtime_2.19.2-amd64.deb
root@rainbow16:~# dpkg -i digilent.adept.runtime_2.19.2-amd64.deb
Selecting previously unselected package digilent.adept.runtime.
(Reading database ... 275077 files and directories currently installed.)
Preparing to unpack digilent.adept.runtime_2.19.2-amd64.deb ...
Unpacking digilent.adept.runtime (2.19.2) ...
Setting up digilent.adept.runtime (2.19.2) ...
Processing triggers for libc-bin (2.23-0ubuntu11) ...
root@rainbow16:~#

#+END_CENTER

The required tool does not seem to be included in the adept runtime:

#+BEGIN_CENTER
root@rainbow16:~# dpkg -l | grep digilent
ii  digilent.adept.runtime                     2.19.2                                       amd64        Digilent Adept Runtime
root@rainbow16:~# dpkg -L digilent.adept.runtime  | grep djtgcfg
root@rainbow16:~#

#+END_CENTER

Trying -tools as well

#+BEGIN_CENTER
[12:55] line:Downloads% scp digilent.adept.utilities_2.2.1-amd64.deb root@rainbow16.place6.ungleich.ch:
digilent.adept.utilities_2.2.1-amd64.deb                                                     100%  465KB   1.2MB/s   00:00
[12:56] line:Downloads%

root@rainbow16:~# ls
10-ipv6-privacy.conf  Desktop  digilent.adept.runtime_2.19.2-amd64.deb  digilent.adept.utilities_2.2.1-amd64.deb
root@rainbow16:~# dpkg -i digilent.adept.utilities_2.2.1-amd64.deb
Selecting previously unselected package digilent.adept.utilities.
(Reading database ... 275201 files and directories currently installed.)
Preparing to unpack digilent.adept.utilities_2.2.1-amd64.deb ...
Unpacking digilent.adept.utilities (2.2.1) ...
Setting up digilent.adept.utilities (2.2.1) ...
Processing triggers for man-db (2.7.5-1) ...
root@rainbow16:~# which  djtgcfg
/usr/bin/djtgcfg
root@rainbow16:~#

#+END_CENTER

New error from the hardware test:

#+BEGIN_CENTER

---------------------------------------------
[pcie]: Running Auto Test
---------------------------------------------
Traceback (most recent call last):
  File "/usr/lib/python2.7/dist-packages/wx-3.0-gtk2/wx/_core.py", line 16765, in <lambda>
    lambda event: event.callable(*event.args, **event.kw) )
  File "sw/host/script/NfSumeTest.py", line 848, in UpdateProgress
    self.progressDlg.Update(self.curProgress, str(localLine))
  File "/usr/lib/python2.7/dist-packages/wx-3.0-gtk2/wx/_core.py", line 16710, in __getattr__
    raise PyDeadObjectError(self.attrStr % self._name)
wx._core.PyDeadObjectError: The C++ part of the NfSumeProgress object has been deleted, attribute access no longer allowed.
Exception in thread Thread-21:
Traceback (most recent call last):
  File "/usr/lib/python2.7/threading.py", line 801, in __bootstrap_inner
    self.run()
  File "sw/host/script/NfSumeTest.py", line 947, in run
    self.target(*self.data)
  File "sw/host/script/NfSumeTest.py", line 466, in TestInterface
    self.serialCon.readlines()
  File "/usr/lib/python2.7/dist-packages/serial/serialposix.py", line 495, in read
    raise SerialException('device reports readiness to read but returned no data (device disconnected or multiple access on port?)')
SerialException: device reports readiness to read but returned no data (device disconnected or multiple access on port?)



#+END_CENTER

*** 2019-06-17: checksum delta / diff approach
**** crc / checksum operation
"The checksum field is the 16 bit one's complement of the one's
complement sum of all 16-bit words in the header and text."
https://en.wikipedia.org/wiki/Transmission_Control_Protocol#Checksum_computation
*** 2019-06-21: create table entries on new card
#+BEGIN_CENTER
>> table_cam_add_entry lookup_table send_to_port1 ff:ff:ff:ff:ff:ff =>
CAM_Init_ValidateContext() - done
WROTE 0x44020050 = 0xffffffff
WROTE 0x44020054 = 0xffff
WROTE 0x44020080 = 0x0003
READ  0x44020044 = 0x0001
WROTE 0x44020040 = 0x0001
READ  0x44020044 = 0x0001
READ  0x44020044 = 0x0001
success
>>

#+END_CENTER
*** 2019-06-24: meeting laurent
*** 2019-06-24: begin porting original code to netpfga: packet mismatch - why??
#+BEGIN_CENTER
+ actual_line=actual   (tlast, tkeep, tdata) = (0, ffffffff, 000000000000000080fe403b0a0000000060dd86012222222208022222222208)
+ [ expected (tlast, tkeep, tdata) = (0, ffffffff, 000000000000000080fe403b0a0000000060dd86022222222208012222222208) != actual   (tlast, tkeep, tdata) = (0, ffffffff, 000000000000000080fe403b0a0000000060dd86012222222208022222222208) ]
+ echo packet mismatch
packet mismatch

#+END_CENTER

v2:

#+BEGIN_CENTER
+ sed -e s/.*= <// -e s/.*= (//
+ actual_line=0, ffffffff, 000000000000000080fe403b0a0000000060dd86012222222208022222222208)
+ [ 0, ffffffff, 000000000000000080fe403b0a0000000060dd86022222222208012222222208) != 0, ffffffff, 000000000000000080fe403b0a0000000060dd86012222222208022222222208) ]
+ echo packet mismatch
packet mismatch
+ exit 1

expected (tlast, tkeep, tdata) = (0, ffffffff, 000000000000000080fe403b0a0000000060dd86022222222208012222222208)
actual   (tlast, tkeep, tdata) = (0, ffffffff, 000000000000000080fe403b0a0000000060dd86012222222208022222222208)

(0, ffffffff, 000000000000000080fe403b0a0000000060dd86022222222208012222222208)
(0, ffffffff, 000000000000000080fe403b0a0000000060dd86012222222208022222222208)

#+END_CENTER
*** 2019-06-24: find out how the expected/actual packet lines are generated
    - afair: indirectly by running gen_testdata.py -> replace script
      with port1
*** 2019-07-01: verify checksumming
#+BEGIN_CENTER
if struct.pack("H",1) == b"\x00\x01": # big endian
    def checksum(pkt):
        if len(pkt) % 2 == 1:
            pkt += b"\0"
        s = sum(array.array("H", pkt))
        s = (s >> 16) + (s & 0xffff)
        s += s >> 16
        s = ~s
        return s & 0xffff
else:
    def checksum(pkt):
        if len(pkt) % 2 == 1:
            pkt += b"\0"
        s = sum(array.array("H", pkt))
        s = (s >> 16) + (s & 0xffff)
        s += s >> 16
        s = ~s
        return (((s>>8)&0xff)|s<<8) & 0xffff

#+END_CENTER
*** 2019-07-01: 128 bit ipv6 struct -> no conversion!
    - https://docs.python.org/2.7/library/struct.html
    - .packed of ipaddress works
*** 2019-07-01: finish sum, use scapy checksum
*** 2019-07-01: meeting Laurent
*** 2019-07-06: test bmv2 / delta
    Story:
    - Static mapping / no controller
    - IPv4 packet goes in
    - Translated to IPv6
    - IPv6 packet goes in
    - Translated to IPv4
    - Checksums match, but we only update it using
      HashAlgorithm.csum16

*** 2019-07-10:
    To be finished today:
    - delta on bmv2
    - general compile on netpfga

** References / Follow up
*** RFC 791 IPv4 https://tools.ietf.org/html/rfc791
*** RFC 792 ICMP https://tools.ietf.org/html/rfc792
*** RFC 826 ARP  https://tools.ietf.org/html/rfc826
*** RFC 1017 ICMP checksum https://tools.ietf.org/html/rfc1071
    - Related to RFC 6052, Host identifier
*** RFC 2373 IP Version 6 Addressing Architecture
    - Referenced by RFC2464
    - Obsoleted by RFC3513


*** RFC 2460 IPv6 (Checksum https://tools.ietf.org/html/rfc2460#section-8.1)
*** RFC 2464  Transmission of IPv6 Packets over Ethernet Networks https://tools.ietf.org/html/rfc2464
    - embedding of Mac addresses
*** RFC 3810 MLD2 https://tools.ietf.org/html/rfc3810
*** RFC 4038 Application Aspects of IPv6 Transition https://tools.ietf.org/html/rfc4038
    - Ref by RFC4291 / mapped ipv4
    -
*** RFC 4291 IP Version 6 Addressing Architecture https://tools.ietf.org/html/rfc4291
    -!

*** RFC 4443 ICMPv6 https://tools.ietf.org/html/rfc4443
*** RFC 4861: https://tools.ietf.org/html/rfc4861 Neighbor discovery
*** RFC 6052: https://tools.ietf.org/html/rfc6052  IPv6 Addressing of IPv4/IPv6 Translators - first NAT64??
*** RFC 6145 IP/ICMP Translation Algorithm
    - Obsoleted by 7915
*** RFC 6146 Stateful nat http://tools.ietf.org/html/rfc6146
    - Referenced from Jool
*** RFC 6147 DNS64 https://tools.ietf.org/html/rfc6147
*** RFC 6586 for deployment experiences using Stateful NAT64.
*** RFC 7757 Explicit Address Mappings for Stateless IP/ICMP Translation - https://tools.ietf.org/html/rfc7757
*** RFC 7915 IP/ICMP Translation Algorithm https://tools.ietf.org/html/rfc7915
    - Requires RFC 6144
    - MUST support one or more address mapping    algorithms, which
      are defined in Section 6.
    - does not  translate IPv6 extension headers except the Fragment Header.


*** EAMT/Jool: https://www.jool.mx/en/eamt.html
*** Solicited node multicast address https://en.wikipedia.org/wiki/Solicited-node_multicast_address
*** Scapy / IPv6: https://www.idsv6.de/Downloads/IPv6PacketCreationWithScapy.pdf
*** V1 model: https://github.com/p4lang/p4c/blob/master/p4include/v1model.p4
*** Cisco NAT64 https://www.cisco.com/c/en/us/td/docs/ios-xml/ios/ipaddr_nat/configuration/xe-3s/nat-xe-3s-book/iadnat-stateful-nat64.pdf
*** Wiki_mac: https://en.wikipedia.org/wiki/MAC_address
* DONE Initial administration
** DONE Clarify PDF / form with Denise Spicher: free form description
** DONE Create task description to be handed in mystudies
** DONE Create list of tasks / initial brainstorming
** DONE Get OK from Ueli Maurer that thesis is valid in Information Security Area
** DONE Find out how-when-whom-where to meet / define schedule
** DONE Latex and/or org-mode for the thesis? org for starting
** DONE Add initial milestones
*** 180d plan
*** 25w
** DONE Proposal / task description
*** Task description for mystudies
**** High speed NAT64 with P4
 Currently there are two main open source NAT64 solution available:
 tayga and jool. The former is a single threaded, cpu bound user
 space solution, the latter a custom Linux kernel module.

 This thesis challenges this status quo by developing a P4 based
 solution supporting all features of jool/tayga and comparing the
 performance, security and adaptivity of the solutions.

 - Milestone 1: Stateless NAT64/NAT46 translations in P4
 - Milestone 2: Stateful (dynamic) NAT64/NAT46 translations
 - Milestone 3: Hardware adaption
*** Original ideas
 Proposal 1: Automating NAT64 with P4

 In IPv6 only data centers IPv4 connectivity is still a business
 requirement. Current state of the art methods include layer 7 proxying
 or static assignments. both featuring static assignments.

 A flexible, dynamic assignment of IPv4 addresses to IPv6 hosts, similar
 to lease times in DHCPv4 and prefix delegations in DHCPv6 could reduce
 the pressure on IPv4 addresses.

 I would suggest the develop of a new protocol (likely UDP embedded) that
 allows hosts to request on-network support for IPv4 addresses. As IPv4
 addresses have to be treated as "expensive", an accounting metric has to
 be introduced. While in the business world this is usually related to
 money, in the network world IPv4 users could be paying the network by
 (reduced) bandwidth.

 If such a metric existed, devices attached to the network could also try
 to negotiate and wait for using IPv4, when the price / penality for IPv4
 is low (this might be very suitable for mail exchangers for instance).


 Proposal 2: High speed NAT64 with P4

 Currently there are two main open source NAT64 solution available:
 tayga[0] and jool[1]. The former is a single threaded, cpu bound user
 space solution, the latter a custom Linux kernel module.

 I would like to challenge this status quo and develop a P4 based
 solution supporting all features of jool/tayga and comparing the
 performance and adaptivity of the solutions.

 [0] http://www.litech.org/tayga/
 [1] https://www.jool.mx/en/index.html


 Proposal 3: Challenging the status quo with IPv10

 The de facto standard in networking is to treat IPv4
 and IPv6 as "impossible to combine". This proposal is
 to challenge this notion with three different methods:

 - Extensions to IPv4 to request remote IPv6 transport
 - Extensions to IPv6 to request remote IPv4 transport
 - Support in network equipment to handle the extensions

 As the IPv4 header does not allow embedding IPv6 addresses due to size
 limitations, embedding the destination address in a secondary header
 might be necessary (possibly encapsulated in UDP).
