+ echo First source all variables and THEN run this script
First source all variables and THEN run this script
+ read something
+ cd /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4
+ make
make -C src/ clean
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/src'
rm -f *.sdnet *.tbl .sdnet_switch_info.dat
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/src'
make -C testdata/ clean
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata'
rm -f *.pcap *.txt *.pyc *.axi config_writes.* *_reg_defines.py
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata'
rm -rf nf_sume_sdnet_ip/
rm -f ./simple_sume_switch/hw/vivado.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/9278bfe6c99dbe18.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/cc4a2809a8a54e43.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/9783353c4ff76f6c.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/bbbd46440b5c7213.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/3b530f2d27ae946b.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/bcb85672e1d51456.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/7bfef02244461664.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/74db4bf3f7578076.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/f84a275938957408.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.cache/ip/2018.2/bb89f09b44165778.logs/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_axi_intc_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_axi_intc_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_uartlite_0_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_uartlite_0_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_iic_0_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_iic_0_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_mdm_1_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_mdm_1_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_rst_clk_wiz_1_100M_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_rst_clk_wiz_1_100M_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_dlmb_v10_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_dlmb_v10_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m07_data_fifo_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m07_data_fifo_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_dlmb_bram_if_cntlr_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_dlmb_bram_if_cntlr_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_clk_wiz_1_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_clk_wiz_1_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_xlconcat_0_synth_1/runme.log ./simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_xlconcat_0_synth_1/vivado.jou ./simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/identifier_ip/summary.log ./simple_sume_switch/hw/ip_repo/contrib/cores/input_arbiter_drr_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/contrib/cores/input_arbiter_drr_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/sss_fallthrough_small_fifo_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/contrib/cores/sss_fallthrough_small_fifo_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/sss_output_queues_v2_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/contrib/cores/sss_output_queues_v2_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_endianess_manager_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_endianess_manager_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/vivado.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk_13175.backup.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xelab.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/xsimkernel.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/xsimcrash.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk_13175.backup.jou ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xsc.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/SimpleSumeSwitch/xvlog.log ./simple_sume_switch/hw/ip_repo/contrib/cores/nf_sume_sdnet_ip/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/fallthrough_small_fifo_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/fallthrough_small_fifo_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/axi_sim_transactor_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/axi_sim_transactor_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/barrier_gluelogic_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/barrier_gluelogic_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/identifier_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/identifier_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/barrier_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/barrier_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/output_queues_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/output_queues_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/nf_10ge_interface_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/nf_10ge_interface_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/nf_10ge_attachment_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/nf_10ge_attachment_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/axis_sim_stim_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/axis_sim_stim_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/nf_10ge_interface_shared_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/nf_10ge_interface_shared_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/axis_fifo_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/axis_fifo_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/input_arbiter_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/input_arbiter_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/nf_riffa_dma_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/nf_riffa_dma_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/nf_axis_converter_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/nf_axis_converter_v1_0_0/vivado.jou ./simple_sume_switch/hw/ip_repo/std/cores/axis_sim_record_v1_0_0/vivado.log ./simple_sume_switch/hw/ip_repo/std/cores/axis_sim_record_v1_0_0/vivado.jou ./simple_sume_switch/hw/vivado.jou ./nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk.jou ./nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.jou ./nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk_13175.backup.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/xelab.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/xsimkernel.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/xsimcrash.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/webtalk_13175.backup.jou ./nf_sume_sdnet_ip/SimpleSumeSwitch/xsc.log ./nf_sume_sdnet_ip/SimpleSumeSwitch/xvlog.log
rm -f sw/config_tables.c
make -C src/
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/src'
p4c-sdnet -o minip4.sdnet --sdnet_info .sdnet_switch_info.dat minip4_solution.p4
minip4_solution.p4(51): [--Wwarn=uninitialized_out_param] warning: out parameter meta may be uninitialized when TopParser terminates
                 out metadata meta,
                              ^^^^
minip4_solution.p4(49)
parser TopParser(packet_in packet,
       ^^^^^^^^^
minip4_solution.p4(52): [--Wwarn=uninitialized_out_param] warning: out parameter digest_data may be uninitialized when TopParser terminates
                 out digest_data_t digest_data,
                                   ^^^^^^^^^^^
minip4_solution.p4(49)
parser TopParser(packet_in packet,
       ^^^^^^^^^
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/p4_px_tables.py commands.txt .sdnet_switch_info.dat
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/src'
make -C testdata/
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata'
./gen_testdata.py
nf0_applied times:  [4]
nf1_applied times:  [4]
nf2_applied times:  [4]
nf3_applied times:  [4]
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/pcap2axi --output Packet_in.axi --bus_width 256 src.pcap
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/pcap2axi --output Packet_expect.axi --bus_width 256 dst.pcap
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata'
sdnet ./src/minip4.sdnet -skipEval -busType axi -busWidth 256 -singlecontrolport -workDir nf_sume_sdnet_ip -altVivadoScripts
Xilinx SDNet Compiler version 2018.2, build 2342300

Compilation successful
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/gen_P4_SWITCH_externs.py src/.sdnet_switch_info.dat nf_sume_sdnet_ip/SimpleSumeSwitch/ /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/templates/ ./testdata/ ./sw/ --base_address 0x44020000
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/gen_P4_SWITCH_API.py src/.sdnet_switch_info.dat nf_sume_sdnet_ip/SimpleSumeSwitch/ sw/ /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/templates/ --base_address 0x44020000
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/gen_P4_SWITCH_CLI.py src/.sdnet_switch_info.dat nf_sume_sdnet_ip/SimpleSumeSwitch/ sw/ /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/templates/ --base_address 0x44020000
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/sw/CLI'
cc -c -fPIC /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/sw/API/CAM.c -I/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/sw/API
cc -std=c99 -Wall -Werror -fPIC -c libcam.c -I/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/sw/sume -I/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/sw/API 
cc -L/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/sw/sume -shared -o libcam.so libcam.o CAM.o -lsumereg 
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/sw/CLI'
# The following command only applies if running P4_SWITCH Questa Simulation with Ubuntu
sed -i 's/vsim/vsim \-ldflags \"\-B\/usr\/lib\/x86\_64\-linux-gnu\"/g' nf_sume_sdnet_ip/SimpleSumeSwitch/questa.bash
# modify the P4_SWITCH_tb so that it writes the table configuration writes to a file
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/modify_P4_SWITCH_tb.py nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/SimpleSumeSwitch_tb.sv
# Fix introduced for SDNet 2017.4
sed -i 's/xsim\.dir\/xsc\/dpi\.so/dpi\.so/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim.bash
sed -i 's/xsim\.dir\/xsc\/dpi\.so/dpi\.so/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
# Fix introduced for SDNet 2018.2
sed -i 's/glbl_sim/glbl/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
sed -i 's/SimpleSumeSwitch_tb_sim#work.glbl/SimpleSumeSwitch_tb/g' nf_sume_sdnet_ip/SimpleSumeSwitch/vivado_sim_waveform.bash
cp src/*.tbl nf_sume_sdnet_ip/SimpleSumeSwitch/
cp testdata/*.txt nf_sume_sdnet_ip/SimpleSumeSwitch/
cp testdata/*.axi nf_sume_sdnet_ip/SimpleSumeSwitch/
+ cd /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch
+ ./vivado_sim.bash
+ tee LOG
+ find -name '*.v' -o -name '*.vp' -o -name '*.sv'
+ xargs -I % /opt/Xilinx/Vivado/2018.2/bin/xvlog -sv %
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_0_t.HDL/TopPipe_lvl_0_t.v" into library work
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_0_t.HDL/TopPipe_lvl_0_t.vp" into library work
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_Engine
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_dummy_table_for_netpfga_sec
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_dummy_table_for_netpfga_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_dummy_table_for_netpfga_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_EngineStage_1
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_do_nothing_0_sec
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_do_nothing_0_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_do_nothing_0_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec_compute_sume_metadata_dst_port
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_EngineStage_2
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_sink
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_sink_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_sink_compute_control_increment_offset
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v" into library work
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for__OUT_.v" into library work
INFO: [VRFC 10-311] analyzing module S_SYNCER_for__OUT_
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v" into library work
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_S_SYNCER_for_TopDeparser
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/xpm_fifo.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_fifo_base
INFO: [VRFC 10-311] analyzing module xpm_fifo_rst
INFO: [VRFC 10-311] analyzing module xpm_counter_updn
INFO: [VRFC 10-311] analyzing module xpm_fifo_reg_vec
INFO: [VRFC 10-311] analyzing module xpm_fifo_reg_bit
INFO: [VRFC 10-311] analyzing module xpm_reg_pipe_bit
INFO: [VRFC 10-311] analyzing module xpm_fifo_sync
INFO: [VRFC 10-311] analyzing module xpm_fifo_async
INFO: [VRFC 10-311] analyzing module xpm_fifo_axis
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/xpm_memory.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_memory_base
INFO: [VRFC 10-311] analyzing module asym_bwe_bb
INFO: [VRFC 10-311] analyzing module xpm_memory_dpdistram
INFO: [VRFC 10-311] analyzing module xpm_memory_dprom
INFO: [VRFC 10-311] analyzing module xpm_memory_sdpram
INFO: [VRFC 10-311] analyzing module xpm_memory_spram
INFO: [VRFC 10-311] analyzing module xpm_memory_sprom
INFO: [VRFC 10-311] analyzing module xpm_memory_tdpram
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/xpm_cdc.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_cdc_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_gray
INFO: [VRFC 10-311] analyzing module xpm_cdc_handshake
INFO: [VRFC 10-311] analyzing module xpm_cdc_pulse
INFO: [VRFC 10-311] analyzing module xpm_cdc_array_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_sync_rst
INFO: [VRFC 10-311] analyzing module xpm_cdc_async_rst
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/glbl.v" into library work
INFO: [VRFC 10-311] analyzing module glbl
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopDeparser.v" into library work
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_TopDeparser
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v" into library work
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_TopParser
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.vp" into library work
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_fifo.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_fifo_base
INFO: [VRFC 10-311] analyzing module xpm_fifo_rst
INFO: [VRFC 10-311] analyzing module xpm_counter_updn
INFO: [VRFC 10-311] analyzing module xpm_fifo_reg_vec
INFO: [VRFC 10-311] analyzing module xpm_fifo_reg_bit
INFO: [VRFC 10-311] analyzing module xpm_reg_pipe_bit
INFO: [VRFC 10-311] analyzing module xpm_fifo_sync
INFO: [VRFC 10-311] analyzing module xpm_fifo_async
INFO: [VRFC 10-311] analyzing module xpm_fifo_axis
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_memory.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_memory_base
INFO: [VRFC 10-311] analyzing module asym_bwe_bb
INFO: [VRFC 10-311] analyzing module xpm_memory_dpdistram
INFO: [VRFC 10-311] analyzing module xpm_memory_dprom
INFO: [VRFC 10-311] analyzing module xpm_memory_sdpram
INFO: [VRFC 10-311] analyzing module xpm_memory_spram
INFO: [VRFC 10-311] analyzing module xpm_memory_sprom
INFO: [VRFC 10-311] analyzing module xpm_memory_tdpram
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_cdc.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_cdc_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_gray
INFO: [VRFC 10-311] analyzing module xpm_cdc_handshake
INFO: [VRFC 10-311] analyzing module xpm_cdc_pulse
INFO: [VRFC 10-311] analyzing module xpm_cdc_array_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_sync_rst
INFO: [VRFC 10-311] analyzing module xpm_cdc_async_rst
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/glbl.v" into library work
INFO: [VRFC 10-311] analyzing module glbl
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.v" into library work
INFO: [VRFC 10-311] analyzing module S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_t.HDL/TopPipe_lvl_t.vp" into library work
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_Engine
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup_compute_dummy_table_for_netpfga_req_lookup_request_key
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup_compute_control_increment_offset
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_t.HDL/TopPipe_lvl_t.v" into library work
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_CONTROLLERs.HDL/S_CONTROLLER_SimpleSumeSwitch.vp" into library work
ERROR: [VRFC 10-1491] unexpected EOF [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_CONTROLLERs.HDL/S_CONTROLLER_SimpleSumeSwitch.vp:37]
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_CONTROLLERs.HDL/S_CONTROLLER_SimpleSumeSwitch.v" into library work
INFO: [VRFC 10-311] analyzing module S_CONTROLLER_SimpleSumeSwitch
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/TB_System_Stim.v" into library work
INFO: [VRFC 10-311] analyzing module TB_System_Stim
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v" into library work
INFO: [VRFC 10-311] analyzing module Check
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/SimpleSumeSwitch_tb.sv" into library work
INFO: [VRFC 10-311] analyzing module SimpleSumeSwitch_tb
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopDeparser_t.HDL/TopDeparser_t.vp" into library work
INFO: [VRFC 10-311] analyzing module TopDeparser_t_Engine
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec_compute_control_remove
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_1
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_1_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_act_sec
INFO: [VRFC 10-311] analyzing module TopDeparser_t_act_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_act_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute__STRUCT_dst_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute__STRUCT_src_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute__STRUCT_ethertype
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_task
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_ingress_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_ethertype
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_table_id
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_version
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_ihl
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_diff_serv
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_ecn
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_totalLen
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_identification
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_flags
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_fragOffset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_ttl
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_protocol
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_hdrChecksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_src_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_dst_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_version
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_traffic_class
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_flow_label
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_payload_length
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_next_header
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_hop_limit
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_src_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_dst_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_hw_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_protocol
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_hw_size
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_protocol_size
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_opcode
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_src_mac_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_src_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_dst_mac_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_dst_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_src_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_dst_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_seqNo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_ackNo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_data_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_res
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_cwr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_ece
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_urg
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_ack
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_psh
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_rst
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_syn
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_fin
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_window
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_urgentPtr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_src_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_dst_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_payload_length
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute__STRUCT_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute__STRUCT_code
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute__STRUCT_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute__STRUCT_code
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_router
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_solicitated
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_override
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_reserved
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_target_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute__STRUCT_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute__STRUCT_ll_length
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute__STRUCT_mac_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataMux
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopDeparser_t.HDL/TopDeparser_t.v" into library work
INFO: [VRFC 10-311] analyzing module TopDeparser_t
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_line.v" into library work
INFO: [VRFC 10-311] analyzing module S_RESETTER_line
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_lookup.v" into library work
INFO: [VRFC 10-311] analyzing module S_RESETTER_lookup
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_control.v" into library work
INFO: [VRFC 10-311] analyzing module S_RESETTER_control
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopParser_t.HDL/TopParser_t.vp" into library work
INFO: [VRFC 10-311] analyzing module TopParser_t_Engine
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_start
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_icmp
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_icmp6
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_icmp6_na_ns
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_ipv4
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_udp_v6
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_udp_v4
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_tcp_v6
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_tcp_v4
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_v4sum
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_v6sum
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_headerdiff
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_dst_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_src_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_ethertype
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_reject
INFO: [VRFC 10-311] analyzing module TopParser_t_reject_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_reject_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_version
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_ihl
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_diff_serv
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_ecn
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_totalLen
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_identification
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_flags
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_fragOffset
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_ttl
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_protocol
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_hdrChecksum
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_src_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_dst_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_meta_length_without_ip_header
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_version
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_traffic_class
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_flow_label
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_payload_length
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_next_header
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_hop_limit
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_src_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_dst_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_meta_length_without_ip_header
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_arp
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_hw_type
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_protocol
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_hw_size
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_protocol_size
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_opcode
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_src_mac_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_src_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_dst_mac_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_dst_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_type
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_code
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_src_port
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_dst_port
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_seqNo
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_ackNo
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_data_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_res
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_cwr
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_ece
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_urg
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_ack
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_psh
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_rst
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_syn
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_fin
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_window
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_urgentPtr
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_udp
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_src_port
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_dst_port
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_payload_length
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_type
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_code
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_router
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_solicitated
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_override
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_reserved
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_target_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_type
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_ll_length
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_mac_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_4
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_4_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_accept
INFO: [VRFC 10-311] analyzing module TopParser_t_accept_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_accept_compute_control_increment_offset
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/TopParser_t.HDL/TopParser_t.v" into library work
INFO: [VRFC 10-311] analyzing module TopParser_t
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v" into library work
INFO: [VRFC 10-311] analyzing module S_PROTOCOL_ADAPTER_EGRESS
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.vp" into library work
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.vp" into library work
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v" into library work
INFO: [VRFC 10-311] analyzing module S_PROTOCOL_ADAPTER_INGRESS
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/dummy_table_for_netpfga_t.vp" into library work
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Wrap
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_IntTop
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Lookup
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Hash_Lookup
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_RamR1RW1
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Cam
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Update
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Hash_Update
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod4
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod4_Rnd
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod5
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod5_Rnd
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_csr
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_memory_base
INFO: [VRFC 10-311] analyzing module asym_bwe_bb
INFO: [VRFC 10-311] analyzing module xpm_memory_dpdistram
INFO: [VRFC 10-311] analyzing module xpm_memory_dprom
INFO: [VRFC 10-311] analyzing module xpm_memory_sdpram
INFO: [VRFC 10-311] analyzing module xpm_memory_spram
INFO: [VRFC 10-311] analyzing module xpm_memory_sprom
INFO: [VRFC 10-311] analyzing module xpm_memory_tdpram
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_cdc.sv" into library work
INFO: [VRFC 10-311] analyzing module xpm_cdc_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_gray
INFO: [VRFC 10-311] analyzing module xpm_cdc_handshake
INFO: [VRFC 10-311] analyzing module xpm_cdc_pulse
INFO: [VRFC 10-311] analyzing module xpm_cdc_array_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_sync_rst
INFO: [VRFC 10-311] analyzing module xpm_cdc_async_rst
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/dummy_table_for_netpfga_t.v" into library work
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v" into library work
INFO: [VRFC 10-311] analyzing module SimpleSumeSwitch
+ true
+ mkdir -p xsim.dir/xsc
+ find -name '*.c'
+ xargs /opt/Xilinx/Vivado/2018.2/bin/xsc -mt off -v 1
Turned off multi-threading.
Running compilation flow
/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/gcc  -fPIC -c -Wa,-W -fPIC -m64 -B/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/../../binutils-2.26/bin/    -I"/opt/Xilinx/Vivado/2018.2/data/xsim/include" -I"/opt/Xilinx/Vivado/2018.2/data/xsim/systemc" "./Testbench/CAM.c" -O1 -o "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work/xsc/CAM.lnx64.o" -DXILINX_SIMULATOR
/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/gcc  -fPIC -c -Wa,-W -fPIC -m64 -B/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/../../binutils-2.26/bin/    -I"/opt/Xilinx/Vivado/2018.2/data/xsim/include" -I"/opt/Xilinx/Vivado/2018.2/data/xsim/systemc" "./Testbench/user.c" -O1 -o "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work/xsc/user.lnx64.o" -DXILINX_SIMULATOR
./Testbench/user.c: In function ‘register_write_control’:
./Testbench/user.c:37:5: warning: implicit declaration of function ‘SV_write_control’ [-Wimplicit-function-declaration]
     SV_write_control(&sv_addr, &sv_data);
     ^~~~~~~~~~~~~~~~
./Testbench/user.c: In function ‘register_read_control’:
./Testbench/user.c:51:5: warning: implicit declaration of function ‘SV_read_control’ [-Wimplicit-function-declaration]
     SV_read_control(&sv_addr, &sv_data);
     ^~~~~~~~~~~~~~~
./Testbench/user.c: In function ‘CAM_Init’:
./Testbench/user.c:88:76: warning: passing argument 9 of ‘CAM_Init_ValidateContext’ from incompatible pointer type [-Wincompatible-pointer-types]
     if(CAM_Init_ValidateContext(cx,baseAddr,256,depth,k,clk_period,v,aging,register_write, register_read, &log_msg, log_level))
                                                                            ^~~~~~~~~~~~~~
In file included from ./Testbench/user.c:7:0:
./Testbench/CAM.h:169:5: note: expected ‘void (*)(addr_t,  uint32_t) {aka void (*)(long long unsigned int,  unsigned int)}’ but argument is of type ‘void (*)(uint32_t,  uint32_t) {aka void (*)(unsigned int,  unsigned int)}’
 int CAM_Init_ValidateContext(
     ^~~~~~~~~~~~~~~~~~~~~~~~
./Testbench/user.c:88:92: warning: passing argument 10 of ‘CAM_Init_ValidateContext’ from incompatible pointer type [-Wincompatible-pointer-types]
     if(CAM_Init_ValidateContext(cx,baseAddr,256,depth,k,clk_period,v,aging,register_write, register_read, &log_msg, log_level))
                                                                                            ^~~~~~~~~~~~~
In file included from ./Testbench/user.c:7:0:
./Testbench/CAM.h:169:5: note: expected ‘uint32_t (*)(addr_t) {aka unsigned int (*)(long long unsigned int)}’ but argument is of type ‘uint32_t (*)(uint32_t) {aka unsigned int (*)(unsigned int)}’
 int CAM_Init_ValidateContext(
     ^~~~~~~~~~~~~~~~~~~~~~~~
Done compilation
Linking with command:
/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/g++ -Wa,-W  -O -fPIC  -m64  -shared  -o "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dpi.so" "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work/xsc/CAM.lnx64.o" "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work/xsc/user.lnx64.o"     -L/opt/Xilinx/Vivado/2018.2/lib/lnx64.o -lrdi_simulator_kernel  -lrdi_xsim_systemc  -B/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/../../binutils-2.26/bin/ 

Running command : /opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/g++ -Wa,-W  -O -fPIC  -m64  -shared  -o "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dpi.so" "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work/xsc/CAM.lnx64.o" "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work/xsc/user.lnx64.o"     -L/opt/Xilinx/Vivado/2018.2/lib/lnx64.o -lrdi_simulator_kernel  -lrdi_xsim_systemc  -B/opt/Xilinx/Vivado/2018.2/lib/lnx64.o/../../tps/lnx64/gcc-6.2.0/bin/../../binutils-2.26/bin/ 
Done linking: "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dpi.so"
+ /opt/Xilinx/Vivado/2018.2/bin/xelab -L work --debug all -sv_lib dpi.so SimpleSumeSwitch_tb glbl
Vivado Simulator 2018.2
Copyright 1986-1999, 2001-2018 Xilinx, Inc. All Rights Reserved.
Running: /opt/Xilinx/Vivado/2018.2/bin/unwrapped/lnx64.o/xelab -L work --debug all -sv_lib dpi.so SimpleSumeSwitch_tb glbl 
Multi-threading is on. Using 6 slave threads.
Starting static elaboration
Completed static elaboration
Starting simulation data flow analysis
Completed simulation data flow analysis
Time Resolution for simulation is 1ps
Compiling module work.S_RESETTER_line
Compiling module work.S_RESETTER_lookup
Compiling module work.S_RESETTER_control
Compiling module work.TopParser_t_EngineStage_0_ErrorC...
Compiling module work.TopParser_t_EngineStage_0_Extrac...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_c...
Compiling module work.TopParser_t_start_compute_meta_v...
Compiling module work.TopParser_t_start_compute_meta_v...
Compiling module work.TopParser_t_start_compute_meta_h...
Compiling module work.TopParser_t_start_compute_hdr_et...
Compiling module work.TopParser_t_start_compute_hdr_et...
Compiling module work.TopParser_t_start_compute_hdr_et...
Compiling module work.TopParser_t_start_compute_hdr_et...
Compiling module work.TopParser_t_start_compute_TopPar...
Compiling module work.TopParser_t_start_compute_contro...
Compiling module work.TopParser_t_start_compute_contro...
Compiling module work.TopParser_t_start
Compiling module work.TopParser_t_reject_compute_contr...
Compiling module work.TopParser_t_reject_compute_contr...
Compiling module work.TopParser_t_reject
Compiling module work.TopParser_t_EngineStage_0_TupleF...
Compiling module work.TopParser_t_EngineStage_0
Compiling module work.TopParser_t_EngineStage_1_ErrorC...
Compiling module work.TopParser_t_EngineStage_1_Extrac...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv4_compute_TopPars...
Compiling module work.TopParser_t_ipv4_compute_meta_le...
Compiling module work.TopParser_t_ipv4_compute_control...
Compiling module work.TopParser_t_ipv4_compute_control...
Compiling module work.TopParser_t_ipv4
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_hdr_ipv...
Compiling module work.TopParser_t_ipv6_compute_TopPars...
Compiling module work.TopParser_t_ipv6_compute_meta_le...
Compiling module work.TopParser_t_ipv6_compute_control...
Compiling module work.TopParser_t_ipv6_compute_control...
Compiling module work.TopParser_t_ipv6
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_hdr_arp_...
Compiling module work.TopParser_t_arp_compute_TopParse...
Compiling module work.TopParser_t_arp_compute_control_...
Compiling module work.TopParser_t_arp_compute_control_...
Compiling module work.TopParser_t_arp
Compiling module work.TopParser_t_EngineStage_1_TupleF...
Compiling module work.TopParser_t_EngineStage_1
Compiling module work.TopParser_t_EngineStage_2_ErrorC...
Compiling module work.TopParser_t_EngineStage_2_Extrac...
Compiling module work.TopParser_t_icmp6_compute_hdr_ic...
Compiling module work.TopParser_t_icmp6_compute_hdr_ic...
Compiling module work.TopParser_t_icmp6_compute_hdr_ic...
Compiling module work.TopParser_t_icmp6_compute_hdr_ic...
Compiling module work.TopParser_t_icmp6_compute_TopPar...
Compiling module work.TopParser_t_icmp6_compute_contro...
Compiling module work.TopParser_t_icmp6_compute_contro...
Compiling module work.TopParser_t_icmp6
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_hdr_tcp_...
Compiling module work.TopParser_t_tcp_compute_TopParse...
Compiling module work.TopParser_t_tcp_compute_control_...
Compiling module work.TopParser_t_tcp_compute_control_...
Compiling module work.TopParser_t_tcp
Compiling module work.TopParser_t_udp_compute_hdr_udp_...
Compiling module work.TopParser_t_udp_compute_hdr_udp_...
Compiling module work.TopParser_t_udp_compute_hdr_udp_...
Compiling module work.TopParser_t_udp_compute_hdr_udp_...
Compiling module work.TopParser_t_udp_compute_hdr_udp_...
Compiling module work.TopParser_t_udp_compute_TopParse...
Compiling module work.TopParser_t_udp_compute_control_...
Compiling module work.TopParser_t_udp_compute_control_...
Compiling module work.TopParser_t_udp
Compiling module work.TopParser_t_icmp_compute_hdr_icm...
Compiling module work.TopParser_t_icmp_compute_hdr_icm...
Compiling module work.TopParser_t_icmp_compute_hdr_icm...
Compiling module work.TopParser_t_icmp_compute_hdr_icm...
Compiling module work.TopParser_t_icmp_compute_TopPars...
Compiling module work.TopParser_t_icmp_compute_control...
Compiling module work.TopParser_t_icmp_compute_control...
Compiling module work.TopParser_t_icmp
Compiling module work.TopParser_t_EngineStage_2_TupleF...
Compiling module work.TopParser_t_EngineStage_2
Compiling module work.TopParser_t_EngineStage_3_ErrorC...
Compiling module work.TopParser_t_EngineStage_3_Extrac...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_icmp6_neighbor_solic...
Compiling module work.TopParser_t_EngineStage_3_TupleF...
Compiling module work.TopParser_t_EngineStage_3
Compiling module work.TopParser_t_EngineStage_4_ErrorC...
Compiling module work.TopParser_t_accept_compute_contr...
Compiling module work.TopParser_t_accept_compute_contr...
Compiling module work.TopParser_t_accept
Compiling module work.TopParser_t_EngineStage_4
Compiling module work.TopParser_t_Engine
Compiling module work.TopParser_t
Compiling module work.TopPipe_lvl_t_setup_compute_dumm...
Compiling module work.TopPipe_lvl_t_setup_compute_cont...
Compiling module work.TopPipe_lvl_t_setup_compute_cont...
Compiling module work.TopPipe_lvl_t_setup
Compiling module work.TopPipe_lvl_t_EngineStage_0
Compiling module work.TopPipe_lvl_t_Engine
Compiling module work.TopPipe_lvl_t
Compiling module work.dummy_table_for_netpfga_t_Hash_L...
Compiling module work.xpm_memory_base(MEMORY_SIZE=992,...
Compiling module work.xpm_memory_tdpram(MEMORY_SIZE=99...
Compiling module work.dummy_table_for_netpfga_t_RamR1R...
Compiling module work.dummy_table_for_netpfga_t_Cam
Compiling module work.dummy_table_for_netpfga_t_Lookup
Compiling module work.dummy_table_for_netpfga_t_Hash_U...
Compiling module work.dummy_table_for_netpfga_t_Randmo...
Compiling module work.dummy_table_for_netpfga_t_Randmo...
Compiling module work.dummy_table_for_netpfga_t_Randmo...
Compiling module work.dummy_table_for_netpfga_t_Randmo...
Compiling module work.dummy_table_for_netpfga_t_Update
Compiling module work.dummy_table_for_netpfga_t_IntTop
Compiling module work.dummy_table_for_netpfga_t_Wrap
Compiling module work.dummy_table_for_netpfga_t_csr
Compiling module work.dummy_table_for_netpfga_t
Compiling module work.TopPipe_lvl_0_t_dummy_table_for_...
Compiling module work.TopPipe_lvl_0_t_dummy_table_for_...
Compiling module work.TopPipe_lvl_0_t_dummy_table_for_...
Compiling module work.TopPipe_lvl_0_t_EngineStage_0
Compiling module work.TopPipe_lvl_0_t_do_nothing_0_sec...
Compiling module work.TopPipe_lvl_0_t_do_nothing_0_sec...
Compiling module work.TopPipe_lvl_0_t_do_nothing_0_sec
Compiling module work.TopPipe_lvl_0_t_send_to_port1_0_...
Compiling module work.TopPipe_lvl_0_t_send_to_port1_0_...
Compiling module work.TopPipe_lvl_0_t_send_to_port1_0_...
Compiling module work.TopPipe_lvl_0_t_send_to_port1_0_...
Compiling module work.TopPipe_lvl_0_t_EngineStage_1
Compiling module work.TopPipe_lvl_0_t_sink_compute_con...
Compiling module work.TopPipe_lvl_0_t_sink_compute_con...
Compiling module work.TopPipe_lvl_0_t_sink
Compiling module work.TopPipe_lvl_0_t_EngineStage_2
Compiling module work.TopPipe_lvl_0_t_Engine
Compiling module work.TopPipe_lvl_0_t
Compiling module work.TopDeparser_t_EngineStage_0_Erro...
Compiling module work.TopDeparser_t_extract_headers_se...
Compiling module work.TopDeparser_t_extract_headers_se...
Compiling module work.TopDeparser_t_extract_headers_se...
Compiling module work.TopDeparser_t_extract_headers_se...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0_Edit...
Compiling module work.TopDeparser_t_EngineStage_0
Compiling module work.TopDeparser_t_EngineStage_1_Erro...
Compiling module work.TopDeparser_t_act_sec_compute_co...
Compiling module work.TopDeparser_t_act_sec_compute_co...
Compiling module work.TopDeparser_t_act_sec
Compiling module work.TopDeparser_t_EngineStage_1
Compiling module work.TopDeparser_t_EngineStage_2_Erro...
Compiling module work.TopDeparser_t_emit_10_compute_co...
Compiling module work.TopDeparser_t_emit_10_compute__S...
Compiling module work.TopDeparser_t_emit_10_compute__S...
Compiling module work.TopDeparser_t_emit_10_compute__S...
Compiling module work.TopDeparser_t_emit_10_compute_co...
Compiling module work.TopDeparser_t_emit_10_compute_co...
Compiling module work.TopDeparser_t_emit_10
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2_Edit...
Compiling module work.TopDeparser_t_EngineStage_2
Compiling module work.TopDeparser_t_EngineStage_3_Erro...
Compiling module work.TopDeparser_t_emit_9_compute_con...
Compiling module work.TopDeparser_t_emit_9_compute__ST...
Compiling module work.TopDeparser_t_emit_9_compute__ST...
Compiling module work.TopDeparser_t_emit_9_compute__ST...
Compiling module work.TopDeparser_t_emit_9_compute__ST...
Compiling module work.TopDeparser_t_emit_9_compute_con...
Compiling module work.TopDeparser_t_emit_9_compute_con...
Compiling module work.TopDeparser_t_emit_9
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3_Edit...
Compiling module work.TopDeparser_t_EngineStage_3
Compiling module work.TopDeparser_t_EngineStage_4_Erro...
Compiling module work.TopDeparser_t_emit_8_compute_con...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute__ST...
Compiling module work.TopDeparser_t_emit_8_compute_con...
Compiling module work.TopDeparser_t_emit_8_compute_con...
Compiling module work.TopDeparser_t_emit_8
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4_Edit...
Compiling module work.TopDeparser_t_EngineStage_4
Compiling module work.TopDeparser_t_EngineStage_5_Erro...
Compiling module work.TopDeparser_t_emit_7_compute_con...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute__ST...
Compiling module work.TopDeparser_t_emit_7_compute_con...
Compiling module work.TopDeparser_t_emit_7_compute_con...
Compiling module work.TopDeparser_t_emit_7
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5_Edit...
Compiling module work.TopDeparser_t_EngineStage_5
Compiling module work.TopDeparser_t_EngineStage_6_Erro...
Compiling module work.TopDeparser_t_emit_6_compute_con...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute__ST...
Compiling module work.TopDeparser_t_emit_6_compute_con...
Compiling module work.TopDeparser_t_emit_6_compute_con...
Compiling module work.TopDeparser_t_emit_6
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6_Edit...
Compiling module work.TopDeparser_t_EngineStage_6
Compiling module work.TopDeparser_t_EngineStage_7_Erro...
Compiling module work.TopDeparser_t_emit_5_compute_con...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute__ST...
Compiling module work.TopDeparser_t_emit_5_compute_con...
Compiling module work.TopDeparser_t_emit_5_compute_con...
Compiling module work.TopDeparser_t_emit_5
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7_Edit...
Compiling module work.TopDeparser_t_EngineStage_7
Compiling module work.TopDeparser_t_EngineStage_8_Erro...
Compiling module work.TopDeparser_t_emit_4_compute_con...
Compiling module work.TopDeparser_t_emit_4_compute__ST...
Compiling module work.TopDeparser_t_emit_4_compute__ST...
Compiling module work.TopDeparser_t_emit_4_compute__ST...
Compiling module work.TopDeparser_t_emit_4_compute__ST...
Compiling module work.TopDeparser_t_emit_4_compute_con...
Compiling module work.TopDeparser_t_emit_4_compute_con...
Compiling module work.TopDeparser_t_emit_4
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8_Edit...
Compiling module work.TopDeparser_t_EngineStage_8
Compiling module work.TopDeparser_t_EngineStage_9_Erro...
Compiling module work.TopDeparser_t_emit_3_compute_con...
Compiling module work.TopDeparser_t_emit_3_compute__ST...
Compiling module work.TopDeparser_t_emit_3_compute__ST...
Compiling module work.TopDeparser_t_emit_3_compute__ST...
Compiling module work.TopDeparser_t_emit_3_compute_con...
Compiling module work.TopDeparser_t_emit_3_compute_con...
Compiling module work.TopDeparser_t_emit_3
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9_Edit...
Compiling module work.TopDeparser_t_EngineStage_9
Compiling module work.TopDeparser_t_EngineStage_10_Err...
Compiling module work.TopDeparser_t_emit_2_compute_con...
Compiling module work.TopDeparser_t_emit_2_compute__ST...
Compiling module work.TopDeparser_t_emit_2_compute__ST...
Compiling module work.TopDeparser_t_emit_2_compute__ST...
Compiling module work.TopDeparser_t_emit_2_compute_con...
Compiling module work.TopDeparser_t_emit_2_compute_con...
Compiling module work.TopDeparser_t_emit_2
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10_Edi...
Compiling module work.TopDeparser_t_EngineStage_10
Compiling module work.TopDeparser_t_EngineStage_11_Err...
Compiling module work.TopDeparser_t_emit_1_compute_con...
Compiling module work.TopDeparser_t_emit_1_compute__ST...
Compiling module work.TopDeparser_t_emit_1_compute__ST...
Compiling module work.TopDeparser_t_emit_1_compute__ST...
Compiling module work.TopDeparser_t_emit_1_compute__ST...
Compiling module work.TopDeparser_t_emit_1_compute__ST...
Compiling module work.TopDeparser_t_emit_1_compute_con...
Compiling module work.TopDeparser_t_emit_1_compute_con...
Compiling module work.TopDeparser_t_emit_1
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11_Edi...
Compiling module work.TopDeparser_t_EngineStage_11
Compiling module work.TopDeparser_t_EngineStage_12_Err...
Compiling module work.TopDeparser_t_emit_0_compute_con...
Compiling module work.TopDeparser_t_emit_0_compute__ST...
Compiling module work.TopDeparser_t_emit_0_compute__ST...
Compiling module work.TopDeparser_t_emit_0_compute__ST...
Compiling module work.TopDeparser_t_emit_0_compute_con...
Compiling module work.TopDeparser_t_emit_0_compute_con...
Compiling module work.TopDeparser_t_emit_0
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12_Edi...
Compiling module work.TopDeparser_t_EngineStage_12
Compiling module work.TopDeparser_t_Engine
Compiling module work.TopDeparser_t
Compiling module work.xpm_cdc_sync_rst(DEST_SYNC_FF=2,...
Compiling module work.xpm_fifo_rst(COMMON_CLOCK=0)
Compiling module work.xpm_fifo_reg_bit
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=9...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=8...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=8...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_cdc_gray(DEST_SYNC_FF=2,INIT...
Compiling module work.xpm_fifo_reg_vec(REG_WIDTH=8)
Compiling module work.xpm_cdc_gray(DEST_SYNC_FF=2,INIT...
Compiling module work.xpm_fifo_reg_vec(REG_WIDTH=9)
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.S_BRIDGER_for_dummy_table_for_ne...
Compiling module work.S_PROTOCOL_ADAPTER_INGRESS
Compiling module work.S_PROTOCOL_ADAPTER_EGRESS
Compiling module work.xpm_fifo_rst_default
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=1...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=9...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=9...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=2...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=1...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.S_SYNCER_for_TopParser
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=1...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.S_SYNCER_for_S_SYNCER_for_S_SYNC...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=1...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=8...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=7...
Compiling module work.xpm_counter_updn(COUNTER_WIDTH=7...
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_cdc_gray(DEST_SYNC_FF=2,INIT...
Compiling module work.xpm_fifo_reg_vec(REG_WIDTH=7)
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.S_SYNCER_for_S_SYNCER_for_TopDep...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=1...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.S_SYNCER_for_TopDeparser
Compiling module work.xpm_memory_base(MEMORY_TYPE=1,ME...
Compiling module work.xpm_fifo_base(FIFO_MEMORY_TYPE=2...
Compiling module work.xpm_fifo_sync(FIFO_MEMORY_TYPE="...
Compiling module work.xpm_fifo_base(COMMON_CLOCK=0,FIF...
Compiling module work.xpm_fifo_async(FIFO_MEMORY_TYPE=...
Compiling module work.S_SYNCER_for__OUT_
Compiling module work.S_CONTROLLER_SimpleSumeSwitch
Compiling module work.SimpleSumeSwitch
Compiling module work.TB_System_Stim
Compiling module work.Check
Compiling module work.SimpleSumeSwitch_tb
Compiling module work.glbl
Built simulation snapshot work.SimpleSumeSwitch_tb#work.glbl

****** Webtalk v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/webtalk/xsim_webtalk.tcl -notrace
INFO: [Common 17-186] '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/webtalk/usage_statistics_ext_xsim.xml' has been successfully sent to Xilinx on Sat Jul 13 19:40:24 2019. For additional details about this file, please refer to the WebTalk help file at /opt/Xilinx/Vivado/2018.2/doc/webtalk_introduction.html.
INFO: [Common 17-206] Exiting Webtalk at Sat Jul 13 19:40:24 2019...
+ /opt/Xilinx/Vivado/2018.2/bin/xsim --runall SimpleSumeSwitch_tb#work.glbl

****** xsim v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source xsim.dir/work.SimpleSumeSwitch_tb#work.glbl/xsim_script.tcl
# xsim {work.SimpleSumeSwitch_tb#work.glbl} -autoloadwcfg -runall
Vivado Simulator 2018.2
Time resolution is 1 ps
run -all
Info: [XPM_MEMORY 20-1] MEMORY_PRIMITIVE (0) instructs Vivado Synthesis to choose the memory primitive type. Depending on their values, other XPM_MEMORY parameters may preclude the choice of certain memory primitive types. Review XPM_MEMORY documentation and parameter values to understand any limitations, or set MEMORY_PRIMITIVE to a different value. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.dummy_table_for_netpfga.dummy_table_for_netpfga_t_Wrap_inst.dummy_table_for_netpfga_t_IntTop_inst.dummy_table_for_netpfga_t_Lookup_inst.dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_0.xpm_memory_tdpram_inst.xpm_memory_base_inst.config_drc
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/dummy_table_for_netpfga/dummy_table_for_netpfga_t_Wrap_inst/dummy_table_for_netpfga_t_IntTop_inst/dummy_table_for_netpfga_t_Lookup_inst/dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_0/xpm_memory_tdpram_inst/xpm_memory_base_inst/Initial270_678  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-1] MEMORY_PRIMITIVE (0) instructs Vivado Synthesis to choose the memory primitive type. Depending on their values, other XPM_MEMORY parameters may preclude the choice of certain memory primitive types. Review XPM_MEMORY documentation and parameter values to understand any limitations, or set MEMORY_PRIMITIVE to a different value. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.dummy_table_for_netpfga.dummy_table_for_netpfga_t_Wrap_inst.dummy_table_for_netpfga_t_IntTop_inst.dummy_table_for_netpfga_t_Lookup_inst.dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_1.xpm_memory_tdpram_inst.xpm_memory_base_inst.config_drc
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/dummy_table_for_netpfga/dummy_table_for_netpfga_t_Wrap_inst/dummy_table_for_netpfga_t_IntTop_inst/dummy_table_for_netpfga_t_Lookup_inst/dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_1/xpm_memory_tdpram_inst/xpm_memory_base_inst/Initial270_678  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-1] MEMORY_PRIMITIVE (0) instructs Vivado Synthesis to choose the memory primitive type. Depending on their values, other XPM_MEMORY parameters may preclude the choice of certain memory primitive types. Review XPM_MEMORY documentation and parameter values to understand any limitations, or set MEMORY_PRIMITIVE to a different value. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.dummy_table_for_netpfga.dummy_table_for_netpfga_t_Wrap_inst.dummy_table_for_netpfga_t_IntTop_inst.dummy_table_for_netpfga_t_Lookup_inst.dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_2.xpm_memory_tdpram_inst.xpm_memory_base_inst.config_drc
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/dummy_table_for_netpfga/dummy_table_for_netpfga_t_Wrap_inst/dummy_table_for_netpfga_t_IntTop_inst/dummy_table_for_netpfga_t_Lookup_inst/dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_2/xpm_memory_tdpram_inst/xpm_memory_base_inst/Initial270_678  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-1] MEMORY_PRIMITIVE (0) instructs Vivado Synthesis to choose the memory primitive type. Depending on their values, other XPM_MEMORY parameters may preclude the choice of certain memory primitive types. Review XPM_MEMORY documentation and parameter values to understand any limitations, or set MEMORY_PRIMITIVE to a different value. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.dummy_table_for_netpfga.dummy_table_for_netpfga_t_Wrap_inst.dummy_table_for_netpfga_t_IntTop_inst.dummy_table_for_netpfga_t_Lookup_inst.dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_3.xpm_memory_tdpram_inst.xpm_memory_base_inst.config_drc
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/dummy_table_for_netpfga/dummy_table_for_netpfga_t_Wrap_inst/dummy_table_for_netpfga_t_IntTop_inst/dummy_table_for_netpfga_t_Lookup_inst/dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_3/xpm_memory_tdpram_inst/xpm_memory_base_inst/Initial270_678  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-1] MEMORY_PRIMITIVE (0) instructs Vivado Synthesis to choose the memory primitive type. Depending on their values, other XPM_MEMORY parameters may preclude the choice of certain memory primitive types. Review XPM_MEMORY documentation and parameter values to understand any limitations, or set MEMORY_PRIMITIVE to a different value. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.dummy_table_for_netpfga.dummy_table_for_netpfga_t_Wrap_inst.dummy_table_for_netpfga_t_IntTop_inst.dummy_table_for_netpfga_t_Lookup_inst.dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_4.xpm_memory_tdpram_inst.xpm_memory_base_inst.config_drc
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/dummy_table_for_netpfga/dummy_table_for_netpfga_t_Wrap_inst/dummy_table_for_netpfga_t_IntTop_inst/dummy_table_for_netpfga_t_Lookup_inst/dummy_table_for_netpfga_t_RamR1RW1_KeyValue_inst_4/xpm_memory_tdpram_inst/xpm_memory_base_inst/Initial270_678  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.myfifo.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request/myfifo/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4841  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopParser.d4r9s1dt31odylca4j08jvaalows_1326.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopParser/d4r9s1dt31odylca4j08jvaalows_1326/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4934  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopParser.shwior7c57px7lhykr69b4h55gy_1189.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopParser/shwior7c57px7lhykr69b4h55gy_1189/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4964  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopParser.n1sx4t3gv74d6ley2bc7vqai0_671.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopParser/n1sx4t3gv74d6ley2bc7vqai0_671/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5028  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopParser.qlx1pdysubk6kdbe7rfumqg94ml_1100.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopParser/qlx1pdysubk6kdbe7rfumqg94ml_1100/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5112  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.r80w27w8xkrfz6fl7c4a1yg3_2547.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/r80w27w8xkrfz6fl7c4a1yg3_2547/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4934  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.akowy96xockbk3r40na1e0_1411.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/akowy96xockbk3r40na1e0_1411/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4964  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.mkx0m7txszkzpcexkt_1012.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/mkx0m7txszkzpcexkt_1012/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5293  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.xoxsx56zo5nmy9crme8ye_2175.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/xoxsx56zo5nmy9crme8ye_2175/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5377  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.ixwolb8izh1mcn3pm82da9zw1bledr_2002.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/ixwolb8izh1mcn3pm82da9zw1bledr_2002/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5461  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.su2btkuygtuf8lj2_1957.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/su2btkuygtuf8lj2_1957/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5028  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.xwepnbeep4q8vrdtit1k_1758.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/xwepnbeep4q8vrdtit1k_1758/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5112  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.nfc245j2kczfctkem5wo_267.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser/nfc245j2kczfctkem5wo_267/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5713  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.xsx0bth0s5vul5bnzys1r15v_636.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/xsx0bth0s5vul5bnzys1r15v_636/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4934  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.e8merxupg0pos42mhwv79s4uzd_2330.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/e8merxupg0pos42mhwv79s4uzd_2330/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4964  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.sm8ad7rbbhczx6axp99i4b4kerlik_2622.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/sm8ad7rbbhczx6axp99i4b4kerlik_2622/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5461  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.ejuqnpxpas6ebnp1wsv03r3hul7c_1779.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/ejuqnpxpas6ebnp1wsv03r3hul7c_1779/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5293  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.s1bq6q30gnlgws57l7ob5_1536.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/s1bq6q30gnlgws57l7ob5_1536/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_6066  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.cdr4wn5f7vf8we6pqlccnwjwwhbk_205.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/cdr4wn5f7vf8we6pqlccnwjwwhbk_205/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5377  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.c5vlijc052mnm1qwhml_2059.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/c5vlijc052mnm1qwhml_2059/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5028  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.fx8dmi6ohxw9f7y17ld3jpi3ovx_1879.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/fx8dmi6ohxw9f7y17ld3jpi3ovx_1879/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_6318  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.jvuwzicuodkmfhrme9ma316m3bqgcr1l_2346.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/jvuwzicuodkmfhrme9ma316m3bqgcr1l_2346/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5112  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_S_SYNCER_for_TopDeparser.ry7j4cxmi66xbhtnzin8ircq33_2068.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_S_SYNCER_for_TopDeparser/ry7j4cxmi66xbhtnzin8ircq33_2068/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5713  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.qp37jigvkkctbg4mw_2611.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/qp37jigvkkctbg4mw_2611/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4934  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.gdlmsweqy7ga1hf76_1891.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/gdlmsweqy7ga1hf76_1891/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4964  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.koj5x4b2mrhepx6j1wm4gdwazr96xbo8_1212.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/koj5x4b2mrhepx6j1wm4gdwazr96xbo8_1212/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5293  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.vclw21ikq86k6h6g133nzde_2512.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/vclw21ikq86k6h6g133nzde_2512/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5377  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.j45zq32et5jfy3smb7kx_2626.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/j45zq32et5jfy3smb7kx_2626/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5461  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.cza0n0z0z15dgswrqyf0f9lvd1dwjgeo_2512.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/cza0n0z0z15dgswrqyf0f9lvd1dwjgeo_2512/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5028  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.f4nv9dak0xeq6b14i_724.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/f4nv9dak0xeq6b14i_724/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5112  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for_TopDeparser.grws3d5reusenvj4f5ui2bfbz_2390.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for_TopDeparser/grws3d5reusenvj4f5ui2bfbz_2390/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5713  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for__OUT_.dr1n8epbxxf9z6nc1v1_2107.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for__OUT_/dr1n8epbxxf9z6nc1v1_2107/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_7172  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for__OUT_.awuy93pjehf0c16umx7_193.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for__OUT_/awuy93pjehf0c16umx7_193/xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_4964  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for__OUT_.zlneebxlhzf2gvvxtoajw8hc_2576.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for__OUT_/zlneebxlhzf2gvvxtoajw8hc_2576/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5461  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's. SimpleSumeSwitch_tb.SimpleSumeSwitch_i.S_SYNCER_for__OUT_.txtaj3d8pz8zdwcn48d_848.gnuram_async_fifo.xpm_fifo_base_inst.gen_sdpram.xpm_memory_base_inst.config_drc  0
Time: 1 ps  Iteration: 0  Process: /SimpleSumeSwitch_tb/SimpleSumeSwitch_i/S_SYNCER_for__OUT_/txtaj3d8pz8zdwcn48d_848/gnuram_async_fifo.xpm_fifo_base_inst/gen_sdpram.xpm_memory_base_inst/Initial270_5028  File: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv
[SW] CAM_Init() - start
[SW] CAM_Init() - done
[SW] CAM_EnableDevice() - start
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_write_control()- start
SV_write_control()- done
[SW] CAM_EnableDevice() - done
CAM UPDATE           0: KEY(hex) = 82222222208 VALUE(hex) = 201
SV_write_control()- start
[SW] CAM_WriteEntry() - start
SV_write_control()- done
SV_write_control()- start
SV_write_control()- done
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_write_control()- start
SV_write_control()- done
SV_read_control()- start
SV_read_control()- done
SV_read_control()- start
[SW] CAM_WriteEntry() - done
SV_read_control()- done
[2850526]  INFO: finished packet stimulus file
[4301612]  INFO: packet 1 tuple OK < tuple_out_digest_data, tuple_out_standard_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001010000 >
[4301612]  INFO: packet 1  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000000081111111108082222222208)
[4304944]  INFO: packet 1  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[4311608]  INFO: packet 2 tuple OK < tuple_out_digest_data, tuple_out_standard_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001040000 >
[4311608]  INFO: packet 2  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000000081111111108082222222208)
[4314940]  INFO: packet 2  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[4321604]  INFO: packet 3 tuple OK < tuple_out_digest_data, tuple_out_standard_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001100000 >
[4321604]  INFO: packet 3  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000000081111111108082222222208)
[4324936]  INFO: packet 3  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[4331600]  INFO: packet 4 tuple OK < tuple_out_digest_data, tuple_out_standard_metadata > = < 0000000000000000000000000000000000000000000000000000000000000000 00000000000000000000000001400000 >
[4331600]  INFO: packet 4  data OK (tlast, tkeep, tdata) = (0, ffffffff, 0000000000000000000000000000000000000000081111111108082222222208)
[4334932]  INFO: packet 4  data OK (tlast, tkeep, tdata) = (1, ffffffff, 0000000000000000000000000000000000000000000000000000000000000000)
[7670264]  INFO: stopping simulation after 1000 idle cycles
[7670264]  INFO: all expected data successfully received
[7670264]  INFO: TEST PASSED
$finish called at time : 7670264 ps : File "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/SimpleSumeSwitch_tb.sv" Line 207
exit
INFO: [Common 17-206] Exiting xsim at Sat Jul 13 19:40:36 2019...
+ grep ^expected LOG
+ sed -e s/.*= <// -e s/.*= (//
+ expected_line=
+ grep ^actual LOG
+ sed -e s/.*= <// -e s/.*= (//
+ actual_line=
+ [  !=  ]
+ cd /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4
+ make config_writes
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/bin/gen_config_writes.py nf_sume_sdnet_ip/SimpleSumeSwitch/config_writes.txt 0x44020000 testdata
orig dic: OrderedDict([(0, ('00000020', '00000001')), (1, ('00000020', '00000000')), (2, ('00000050', '22222208')), (3, ('00000054', '00000822')), (4, ('00000080', '00000201')), (5, ('00000040', '00000001'))])
new dic: OrderedDict([(2, ('00000050', '22222208')), (3, ('00000054', '00000822')), (4, ('00000080', '00000201')), (5, ('00000040', '00000001'))])
+ cd /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4
+ make uninstall_sdnet
rm -rf /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip
+ make install_sdnet
rm -rf /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip
cp -r nf_sume_sdnet_ip /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/
mkdir /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/wrapper
cp /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/templates/sss_wrapper/hdl/* /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/wrapper/
cp /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/templates/sss_wrapper/tcl/* /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/
cp /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/templates/sss_wrapper/Makefile /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/
make -C /home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip'
rm -rf ip_*  vivado*.* *.xml xgui/ .Xil* *.*~ *.zip 
vivado -mode batch -source nf_sume_sdnet.tcl

****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source nf_sume_sdnet.tcl
# set design nf_sume_sdnet
# set top nf_sume_sdnet
# set device xc7vx690t-3-ffg1761
# set proj_dir ./ip_proj
# set ip_version 1.00
# set lib_name NetFPGA
# create_project -name ${design} -force -dir "./${proj_dir}" -part ${device}
# set_property source_mgmt_mode All [current_project]  
# set_property top ${top} [current_fileset]
# set_property ip_repo_paths $::env(SUME_FOLDER)/lib/hw/  [current_fileset]
# update_ip_catalog
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/lib/hw'.
WARNING: [IP_Flow 19-3656] If you move the project, the path for repository '/home/nico/projects/P4-NetFPGA/lib/hw' may become invalid. A better location for the repository would be in a path adjacent to the project. (Current project location is '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj'.)
INFO: [IP_Flow 19-2313] Loaded Vivado IP repository '/opt/Xilinx/Vivado/2018.2/data/ip'.
# puts "nf_sume_sdnet"
nf_sume_sdnet
# read_verilog "./wrapper/sume_to_sdnet.v"
# read_verilog "./wrapper/nf_sume_sdnet.v"
# read_verilog "./wrapper/changeEndian.v"
# add_files -scan_for_includes ./SimpleSumeSwitch/
# import_files -force
INFO: [filemgmt 20-348] Importing the appropriate files for fileset: 'sources_1'
# update_compile_order -fileset sources_1
update_compile_order: Time (s): cpu = 00:00:03 ; elapsed = 00:00:05 . Memory (MB): peak = 1252.852 ; gain = 4.000 ; free physical = 10549 ; free virtual = 15744
# update_compile_order -fileset sim_1
update_compile_order: Time (s): cpu = 00:00:03 ; elapsed = 00:00:05 . Memory (MB): peak = 1254.852 ; gain = 2.000 ; free physical = 10547 ; free virtual = 15742
# ipx::package_project
WARNING: [IP_Flow 19-3899] Cannot get the environment domain name variable for the component vendor name. Setting the vendor name to 'user.org'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/wrapper/changeEndian.v'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.h'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.vp'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.vp'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/SimpleSumeSwitch_tb.sv'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/dpi.h'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/Check.v'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/CAM.h'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/CAM_INST0.h'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/Testbench/TB_System_Stim.v'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_CONTROLLERs.HDL/S_CONTROLLER_SimpleSumeSwitch.vp'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/glbl.v'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_cdc.sv'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_memory.sv'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/xpm_fifo.sv'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.vp'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/glbl.v'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/xpm_cdc.sv'.
WARNING: [IP_Flow 19-3833] Unreferenced file from the top module is not packaged: '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj/nf_sume_sdnet.srcs/sources_1/imports/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/xpm_memory.sv'.
INFO: [IP_Flow 19-5169] Module 'nf_sume_sdnet' uses SystemVerilog sources with a Verilog top file. These SystemVerilog files will not be analysed by the packager.
INFO: [IP_Flow 19-5107] Inferred bus interface 'm_axis' of definition 'xilinx.com:interface:axis:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-5107] Inferred bus interface 's_axis' of definition 'xilinx.com:interface:axis:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-5107] Inferred bus interface 'S_AXI' of definition 'xilinx.com:interface:aximm:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-5107] Inferred bus interface 'S_AXI_ARESETN' of definition 'xilinx.com:signal:reset:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-5107] Inferred bus interface 'axis_resetn' of definition 'xilinx.com:signal:reset:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-5107] Inferred bus interface 'S_AXI_ACLK' of definition 'xilinx.com:signal:clock:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-5107] Inferred bus interface 'axis_aclk' of definition 'xilinx.com:signal:clock:1.0' (from Xilinx Repository).
INFO: [IP_Flow 19-4728] Bus Interface 'S_AXI_ARESETN': Added interface parameter 'POLARITY' with value 'ACTIVE_LOW'.
INFO: [IP_Flow 19-4728] Bus Interface 'axis_resetn': Added interface parameter 'POLARITY' with value 'ACTIVE_LOW'.
INFO: [IP_Flow 19-4728] Bus Interface 'S_AXI_ACLK': Added interface parameter 'ASSOCIATED_BUSIF' with value 'S_AXI'.
INFO: [IP_Flow 19-4728] Bus Interface 'axis_aclk': Added interface parameter 'ASSOCIATED_BUSIF' with value 'm_axis'.
INFO: [IP_Flow 19-4728] Bus Interface 'S_AXI_ACLK': Added interface parameter 'ASSOCIATED_RESET' with value 'S_AXI_ARESETN'.
INFO: [IP_Flow 19-4728] Bus Interface 'axis_aclk': Added interface parameter 'ASSOCIATED_RESET' with value 'axis_resetn'.
INFO: [IP_Flow 19-2181] Payment Required is not set for this core.
INFO: [IP_Flow 19-2187] The Product Guide file is missing.
ipx::package_project: Time (s): cpu = 00:00:05 ; elapsed = 00:00:11 . Memory (MB): peak = 1313.492 ; gain = 31.000 ; free physical = 10532 ; free virtual = 15726
# set_property name ${design} [ipx::current_core]
# set_property library ${lib_name} [ipx::current_core]
# set_property vendor_display_name {NetFPGA} [ipx::current_core]
# set_property company_url {http://www.netfpga.org} [ipx::current_core]
# set_property vendor {NetFPGA} [ipx::current_core]
# set_property supported_families {{virtex7} {Production}} [ipx::current_core]
# set_property taxonomy {{/NetFPGA/Generic}} [ipx::current_core]
# set_property version ${ip_version} [ipx::current_core]
# set_property display_name ${design} [ipx::current_core]
# set_property description ${design} [ipx::current_core]
# ipx::add_user_parameter {C_M_AXIS_DATA_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter C_M_AXIS_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {C_M_AXIS_DATA_WIDTH} [ipx::get_user_parameter C_M_AXIS_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {256} [ipx::get_user_parameter C_M_AXIS_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter C_M_AXIS_DATA_WIDTH [ipx::current_core]]
# ipx::add_user_parameter {C_S_AXIS_DATA_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter C_S_AXIS_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {C_S_AXIS_DATA_WIDTH} [ipx::get_user_parameter C_S_AXIS_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {256} [ipx::get_user_parameter C_S_AXIS_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter C_S_AXIS_DATA_WIDTH [ipx::current_core]]
# ipx::add_user_parameter {C_M_AXIS_TUSER_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter C_M_AXIS_TUSER_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {C_M_AXIS_TUSER_WIDTH} [ipx::get_user_parameter C_M_AXIS_TUSER_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {128} [ipx::get_user_parameter C_M_AXIS_TUSER_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter C_M_AXIS_TUSER_WIDTH [ipx::current_core]]
# ipx::add_user_parameter {C_S_AXIS_TUSER_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter C_S_AXIS_TUSER_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {C_S_AXIS_TUSER_WIDTH} [ipx::get_user_parameter C_S_AXIS_TUSER_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {128} [ipx::get_user_parameter C_S_AXIS_TUSER_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter C_S_AXIS_TUSER_WIDTH [ipx::current_core]]
# ipx::add_user_parameter {C_S_AXI_DATA_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter C_S_AXI_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {C_S_AXI_DATA_WIDTH} [ipx::get_user_parameter C_S_AXI_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {32} [ipx::get_user_parameter C_S_AXI_DATA_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter C_S_AXI_DATA_WIDTH [ipx::current_core]]
# ipx::add_user_parameter {C_S_AXI_ADDR_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter C_S_AXI_ADDR_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {C_S_AXI_ADDR_WIDTH} [ipx::get_user_parameter C_S_AXI_ADDR_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {12} [ipx::get_user_parameter C_S_AXI_ADDR_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter C_S_AXI_ADDR_WIDTH [ipx::current_core]]
# ipx::add_user_parameter {SDNET_ADDR_WIDTH} [ipx::current_core]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_resolve_type {user} [ipx::get_user_parameter SDNET_ADDR_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property display_name {SDNET_ADDR_WIDTH} [ipx::get_user_parameter SDNET_ADDR_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value {11} [ipx::get_user_parameter SDNET_ADDR_WIDTH [ipx::current_core]]
WARNING: command 'get_user_parameter' will be removed in the 2015.3 release, use 'get_user_parameters' instead
# set_property value_format {long} [ipx::get_user_parameter SDNET_ADDR_WIDTH [ipx::current_core]]
# ipx::add_subcore xilinx.com:ip:axis_data_fifo:1.1 [ipx::get_file_groups xilinx_anylanguagesynthesis -of_objects [ipx::current_core]]
# ipx::add_subcore xilinx.com:ip:axis_data_fifo:1.1 [ipx::get_file_groups xilinx_anylanguagebehavioralsimulation -of_objects [ipx::current_core]]
# ipx::add_bus_parameter FREQ_HZ [ipx::get_bus_interfaces m_axis -of_objects [ipx::current_core]]
# ipx::add_bus_parameter FREQ_HZ [ipx::get_bus_interfaces s_axis -of_objects [ipx::current_core]]
# update_ip_catalog -rebuild 
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/lib/hw'.
WARNING: [IP_Flow 19-3656] If you move the project, the path for repository '/home/nico/projects/P4-NetFPGA/lib/hw' may become invalid. A better location for the repository would be in a path adjacent to the project. (Current project location is '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip/ip_proj'.)
# ipx::infer_user_parameters [ipx::current_core]
# ipx::check_integrity [ipx::current_core]
INFO: [IP_Flow 19-861] XGUI layout file basename "xgui/nf_sume_sdnet_v1_0.tcl" does not have the current IP <name>_v<version> format. If the IP name or version was changed recently, recreate this file to update the file format.
INFO: [IP_Flow 19-2181] Payment Required is not set for this core.
INFO: [IP_Flow 19-2187] The Product Guide file is missing.
INFO: [Ipptcl 7-1486] check_integrity: Integrity check passed.
# ipx::save_core [ipx::current_core]
# update_ip_catalog
# close_project
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 19:41:09 2019...
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/lib/hw/contrib/cores/nf_sume_sdnet_ip'
+ cd /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default
+ make
rm -f config_writes.py*
rm -f *.pyc
cp /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata/config_writes.py ./ 
+ cd /home/nico/projects/P4-NetFPGA
+ ./tools/scripts/nf_test.py sim --major switch --minor default
make: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test'
vivado -mode batch -source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_defines.tcl

****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_defines.tcl
# set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
# set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
# set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
# set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
# set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
# set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
# set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
# set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
# set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
# set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
# set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
# set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
# set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
# set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
# set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
# set M00_BASEADDR 0x44000000
# set M00_HIGHADDR 0x44000FFF
# set M00_SIZEADDR 0x1000
# set M01_BASEADDR 0x44010000
# set M01_HIGHADDR 0x44010FFF
# set M01_SIZEADDR 0x1000
# set M02_BASEADDR 0x44020000
# set M02_HIGHADDR 0x44020FFF
# set M02_SIZEADDR 0x1000
# set M03_BASEADDR 0x44030000
# set M03_HIGHADDR 0x44030FFF
# set M03_SIZEADDR 0x1000
# set M04_BASEADDR 0x44040000
# set M04_HIGHADDR 0x44040FFF
# set M04_SIZEADDR 0x1000
# set M05_BASEADDR 0x44050000
# set M05_HIGHADDR 0x44050FFF
# set M05_SIZEADDR 0x1000
# set M06_BASEADDR 0x44060000
# set M06_HIGHADDR 0x44060FFF
# set M06_SIZEADDR 0x1000
# set M07_BASEADDR 0x44070000
# set M07_HIGHADDR 0x44070FFF
# set M07_SIZEADDR 0x1000
# set M08_BASEADDR 0x44080000
# set M08_HIGHADDR 0x44080FFF
# set M08_SIZEADDR 0x1000
# set IDENTIFIER_BASEADDR $M00_BASEADDR
# set IDENTIFIER_HIGHADDR $M00_HIGHADDR
# set IDENTIFIER_SIZEADDR $M00_SIZEADDR
# set INPUT_ARBITER_BASEADDR $M01_BASEADDR
# set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
# set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
# set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
# set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
# set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
# set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
# set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
# set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
# set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
# set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
# set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
# set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
# set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
# set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
# set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
# set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
# set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
# set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
# set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
# set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
# set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
# set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
# set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 19:41:14 2019...
vivado -mode batch -source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/export_registers.tcl	

****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/export_registers.tcl
# set DEF_LIST {
# 	{MICROBLAZE_AXI_IIC 0 0 ""} \
# 	{MICROBLAZE_UARTLITE 0 0 ""} \
# 	{MICROBLAZE_DLMB_BRAM 0 0 ""} \
# 	{MICROBLAZE_ILMB_BRAM 0 0 ""} \
# 	{MICROBLAZE_AXI_INTC 0 0 ""} \
# 	{INPUT_ARBITER 0 1 input_arbiter_v1_0_0/data/input_arbiter_regs_defines.txt} \
# 	{OUTPUT_QUEUES 0 1 output_queues_v1_0_0/data/output_queues_regs_defines.txt} \
# 	{OUTPUT_PORT_LOOKUP 0 1 switch_output_port_lookup_v1_0_1/data/output_port_lookup_regs_defines.txt} \
# 	{NF_10G_INTERFACE0 0 1 nf_10ge_interface_shared_v1_0_0/data/nf_10g_interface_shared_regs_defines.txt} \
# 	{NF_10G_INTERFACE1 1 1 nf_10ge_interface_v1_0_0/data/nf_10g_interface_regs_defines.txt} \
# 	{NF_10G_INTERFACE2 2 1 nf_10ge_interface_v1_0_0/data/nf_10g_interface_regs_defines.txt} \
# 	{NF_10G_INTERFACE3 3 1 nf_10ge_interface_v1_0_0/data/nf_10g_interface_regs_defines.txt} \
# 	{NF_RIFFA_DMA 0 1 nf_riffa_dma_v1_0_0/data/nf_riffa_dma_regs_defines.txt} \
# 
# 
# }
# set target_path $::env(NF_DESIGN_DIR)/sw/embedded/src/
# set target_file $target_path/sume_register_defines.h
# proc write_header { target_file } {
# 
# # creat a blank header file
# # do a fresh rewrite in case the file already exits
# file delete -force $target_file
# open $target_file "w"
# set h_file [open $target_file "w"]
# 
# 
# puts $h_file "//-"
# puts $h_file "// Copyright (c) 2015 University of Cambridge"
# puts $h_file "// All rights reserved."
# puts $h_file "//"
# puts $h_file "// This software was developed by Stanford University and the University of Cambridge Computer Laboratory "
# puts $h_file "// under National Science Foundation under Grant No. CNS-0855268,"
# puts $h_file "// the University of Cambridge Computer Laboratory under EPSRC INTERNET Project EP/H040536/1 and"
# puts $h_file "// by the University of Cambridge Computer Laboratory under DARPA/AFRL contract FA8750-11-C-0249 (\"MRC2\"), "
# puts $h_file "// as part of the DARPA MRC research programme."
# puts $h_file "//"
# puts $h_file "// @NETFPGA_LICENSE_HEADER_START@"
# puts $h_file "//"
# puts $h_file "// Licensed to NetFPGA C.I.C. (NetFPGA) under one or more contributor"
# puts $h_file "// license agreements.  See the NOTICE file distributed with this work for"
# puts $h_file "// additional information regarding copyright ownership.  NetFPGA licenses this"
# puts $h_file "// file to you under the NetFPGA Hardware-Software License, Version 1.0 (the"
# puts $h_file "// \"License\"); you may not use this file except in compliance with the"
# puts $h_file "// License.  You may obtain a copy of the License at:"
# puts $h_file "//"
# puts $h_file "//   http://www.netfpga-cic.org"
# puts $h_file "//"
# puts $h_file "// Unless required by applicable law or agreed to in writing, Work distributed"
# puts $h_file "// under the License is distributed on an \"AS IS\" BASIS, WITHOUT WARRANTIES OR"
# puts $h_file "// CONDITIONS OF ANY KIND, either express or implied.  See the License for the"
# puts $h_file "// specific language governing permissions and limitations under the License."
# puts $h_file "//"
# puts $h_file "// @NETFPGA_LICENSE_HEADER_END@"
# puts $h_file "/////////////////////////////////////////////////////////////////////////////////"
# puts $h_file "// This is an automatically generated header definitions file"
# puts $h_file "/////////////////////////////////////////////////////////////////////////////////"
# puts $h_file ""
# 
# close $h_file 
# 
# };
# proc write_core {target_file prefix id has_registers lib_name} {
# 
# 
# set h_file [open $target_file "a"]
# 
# #First, read the memory map information from the reference_project defines file
# source $::env(NF_DESIGN_DIR)/hw/tcl/$::env(NF_PROJECT_NAME)_defines.tcl
# set public_repo_dir $::env(SUME_FOLDER)/lib/hw/
# 
# 
# set baseaddr [set $prefix\_BASEADDR]
# set highaddr [set $prefix\_HIGHADDR]
# set sizeaddr [set $prefix\_SIZEADDR]
# 
# puts $h_file "//######################################################"
# puts $h_file "//# Definitions for $prefix"
# puts $h_file "//######################################################"
# 
# puts $h_file "#define SUME_$prefix\_BASEADDR $baseaddr"
# puts $h_file "#define SUME_$prefix\_HIGHADDR $highaddr"
# puts $h_file "#define SUME_$prefix\_SIZEADDR $sizeaddr"
# puts $h_file ""
# 
# #Second, read the registers information from the library defines file
# if $has_registers {
# 	set lib_path "$public_repo_dir/std/cores/$lib_name"
# 	set regs_h_define_file $lib_path
# 	set regs_h_define_file_read [open $regs_h_define_file r]
# 	set regs_h_define_file_data [read $regs_h_define_file_read]
# 	close $regs_h_define_file_read
# 	set regs_h_define_file_data_line [split $regs_h_define_file_data "\n"]
# 
#        foreach read_line $regs_h_define_file_data_line {
#             if {[regexp "#define" $read_line]} {
#                 puts $h_file "#define SUME_[lindex $read_line 2]\_$id\_[lindex $read_line 3]\_[lindex $read_line 4] [lindex $read_line 5]"
#             }
# 	}
# }
# puts $h_file ""
# close $h_file 
# };
# write_header  $target_file 
# foreach lib_item $DEF_LIST { 
#      write_core  $target_file [lindex $lib_item 0] [lindex $lib_item 1] [lindex $lib_item 2] [lindex $lib_item 3] 
# }
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 19:41:20 2019...
cd ../sw/embedded/src  && cp /home/nico/projects/P4-NetFPGA/tools/scripts/xparam2regdefines.py . && python xparam2regdefines.py
cd ../sw/embedded/src  && rm -f xparam2regdefines.py && mv reg_defines.h ../
cd ../sw/embedded && cp /home/nico/projects/P4-NetFPGA/tools/scripts/python_parser.py . && python python_parser.py
cd ../sw/embedded && rm -f python_parser.py && mv reg_defines.py ../../test/reg_defines_simple_sume_switch.py 
make: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test'
make: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test'
rm -rf proj_* vivado*.* *.*~ .Xil* /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/ip_repo/ /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/
rm -rf *[0-9]_{stim,expected,log}.axi
rm -f *.axi
rm -f portconfig.sim
rm -f seed
rm -f *.log
rm -f ../test/Makefile
rm -rf ../test/*.log
rm -rf ../test/*.axi
rm -rf ../test/seed
rm -rf ../test/*.sim
rm -rf ../test/proj_*
rm -rf ../test/ip_repo
rm -f ../test/vivado*.*
rm -f ../test/*_*_*/reg_defines_simple_sume_switch.py
rm -f ../test/*_*_*/reg_defines_simple_sume_switch.pyc
rm -f ../hw/create_ip/id_rom16x32.coe
cp /home/nico/projects/P4-NetFPGA/tools/scripts/epoch.sh . && sh epoch.sh && rm -f epoch.sh
echo 16028002 >> rom_data.txt
echo `/home/nico/projects/P4-NetFPGA/run_tag.sh` >> rom_data.txt
grep: ../../../RELEASE_NOTES: No such file or directory
echo 00000204 >> rom_data.txt
echo 0000FFFF >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
cp /home/nico/projects/P4-NetFPGA/tools/scripts/format_coe.py . && python format_coe.py && rm -f format_coe.py 
16

mv -f id_rom16x32.coe ../hw/create_ip/
mv -f rom_data.txt ../hw/create_ip/
cp -f /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/reg_defines_simple_sume_switch.py /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/reg_defines_simple_sume_switch.py
vivado -mode batch -source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_sim.tcl -tclargs sim_switch_default

****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_sim.tcl
# set design $::env(NF_PROJECT_NAME)
# set top top_sim
# set sim_top top_tb
# set device  xc7vx690t-3-ffg1761
# set proj_dir ./project
# set public_repo_dir $::env(SUME_FOLDER)/lib/hw/
# set xilinx_repo_dir $::env(XILINX_VIVADO)/data/ip/xilinx/
# set repo_dir ./ip_repo
# set bit_settings $::env(CONSTRAINTS)/generic_bit.xdc 
# set project_constraints $::env(NF_DESIGN_DIR)/hw/constraints/nf_sume_general.xdc
# set nf_10g_constraints $::env(NF_DESIGN_DIR)/hw/constraints/nf_sume_10g.xdc
# set test_name [lindex $argv 0] 
# source $::env(NF_DESIGN_DIR)/hw/tcl/$::env(NF_PROJECT_NAME)_defines.tcl
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
# create_project -name ${design} -force -dir "$::env(NF_DESIGN_DIR)/hw/${proj_dir}" -part ${device}
# set_property source_mgmt_mode DisplayOnly [current_project]  
# set_property top ${top} [current_fileset]
# puts "Creating User Datapath reference project"
Creating User Datapath reference project
# create_fileset -constrset -quiet constraints
# file copy ${public_repo_dir}/ ${repo_dir}
# set_property ip_repo_paths ${repo_dir} [current_fileset]
# add_files -fileset constraints -norecurse ${bit_settings}
# add_files -fileset constraints -norecurse ${project_constraints}
# add_files -fileset constraints -norecurse ${nf_10g_constraints}
# set_property is_enabled true [get_files ${project_constraints}]
# set_property is_enabled true [get_files ${bit_settings}]
# set_property is_enabled true [get_files ${project_constraints}]
# update_ip_catalog
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/ip_repo'.
INFO: [IP_Flow 19-2313] Loaded Vivado IP repository '/opt/Xilinx/Vivado/2018.2/data/ip'.
# create_ip -name nf_sume_sdnet -vendor NetFPGA -library NetFPGA -module_name nf_sume_sdnet_ip
# set_property generate_synth_checkpoint false [get_files nf_sume_sdnet_ip.xci]
# reset_target all [get_ips nf_sume_sdnet_ip]
# generate_target all [get_ips nf_sume_sdnet_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'nf_sume_sdnet_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'nf_sume_sdnet_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'nf_sume_sdnet_ip'...
# create_ip -name input_arbiter -vendor NetFPGA -library NetFPGA -module_name input_arbiter_ip
# set_property -dict [list CONFIG.C_BASEADDR $INPUT_ARBITER_BASEADDR] [get_ips input_arbiter_ip]
# set_property generate_synth_checkpoint false [get_files input_arbiter_ip.xci]
# reset_target all [get_ips input_arbiter_ip]
# generate_target all [get_ips input_arbiter_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'input_arbiter_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'input_arbiter_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'input_arbiter_ip'...
# create_ip -name sss_output_queues -vendor NetFPGA -library NetFPGA -module_name sss_output_queues_ip
# set_property -dict [list CONFIG.C_BASEADDR $OUTPUT_QUEUES_BASEADDR] [get_ips sss_output_queues_ip]
# set_property generate_synth_checkpoint false [get_files sss_output_queues_ip.xci]
# reset_target all [get_ips sss_output_queues_ip]
# generate_target all [get_ips sss_output_queues_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'sss_output_queues_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'sss_output_queues_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'sss_output_queues_ip'...
# create_ip -name blk_mem_gen -vendor xilinx.com -library ip -version 8.4 -module_name identifier_ip
INFO: [Device 21-403] Loading part xc7vx690tffg1761-3
create_ip: Time (s): cpu = 00:00:22 ; elapsed = 00:00:59 . Memory (MB): peak = 1690.250 ; gain = 390.395 ; free physical = 10400 ; free virtual = 15395
# set_property -dict [list CONFIG.Interface_Type {AXI4} CONFIG.AXI_Type {AXI4_Lite} CONFIG.AXI_Slave_Type {Memory_Slave} CONFIG.Use_AXI_ID {false} CONFIG.Load_Init_File {true} CONFIG.Coe_File {/../../../../../../create_ip/id_rom16x32.coe} CONFIG.Fill_Remaining_Memory_Locations {true} CONFIG.Remaining_Memory_Locations {DEADDEAD} CONFIG.Memory_Type {Simple_Dual_Port_RAM} CONFIG.Use_Byte_Write_Enable {true} CONFIG.Byte_Size {8} CONFIG.Assume_Synchronous_Clk {true} CONFIG.Write_Width_A {32} CONFIG.Write_Depth_A {1024} CONFIG.Read_Width_A {32} CONFIG.Operating_Mode_A {READ_FIRST} CONFIG.Write_Width_B {32} CONFIG.Read_Width_B {32} CONFIG.Operating_Mode_B {READ_FIRST} CONFIG.Enable_B {Use_ENB_Pin} CONFIG.Register_PortA_Output_of_Memory_Primitives {false} CONFIG.Register_PortB_Output_of_Memory_Primitives {false} CONFIG.Use_RSTB_Pin {true} CONFIG.Reset_Type {ASYNC} CONFIG.Port_A_Write_Rate {50} CONFIG.Port_B_Clock {100} CONFIG.Port_B_Enable_Rate {100}] [get_ips identifier_ip]
# set_property generate_synth_checkpoint false [get_files identifier_ip.xci]
# reset_target all [get_ips identifier_ip]
# generate_target all [get_ips identifier_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Miscellaneous' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'identifier_ip'...
# create_ip -name clk_wiz -vendor xilinx.com -library ip -version 6.0 -module_name clk_wiz_ip
# set_property -dict [list CONFIG.PRIM_IN_FREQ {200.00} CONFIG.CLKOUT1_REQUESTED_OUT_FREQ {200.000} CONFIG.USE_SAFE_CLOCK_STARTUP {true} CONFIG.RESET_TYPE {ACTIVE_LOW} CONFIG.CLKIN1_JITTER_PS {50.0} CONFIG.CLKOUT1_DRIVES {BUFGCE} CONFIG.CLKOUT2_DRIVES {BUFGCE} CONFIG.CLKOUT3_DRIVES {BUFGCE} CONFIG.CLKOUT4_DRIVES {BUFGCE} CONFIG.CLKOUT5_DRIVES {BUFGCE} CONFIG.CLKOUT6_DRIVES {BUFGCE} CONFIG.CLKOUT7_DRIVES {BUFGCE} CONFIG.MMCM_CLKFBOUT_MULT_F {5.000} CONFIG.MMCM_CLKIN1_PERIOD {5.0} CONFIG.MMCM_CLKOUT0_DIVIDE_F {5.000} CONFIG.RESET_PORT {resetn} CONFIG.CLKOUT1_JITTER {98.146} CONFIG.CLKOUT1_PHASE_ERROR {89.971}] [get_ips clk_wiz_ip]
WARNING: [IP_Flow 19-3374] An attempt to modify the value of disabled parameter 'MMCM_CLKIN1_PERIOD' from '5.000' to '5.0' has been ignored for IP 'clk_wiz_ip'
# set_property generate_synth_checkpoint false [get_files clk_wiz_ip.xci]
# reset_target all [get_ips clk_wiz_ip]
# generate_target all [get_ips clk_wiz_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Implementation' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'clk_wiz_ip'...
# create_ip -name barrier -vendor NetFPGA -library NetFPGA -module_name barrier_ip
# reset_target all [get_ips barrier_ip]
# generate_target all [get_ips barrier_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'barrier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'barrier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'barrier_ip'...
# create_ip -name axis_sim_record -vendor NetFPGA -library NetFPGA -module_name axis_sim_record_ip0
# set_property -dict [list CONFIG.OUTPUT_FILE $::env(NF_DESIGN_DIR)/test/nf_interface_0_log.axi] [get_ips axis_sim_record_ip0]
# reset_target all [get_ips axis_sim_record_ip0]
# generate_target all [get_ips axis_sim_record_ip0]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_record_ip0'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_record_ip0'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_record_ip0'...
# create_ip -name axis_sim_record -vendor NetFPGA -library NetFPGA -module_name axis_sim_record_ip1
# set_property -dict [list CONFIG.OUTPUT_FILE $::env(NF_DESIGN_DIR)/test/nf_interface_1_log.axi] [get_ips axis_sim_record_ip1]
# reset_target all [get_ips axis_sim_record_ip1]
# generate_target all [get_ips axis_sim_record_ip1]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_record_ip1'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_record_ip1'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_record_ip1'...
# create_ip -name axis_sim_record -vendor NetFPGA -library NetFPGA -module_name axis_sim_record_ip2
# set_property -dict [list CONFIG.OUTPUT_FILE $::env(NF_DESIGN_DIR)/test/nf_interface_2_log.axi] [get_ips axis_sim_record_ip2]
# reset_target all [get_ips axis_sim_record_ip2]
# generate_target all [get_ips axis_sim_record_ip2]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_record_ip2'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_record_ip2'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_record_ip2'...
# create_ip -name axis_sim_record -vendor NetFPGA -library NetFPGA -module_name axis_sim_record_ip3
# set_property -dict [list CONFIG.OUTPUT_FILE $::env(NF_DESIGN_DIR)/test/nf_interface_3_log.axi] [get_ips axis_sim_record_ip3]
# reset_target all [get_ips axis_sim_record_ip3]
# generate_target all [get_ips axis_sim_record_ip3]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_record_ip3'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_record_ip3'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_record_ip3'...
# create_ip -name axis_sim_record -vendor NetFPGA -library NetFPGA -module_name axis_sim_record_ip4
# set_property -dict [list CONFIG.OUTPUT_FILE $::env(NF_DESIGN_DIR)/test/dma_0_log.axi] [get_ips axis_sim_record_ip4]
# reset_target all [get_ips axis_sim_record_ip4]
# generate_target all [get_ips axis_sim_record_ip4]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_record_ip4'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_record_ip4'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_record_ip4'...
# create_ip -name axis_sim_stim -vendor NetFPGA -library NetFPGA -module_name axis_sim_stim_ip0
# set_property -dict [list CONFIG.input_file $::env(NF_DESIGN_DIR)/test/nf_interface_0_stim.axi] [get_ips axis_sim_stim_ip0]
# generate_target all [get_ips axis_sim_stim_ip0]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_stim_ip0'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_stim_ip0'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_stim_ip0'...
# create_ip -name axis_sim_stim -vendor NetFPGA -library NetFPGA -module_name axis_sim_stim_ip1
# set_property -dict [list CONFIG.input_file $::env(NF_DESIGN_DIR)/test/nf_interface_1_stim.axi] [get_ips axis_sim_stim_ip1]
# generate_target all [get_ips axis_sim_stim_ip1]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_stim_ip1'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_stim_ip1'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_stim_ip1'...
# create_ip -name axis_sim_stim -vendor NetFPGA -library NetFPGA -module_name axis_sim_stim_ip2
# set_property -dict [list CONFIG.input_file $::env(NF_DESIGN_DIR)/test/nf_interface_2_stim.axi] [get_ips axis_sim_stim_ip2]
# generate_target all [get_ips axis_sim_stim_ip2]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_stim_ip2'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_stim_ip2'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_stim_ip2'...
# create_ip -name axis_sim_stim -vendor NetFPGA -library NetFPGA -module_name axis_sim_stim_ip3
# set_property -dict [list CONFIG.input_file $::env(NF_DESIGN_DIR)/test/nf_interface_3_stim.axi] [get_ips axis_sim_stim_ip3]
# generate_target all [get_ips axis_sim_stim_ip3]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_stim_ip3'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_stim_ip3'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_stim_ip3'...
# create_ip -name axis_sim_stim -vendor NetFPGA -library NetFPGA -module_name axis_sim_stim_ip4
# set_property -dict [list CONFIG.input_file $::env(NF_DESIGN_DIR)/test/dma_0_stim.axi] [get_ips axis_sim_stim_ip4]
# generate_target all [get_ips axis_sim_stim_ip4]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axis_sim_stim_ip4'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axis_sim_stim_ip4'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axis_sim_stim_ip4'...
# create_ip -name axi_sim_transactor -vendor NetFPGA -library NetFPGA -module_name axi_sim_transactor_ip
# set_property -dict [list CONFIG.STIM_FILE $::env(NF_DESIGN_DIR)/test/reg_stim.axi CONFIG.EXPECT_FILE $::env(NF_DESIGN_DIR)/test/reg_expect.axi CONFIG.LOG_FILE $::env(NF_DESIGN_DIR)/test/reg_stim.log] [get_ips axi_sim_transactor_ip]
# reset_target all [get_ips axi_sim_transactor_ip]
# generate_target all [get_ips axi_sim_transactor_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axi_sim_transactor_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axi_sim_transactor_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axi_sim_transactor_ip'...
# update_ip_catalog
# source $::env(NF_DESIGN_DIR)/hw/tcl/control_sub_sim.tcl
## set scripts_vivado_version 2018.2
## set current_vivado_version [version -short]
## if { [string first $scripts_vivado_version $current_vivado_version] == -1 } {
##    puts ""
##    puts "ERROR: This script was created for Vivado <$scripts_vivado_version> and is being run in <$current_vivado_version> of Vivado. Please run the script in Vivado <$scripts_vivado_version> then open the design in Vivado <$current_vivado_version>. Upgrade the design by running \"Tools => Report => Report IP Status...\", then run write_bd_tcl to create an updated script."
## 
##    return 1
## }
## set design_name control_sub
## if { [get_projects -quiet] eq "" } {
##    puts "ERROR: Please open or create a project!"
##    return 1
## }
## set errMsg ""
## set nRet 0
## set cur_design [current_bd_design -quiet]
## set list_cells [get_bd_cells -quiet]
## if { ${design_name} eq "" } {
##    # USE CASES:
##    #    1) Design_name not set
## 
##    set errMsg "ERROR: Please set the variable <design_name> to a non-empty value."
##    set nRet 1
## 
## } elseif { ${cur_design} ne "" && ${list_cells} eq "" } {
##    # USE CASES:
##    #    2): Current design opened AND is empty AND names same.
##    #    3): Current design opened AND is empty AND names diff; design_name NOT in project.
##    #    4): Current design opened AND is empty AND names diff; design_name exists in project.
## 
##    if { $cur_design ne $design_name } {
##       puts "INFO: Changing value of <design_name> from <$design_name> to <$cur_design> since current design is empty."
##       set design_name [get_property NAME $cur_design]
##    }
##    puts "INFO: Constructing design in IPI design <$cur_design>..."
## 
## } elseif { ${cur_design} ne "" && $list_cells ne "" && $cur_design eq $design_name } {
##    # USE CASES:
##    #    5) Current design opened AND has components AND same names.
## 
##    set errMsg "ERROR: Design <$design_name> already exists in your project, please set the variable <design_name> to another value."
##    set nRet 1
## } elseif { [get_files -quiet ${design_name}.bd] ne "" } {
##    # USE CASES: 
##    #    6) Current opened design, has components, but diff names, design_name exists in project.
##    #    7) No opened design, design_name exists in project.
## 
##    set errMsg "ERROR: Design <$design_name> already exists in your project, please set the variable <design_name> to another value."
##    set nRet 2
## 
## } else {
##    # USE CASES:
##    #    8) No opened design, design_name not in project.
##    #    9) Current opened design, has components, but diff names, design_name not in project.
## 
##    puts "INFO: Currently there is no design <$design_name> in project, so creating one..."
## 
##    create_bd_design $design_name
## 
##    puts "INFO: Making design <$design_name> as current_bd_design."
##    current_bd_design $design_name
## 
## }
INFO: Currently there is no design <control_sub> in project, so creating one...
Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd> 
INFO: Making design <control_sub> as current_bd_design.
## puts "INFO: Currently the variable <design_name> is equal to \"$design_name\"."
INFO: Currently the variable <design_name> is equal to "control_sub".
## if { $nRet != 0 } {
##    puts $errMsg
##    return $nRet
## }
## proc create_root_design { parentCell } {
## 
##   if { $parentCell eq "" } {
##      set parentCell [get_bd_cells /]
##   }
## 
##   # Get object for parentCell
##   set parentObj [get_bd_cells $parentCell]
##   if { $parentObj == "" } {
##      puts "ERROR: Unable to find parent cell <$parentCell>!"
##      return
##   }
## 
##   # Make sure parentObj is hier blk
##   set parentType [get_property TYPE $parentObj]
##   if { $parentType ne "hier" } {
##      puts "ERROR: Parent <$parentObj> has TYPE = <$parentType>. Expected to be <hier>."
##      return
##   }
## 
##   # Save current instance; Restore later
##   set oldCurInst [current_bd_instance .]
## 
##   # Set parent object as current
##   current_bd_instance $parentObj
## 
## 
##   # Create interface ports
##   set M00_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M00_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M00_AXI
##   set M01_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M01_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M01_AXI
##   set M02_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M02_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M02_AXI
##   set M03_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M03_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M03_AXI
##   set M04_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M04_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M04_AXI
##   set M05_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M05_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M05_AXI
##   set M06_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M06_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M06_AXI
##   set M07_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M07_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M07_AXI
##   set S00_AXI [ create_bd_intf_port -mode Slave -vlnv xilinx.com:interface:aximm_rtl:1.0 S00_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {32} CONFIG.ARUSER_WIDTH {0} CONFIG.AWUSER_WIDTH {0} CONFIG.BUSER_WIDTH {0} CONFIG.CLK_DOMAIN {} CONFIG.DATA_WIDTH {32} CONFIG.FREQ_HZ {100000000} CONFIG.ID_WIDTH {0} CONFIG.MAX_BURST_LENGTH {256} CONFIG.NUM_READ_OUTSTANDING {2} CONFIG.NUM_WRITE_OUTSTANDING {2} CONFIG.PHASE {0.000} CONFIG.PROTOCOL {AXI4} CONFIG.READ_WRITE_MODE {READ_WRITE} CONFIG.RUSER_WIDTH {0} CONFIG.SUPPORTS_NARROW_BURST {1} CONFIG.WUSER_WIDTH {0}  ] $S00_AXI
## 
##   # Create ports
##   set axi_lite_aclk [ create_bd_port -dir I -type clk axi_lite_aclk ]
##   set axi_lite_areset [ create_bd_port -dir I -type rst axi_lite_areset ]
##   set core_clk [ create_bd_port -dir I -type clk core_clk ]
##   set_property -dict [ list CONFIG.FREQ_HZ {200000000}  ] $core_clk
##   set core_resetn [ create_bd_port -dir I -type rst core_resetn ]
##   
##   
##     
## 
##   # Create instance: axi_interconnect_0, and set properties
##   set axi_interconnect_0 [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_interconnect:2.1 axi_interconnect_0 ]
##   set_property -dict [ list CONFIG.NUM_MI {8} CONFIG.TRANSLATION_MODE {0} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M00_HAS_REGSLICE {3} CONFIG.M00_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M01_HAS_REGSLICE {3} CONFIG.M01_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M02_HAS_REGSLICE {3} CONFIG.M02_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M03_HAS_REGSLICE {3} CONFIG.M03_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M04_HAS_REGSLICE {3} CONFIG.M04_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M05_HAS_REGSLICE {3} CONFIG.M05_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M06_HAS_REGSLICE {3} CONFIG.M06_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M07_HAS_REGSLICE {3} CONFIG.M07_HAS_DATA_FIFO {1} ] $axi_interconnect_0              
##   set_property -dict [list CONFIG.S00_HAS_REGSLICE {3} CONFIG.S00_HAS_DATA_FIFO {1} ] $axi_interconnect_0
## 
## 
## # Add AXI clock converter
## create_bd_cell -type ip -vlnv xilinx.com:ip:axi_clock_converter:2.1 axi_clock_converter_0
## connect_bd_intf_net [get_bd_intf_ports S00_AXI] [get_bd_intf_pins axi_clock_converter_0/S_AXI]
## connect_bd_intf_net [get_bd_intf_pins axi_clock_converter_0/M_AXI] -boundary_type upper [get_bd_intf_pins axi_interconnect_0/S00_AXI]
## 
##   # Create interface connections
##   connect_bd_intf_net -intf_net axi_interconnect_0_M00_AXI [get_bd_intf_ports M00_AXI] [get_bd_intf_pins axi_interconnect_0/M00_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M01_AXI [get_bd_intf_ports M01_AXI] [get_bd_intf_pins axi_interconnect_0/M01_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M02_AXI [get_bd_intf_ports M02_AXI] [get_bd_intf_pins axi_interconnect_0/M02_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M03_AXI [get_bd_intf_ports M03_AXI] [get_bd_intf_pins axi_interconnect_0/M03_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M04_AXI [get_bd_intf_ports M04_AXI] [get_bd_intf_pins axi_interconnect_0/M04_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M05_AXI [get_bd_intf_ports M05_AXI] [get_bd_intf_pins axi_interconnect_0/M05_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M06_AXI [get_bd_intf_ports M06_AXI] [get_bd_intf_pins axi_interconnect_0/M06_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M07_AXI [get_bd_intf_ports M07_AXI] [get_bd_intf_pins axi_interconnect_0/M07_AXI]
## 
##   # Create port connections
##   connect_bd_net -net axi_lite_aclk_1 [get_bd_ports axi_lite_aclk]  [get_bd_pins axi_clock_converter_0/s_axi_aclk] 
## connect_bd_net -net core_clk_1 [get_bd_ports core_clk]  [get_bd_pins axi_clock_converter_0/m_axi_aclk] [get_bd_pins axi_interconnect_0/ACLK] [get_bd_pins axi_interconnect_0/S00_ACLK] [get_bd_pins axi_interconnect_0/M00_ACLK] [get_bd_pins axi_interconnect_0/M01_ACLK] [get_bd_pins axi_interconnect_0/M02_ACLK] [get_bd_pins axi_interconnect_0/M03_ACLK] [get_bd_pins axi_interconnect_0/M04_ACLK] [get_bd_pins axi_interconnect_0/M05_ACLK] [get_bd_pins axi_interconnect_0/M06_ACLK] [get_bd_pins axi_interconnect_0/M07_ACLK] 
## connect_bd_net -net axi_lite_areset_1 [get_bd_ports axi_lite_areset] [get_bd_pins axi_clock_converter_0/s_axi_aresetn] 
## connect_bd_net -net core_resetn_1 [get_bd_ports core_resetn] [get_bd_pins axi_clock_converter_0/m_axi_aresetn] [get_bd_pins axi_interconnect_0/S00_ARESETN] [get_bd_pins axi_interconnect_0/M00_ARESETN] [get_bd_pins axi_interconnect_0/M01_ARESETN] [get_bd_pins axi_interconnect_0/ARESETN]  [get_bd_pins axi_interconnect_0/M02_ARESETN] [get_bd_pins axi_interconnect_0/M03_ARESETN] [get_bd_pins axi_interconnect_0/M04_ARESETN] [get_bd_pins axi_interconnect_0/M05_ARESETN] [get_bd_pins axi_interconnect_0/M06_ARESETN] [get_bd_pins axi_interconnect_0/M07_ARESETN] 
## 
##   # Create address segments
## source $::env(NF_DESIGN_DIR)/hw/tcl/$::env(NF_PROJECT_NAME)_defines.tcl
##   assign_bd_address [get_bd_addr_segs {M00_AXI/Reg }]  
##   set_property offset $M00_BASEADDR [get_bd_addr_segs {S00_AXI/SEG_M00_AXI_Reg}]
##   set_property range $M00_SIZEADDR [get_bd_addr_segs {S00_AXI/SEG_M00_AXI_Reg}] 
## 
##  assign_bd_address [get_bd_addr_segs {M01_AXI/Reg }]  
##   set_property offset $M01_BASEADDR [get_bd_addr_segs {S00_AXI/SEG_M01_AXI_Reg}]
##   set_property range $M01_SIZEADDR [get_bd_addr_segs {S00_AXI/SEG_M01_AXI_Reg}] 
## 
## 
## assign_bd_address [get_bd_addr_segs {M02_AXI/Reg }]  
##   set_property offset $M02_BASEADDR [get_bd_addr_segs {S00_AXI/SEG_M02_AXI_Reg}]
##   set_property range $M02_SIZEADDR [get_bd_addr_segs {S00_AXI/SEG_M02_AXI_Reg}] 
## 
## assign_bd_address [get_bd_addr_segs {M03_AXI/Reg }]  
##   set_property offset $M03_BASEADDR [get_bd_addr_segs {S00_AXI/SEG_M03_AXI_Reg}]
##   set_property range $M03_SIZEADDR [get_bd_addr_segs {S00_AXI/SEG_M03_AXI_Reg}] 
## 
##  
##   # Restore current instance
##   current_bd_instance $oldCurInst
## 
##   save_bd_design
## }
## create_root_design ""
CRITICAL WARNING: [BD 41-737] Cannot set the parameter TRANSLATION_MODE on /axi_interconnect_0. It is read-only.
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
</M00_AXI/Reg> is being mapped into </S00_AXI> at <0x44A00000 [ 64K ]>
</M01_AXI/Reg> is being mapped into </S00_AXI> at <0x44A00000 [ 64K ]>
</M02_AXI/Reg> is being mapped into </S00_AXI> at <0x44A00000 [ 64K ]>
</M03_AXI/Reg> is being mapped into </S00_AXI> at <0x44A00000 [ 64K ]>
Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd> 
# read_verilog "$::env(NF_DESIGN_DIR)/hw/hdl/axi_clocking.v"
# read_verilog "$::env(NF_DESIGN_DIR)/hw/hdl/nf_datapath.v"
# read_verilog "$::env(NF_DESIGN_DIR)/hw/hdl/top_sim.v"
# read_verilog "$::env(NF_DESIGN_DIR)/hw/hdl/top_tb.v"
# update_compile_order -fileset sources_1
# update_compile_order -fileset sim_1
# set_property top ${sim_top} [get_filesets sim_1]
# set_property include_dirs ${proj_dir} [get_filesets sim_1]
# set_property simulator_language Mixed [current_project]
# set_property verilog_define { {SIMULATION=1} } [get_filesets sim_1]
# set_property -name xsim.more_options -value {-testplusarg TESTNAME=basic_test} -objects [get_filesets sim_1]
# set_property runtime {} [get_filesets sim_1]
# set_property target_simulator xsim [current_project]
# set_property compxlib.xsim_compiled_library_dir {} [current_project]
# set_property top_lib xil_defaultlib [get_filesets sim_1]
# update_compile_order -fileset sim_1
update_compile_order: Time (s): cpu = 00:00:21 ; elapsed = 00:00:11 . Memory (MB): peak = 2021.406 ; gain = 0.012 ; free physical = 10266 ; free virtual = 15281
# set output [exec python $::env(NF_DESIGN_DIR)/test/${test_name}/run.py]
# puts $output
loading libsume..
About to start the test
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata/nf1_expected.pcap  not found
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata/nf2_expected.pcap  not found
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/testdata/nf3_expected.pcap  not found
scheduling pkts ...
done scheduling pkts ...
scheduling pkts ...
done scheduling pkts ...
scheduling pkts ...
done scheduling pkts ...
scheduling pkts ...
done scheduling pkts ...
sending pkts ...
starting barrier ...
starting nftest_finish ...
complete !!
# set_property xsim.view {} [get_filesets sim_1]
# launch_simulation -simset sim_1 -mode behavioral
INFO: [Vivado 12-5698] Checking validity of IPs in the design for the 'XSim' simulator...
CRITICAL WARNING: [BD 41-1356] Address block </M04_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M05_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M06_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M07_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M04_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M05_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M06_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
CRITICAL WARNING: [BD 41-1356] Address block </M07_AXI/Reg> is not mapped into </S00_AXI>. Please use Address Editor to either map or exclude it.
Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd> 
VHDL Output written to : /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/synth/control_sub.v
VHDL Output written to : /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/sim/control_sub.v
VHDL Output written to : /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/hdl/control_sub_wrapper.v
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_clock_converter_0 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/xbar .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/s00_mmu .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m07_couplers/m07_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m06_couplers/m06_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m05_couplers/m05_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m04_couplers/m04_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m03_couplers/m03_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m02_couplers/m02_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m01_couplers/m01_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/m00_couplers/m00_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/s00_couplers/s00_data_fifo .
INFO: [BD 41-1029] Generation completed for the IP Integrator block axi_interconnect_0/s00_couplers/auto_pc .
Exporting to file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/hw_handoff/control_sub.hwh
Generated Block Design Tcl file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/hw_handoff/control_sub_bd.tcl
Generated Hardware Definition File /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/synth/control_sub.hwdef
INFO: [Vivado 12-5682] Launching behavioral simulation in '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim'
INFO: [Vivado 12-4795] Using compiled simulation libraries for IPs
INFO: [SIM-utils-51] Simulation object is 'sim_1'
INFO: [USF-XSim-7] Finding pre-compiled libraries...
INFO: [USF-XSim-11] File '/opt/Xilinx/Vivado/2018.2/data/xsim/xsim.ini' copied to run dir:'/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim'
INFO: [SIM-utils-54] Inspecting design source files for 'top_tb' in fileset 'sim_1'...
INFO: [SIM-utils-43] Exported '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim/id_rom16x32.coe'
INFO: [SIM-utils-43] Exported '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim/identifier_ip.mif'
INFO: [USF-XSim-97] Finding global include files...
INFO: [USF-XSim-100] Fetching design files from 'sources_1'...(this may take a while)...
INFO: [USF-XSim-101] Fetching design files from 'sim_1'...
INFO: [USF-XSim-2] XSim::Compile design
INFO: [USF-XSim-61] Executing 'COMPILE and ANALYZE' step in '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim'
xvlog --incr --relax -prj top_tb_vlog.prj
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/barrier_ip/hdl/barrier.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module barrier
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/barrier_ip/sim/barrier_ip.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module barrier_ip
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v" into library fifo_generator_v13_2_2
INFO: [VRFC 10-311] analyzing module fifo_generator_vlog_beh
INFO: [VRFC 10-2458] undeclared symbol wr_rst_busy_i, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:1249]
INFO: [VRFC 10-2458] undeclared symbol wr_eop_ad, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:1331]
INFO: [VRFC 10-2458] undeclared symbol rd_eop_ad, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:1332]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_axis, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:1574]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_wach, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:2099]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_wdch, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:2319]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_wrch, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:2486]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_rach, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:2866]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_rdch, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:3099]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_CONV_VER
INFO: [VRFC 10-2458] undeclared symbol safety_ckt_rd_rst, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:4153]
INFO: [VRFC 10-2458] undeclared symbol safety_ckt_rd_rst, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:4361]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_sync_stage
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_bhv_ver_as
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_beh_ver_ll_afifo
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_bhv_ver_ss
INFO: [VRFC 10-2458] undeclared symbol srst_wrst_busy, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/simulation/fifo_generator_vlog_beh.v:7793]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_bhv_ver_preload0
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_axic_reg_slice
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/hdl/fifo_generator_v13_2_rfs.v" into library fifo_generator_v13_2_2
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2
INFO: [VRFC 10-2458] undeclared symbol sleep_i, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/hdl/fifo_generator_v13_2_rfs.v:519]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_axi_clock_converter_0_0/sim/control_sub_axi_clock_converter_0_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_axi_clock_converter_0_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_xbar_0/sim/control_sub_xbar_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_xbar_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_s00_mmu_0/sim/control_sub_s00_mmu_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_s00_mmu_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m07_data_fifo_0/sim/control_sub_m07_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m07_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m06_data_fifo_0/sim/control_sub_m06_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m06_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m05_data_fifo_0/sim/control_sub_m05_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m05_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m04_data_fifo_0/sim/control_sub_m04_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m04_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m03_data_fifo_0/sim/control_sub_m03_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m03_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m02_data_fifo_0/sim/control_sub_m02_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m02_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m01_data_fifo_0/sim/control_sub_m01_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m01_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_m00_data_fifo_0/sim/control_sub_m00_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_m00_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_s00_data_fifo_0/sim/control_sub_s00_data_fifo_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_s00_data_fifo_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/ip/control_sub_auto_pc_0/sim/control_sub_auto_pc_0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub_auto_pc_0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/bd/control_sub/sim/control_sub.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module control_sub
INFO: [VRFC 10-311] analyzing module control_sub_axi_interconnect_0_0
INFO: [VRFC 10-311] analyzing module m00_couplers_imp_35MSE9
INFO: [VRFC 10-311] analyzing module m01_couplers_imp_159MA5B
INFO: [VRFC 10-311] analyzing module m02_couplers_imp_1UHPQGS
INFO: [VRFC 10-311] analyzing module m03_couplers_imp_V7OM1U
INFO: [VRFC 10-311] analyzing module m04_couplers_imp_73P722
INFO: [VRFC 10-311] analyzing module m05_couplers_imp_1194TWK
INFO: [VRFC 10-311] analyzing module m06_couplers_imp_1YASCCN
INFO: [VRFC 10-311] analyzing module m07_couplers_imp_RC6YHL
INFO: [VRFC 10-311] analyzing module s00_couplers_imp_1S77UJ5
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip4/hdl/axis_sim_record.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record
WARNING: [VRFC 10-756] identifier state is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip4/hdl/axis_sim_record.v:93]
WARNING: [VRFC 10-756] identifier ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip4/hdl/axis_sim_record.v:94]
WARNING: [VRFC 10-756] identifier not_ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip4/hdl/axis_sim_record.v:95]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip4/sim/axis_sim_record_ip4.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record_ip4
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip3/hdl/axis_sim_record.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record
WARNING: [VRFC 10-756] identifier state is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip3/hdl/axis_sim_record.v:93]
WARNING: [VRFC 10-756] identifier ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip3/hdl/axis_sim_record.v:94]
WARNING: [VRFC 10-756] identifier not_ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip3/hdl/axis_sim_record.v:95]
WARNING: [VRFC 10-2845] overwriting previous definition of module axis_sim_record [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip3/hdl/axis_sim_record.v:59]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip3/sim/axis_sim_record_ip3.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record_ip3
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip2/hdl/axis_sim_record.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record
WARNING: [VRFC 10-756] identifier state is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip2/hdl/axis_sim_record.v:93]
WARNING: [VRFC 10-756] identifier ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip2/hdl/axis_sim_record.v:94]
WARNING: [VRFC 10-756] identifier not_ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip2/hdl/axis_sim_record.v:95]
WARNING: [VRFC 10-2845] overwriting previous definition of module axis_sim_record [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip2/hdl/axis_sim_record.v:59]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip2/sim/axis_sim_record_ip2.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record_ip2
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip1/hdl/axis_sim_record.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record
WARNING: [VRFC 10-756] identifier state is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip1/hdl/axis_sim_record.v:93]
WARNING: [VRFC 10-756] identifier ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip1/hdl/axis_sim_record.v:94]
WARNING: [VRFC 10-756] identifier not_ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip1/hdl/axis_sim_record.v:95]
WARNING: [VRFC 10-2845] overwriting previous definition of module axis_sim_record [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip1/hdl/axis_sim_record.v:59]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip1/sim/axis_sim_record_ip1.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record_ip1
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip0/hdl/axis_sim_record.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record
WARNING: [VRFC 10-756] identifier state is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip0/hdl/axis_sim_record.v:93]
WARNING: [VRFC 10-756] identifier ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip0/hdl/axis_sim_record.v:94]
WARNING: [VRFC 10-756] identifier not_ready_count is used before its declaration [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip0/hdl/axis_sim_record.v:95]
WARNING: [VRFC 10-2845] overwriting previous definition of module axis_sim_record [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip0/hdl/axis_sim_record.v:59]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_record_ip0/sim/axis_sim_record_ip0.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axis_sim_record_ip0
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/identifier_ip/sim/identifier_ip.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module identifier_ip
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_small_fifo.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module sss_small_fifo
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_fallthrough_small_fifo.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module sss_fallthrough_small_fifo
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/small_fifo.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module small_fifo
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/fallthrough_small_fifo.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module fallthrough_small_fifo
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_output_queues_cpu_regs.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module sss_output_queues_cpu_regs
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_output_queues.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module sss_output_queues
INFO: [VRFC 10-2458] undeclared symbol resetn_sync, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_output_queues.v:754]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/sim/sss_output_queues_ip.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module sss_output_queues_ip
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/axis_infrastructure_v1_1_0/hdl/axis_infrastructure_v1_1_vl_rfs.v" into library axis_infrastructure_v1_1_0
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_mux_enc
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_util_aclken_converter
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_util_aclken_converter_wrapper
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_util_axis2vector
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_util_vector2axis
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_clock_synchronizer
INFO: [VRFC 10-311] analyzing module axis_infrastructure_v1_1_0_cdc_handshake
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v" into library fifo_generator_v13_2_2
INFO: [VRFC 10-311] analyzing module fifo_generator_vlog_beh
INFO: [VRFC 10-2458] undeclared symbol wr_rst_busy_i, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:1249]
INFO: [VRFC 10-2458] undeclared symbol wr_eop_ad, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:1331]
INFO: [VRFC 10-2458] undeclared symbol rd_eop_ad, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:1332]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_axis, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:1574]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_wach, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:2099]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_wdch, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:2319]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_wrch, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:2486]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_rach, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:2866]
INFO: [VRFC 10-2458] undeclared symbol rd_rst_busy_rdch, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:3099]
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_vlog_beh [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:98]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_CONV_VER
INFO: [VRFC 10-2458] undeclared symbol safety_ckt_rd_rst, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:4153]
INFO: [VRFC 10-2458] undeclared symbol safety_ckt_rd_rst, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:4361]
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_CONV_VER [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:3366]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_sync_stage
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_sync_stage [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:4938]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_bhv_ver_as
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_bhv_ver_as [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:4959]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_beh_ver_ll_afifo
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_beh_ver_ll_afifo [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:6937]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_bhv_ver_ss
INFO: [VRFC 10-2458] undeclared symbol srst_wrst_busy, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:7793]
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_bhv_ver_ss [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:7065]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_bhv_ver_preload0
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_bhv_ver_preload0 [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:9206]
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2_axic_reg_slice
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2_axic_reg_slice [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/simulation/fifo_generator_vlog_beh.v:10324]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/hdl/fifo_generator_v13_2_rfs.v" into library fifo_generator_v13_2_2
INFO: [VRFC 10-311] analyzing module fifo_generator_v13_2_2
INFO: [VRFC 10-2458] undeclared symbol sleep_i, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/hdl/fifo_generator_v13_2_rfs.v:519]
WARNING: [VRFC 10-2845] overwriting previous definition of module fifo_generator_v13_2_2 [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/hdl/fifo_generator_v13_2_rfs.v:74]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/axis_data_fifo_v1_1_18/hdl/axis_data_fifo_v1_1_vl_rfs.v" into library axis_data_fifo_v1_1_18
INFO: [VRFC 10-311] analyzing module axis_data_fifo_v1_1_18_axis_data_fifo
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_CONTROLLERs.HDL/S_CONTROLLER_SimpleSumeSwitch.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_CONTROLLER_SimpleSumeSwitch
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_PROTOCOL_ADAPTER_EGRESS
WARNING: [VRFC 10-2654] begin/end is required for generate-for in this mode of verilog [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v:111]
WARNING: [VRFC 10-2654] begin/end is required for generate-for in this mode of verilog [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v:110]
WARNING: [VRFC 10-2654] begin/end is required for generate-for in this mode of verilog [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v:112]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_PROTOCOL_ADAPTER_INGRESS
WARNING: [VRFC 10-2654] begin/end is required for generate-for in this mode of verilog [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:218]
WARNING: [VRFC 10-2654] begin/end is required for generate-for in this mode of verilog [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:217]
WARNING: [VRFC 10-2654] begin/end is required for generate-for in this mode of verilog [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:219]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_control.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_RESETTER_control
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_line.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_RESETTER_line
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_lookup.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_RESETTER_lookup
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_S_SYNCER_for_TopDeparser
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopDeparser.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_TopDeparser
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_SYNCER_for_TopParser
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for__OUT_.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module S_SYNCER_for__OUT_
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module SimpleSumeSwitch
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopDeparser_t.HDL/TopDeparser_t.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopDeparser_t
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopDeparser_t.HDL/TopDeparser_t.vp" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopDeparser_t_Engine
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec_compute_control_remove
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_extract_headers_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_0_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_1
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_1_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_act_sec
INFO: [VRFC 10-311] analyzing module TopDeparser_t_act_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_act_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute__STRUCT_dst_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute__STRUCT_src_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute__STRUCT_ethertype
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_10_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_2_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_task
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_ingress_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_ethertype
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute__STRUCT_table_id
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_9_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_3_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_version
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_ihl
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_diff_serv
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_ecn
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_totalLen
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_identification
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_flags
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_fragOffset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_ttl
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_protocol
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_hdrChecksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_src_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute__STRUCT_dst_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_8_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_4_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_version
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_traffic_class
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_flow_label
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_payload_length
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_next_header
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_hop_limit
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_src_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute__STRUCT_dst_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_7_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_5_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_hw_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_protocol
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_hw_size
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_protocol_size
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_opcode
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_src_mac_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_src_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_dst_mac_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute__STRUCT_dst_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_6_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_6_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_src_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_dst_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_seqNo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_ackNo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_data_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_res
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_cwr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_ece
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_urg
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_ack
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_psh
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_rst
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_syn
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_fin
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_window
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute__STRUCT_urgentPtr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_5_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_7_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_src_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_dst_port
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_payload_length
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_4_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_8_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute__STRUCT_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute__STRUCT_code
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_3_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_9_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute__STRUCT_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute__STRUCT_code
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute__STRUCT_checksum
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_2_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_10_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_router
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_solicitated
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_override
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_reserved
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute__STRUCT_target_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_1_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_11_Editor_DataMux
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute_control_insert
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute__STRUCT_type
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute__STRUCT_ll_length
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute__STRUCT_mac_addr
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopDeparser_t_emit_0_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_FifoWriter
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DscFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DscFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_LatencyBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_PktFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_PktFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleFifo
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleFifo_RAM
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_FifoReader
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataShift_UniShifterSelect
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataBuffer
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataBuffer_BarrelShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataBuffer_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleMerge
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleMerge_UniShifterDownMask
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleMerge_UniShifterDownTuple
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_UniShifterDown
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_UniShifterUp
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_BidirShifterUpdate
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_TupleShift_BidirShifterUpdate_UniShifter2X
INFO: [VRFC 10-311] analyzing module TopDeparser_t_EngineStage_12_Editor_DataMux
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopParser_t.HDL/TopParser_t.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopParser_t
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopParser_t.HDL/TopParser_t.vp" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopParser_t_Engine
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_start
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_icmp
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_icmp6
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_icmp6_na_ns
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_ipv4
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_udp_v6
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_udp_v4
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_tcp_v6
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_chk_tcp_v4
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_v4sum
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_v6sum
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_meta_headerdiff
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_dst_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_src_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_hdr_ethernet_ethertype
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_start_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_reject
INFO: [VRFC 10-311] analyzing module TopParser_t_reject_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_reject_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_0_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_version
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_ihl
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_diff_serv
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_ecn
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_totalLen
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_identification
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_flags
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_fragOffset
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_ttl
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_protocol
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_hdrChecksum
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_src_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_hdr_ipv4_dst_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_meta_length_without_ip_header
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv4_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_version
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_traffic_class
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_flow_label
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_payload_length
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_next_header
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_hop_limit
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_src_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_hdr_ipv6_dst_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_meta_length_without_ip_header
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_ipv6_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_arp
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_hw_type
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_protocol
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_hw_size
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_protocol_size
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_opcode
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_src_mac_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_src_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_dst_mac_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_hdr_arp_dst_ipv4_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_arp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_1_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_type
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_code
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_hdr_icmp6_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_src_port
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_dst_port
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_seqNo
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_ackNo
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_data_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_res
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_cwr
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_ece
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_urg
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_ack
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_psh
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_rst
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_syn
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_fin
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_window
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_hdr_tcp_urgentPtr
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_tcp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_udp
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_src_port
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_dst_port
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_payload_length
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_hdr_udp_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_udp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_type
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_code
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_hdr_icmp_checksum
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_2_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3_ExtractShifter
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_router
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_solicitated
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_override
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_reserved
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_na_ns_target_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_isValid
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_type
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_ll_length
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_hdr_icmp6_option_link_layer_addr_mac_addr
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_TopParser_extracts_size
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_icmp6_neighbor_solicitation_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_3_TupleForward
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_4
INFO: [VRFC 10-311] analyzing module TopParser_t_EngineStage_4_ErrorCheck
INFO: [VRFC 10-311] analyzing module TopParser_t_accept
INFO: [VRFC 10-311] analyzing module TopParser_t_accept_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopParser_t_accept_compute_control_increment_offset
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_0_t.HDL/TopPipe_lvl_0_t.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_0_t.HDL/TopPipe_lvl_0_t.vp" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_Engine
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_dummy_table_for_netpfga_sec
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_dummy_table_for_netpfga_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_dummy_table_for_netpfga_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_EngineStage_1
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_do_nothing_0_sec
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_do_nothing_0_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_do_nothing_0_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec_compute_sume_metadata_dst_port
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_send_to_port1_0_sec_compute_control_increment_offset
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_EngineStage_2
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_sink
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_sink_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_0_t_sink_compute_control_increment_offset
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_t.HDL/TopPipe_lvl_t.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_t.HDL/TopPipe_lvl_t.vp" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_Engine
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_EngineStage_0
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup_compute_dummy_table_for_netpfga_req_lookup_request_key
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup_compute_control_nextSection
INFO: [VRFC 10-311] analyzing module TopPipe_lvl_t_setup_compute_control_increment_offset
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/dummy_table_for_netpfga_t.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/dummy_table_for_netpfga_t.vp" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Wrap
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_IntTop
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Lookup
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Hash_Lookup
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_RamR1RW1
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Cam
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Update
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Hash_Update
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod4
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod4_Rnd
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod5
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_Randmod5_Rnd
INFO: [VRFC 10-311] analyzing module dummy_table_for_netpfga_t_csr
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/sume_to_sdnet.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module sume_to_sdnet
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_cdc.sv" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module xpm_cdc_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_gray
INFO: [VRFC 10-311] analyzing module xpm_cdc_handshake
INFO: [VRFC 10-311] analyzing module xpm_cdc_pulse
INFO: [VRFC 10-311] analyzing module xpm_cdc_array_single
INFO: [VRFC 10-311] analyzing module xpm_cdc_sync_rst
INFO: [VRFC 10-311] analyzing module xpm_cdc_async_rst
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/xpm_fifo.sv" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module xpm_fifo_base
INFO: [VRFC 10-311] analyzing module xpm_fifo_rst
INFO: [VRFC 10-311] analyzing module xpm_counter_updn
INFO: [VRFC 10-311] analyzing module xpm_fifo_reg_vec
INFO: [VRFC 10-311] analyzing module xpm_fifo_reg_bit
INFO: [VRFC 10-311] analyzing module xpm_reg_pipe_bit
INFO: [VRFC 10-311] analyzing module xpm_fifo_sync
INFO: [VRFC 10-311] analyzing module xpm_fifo_async
INFO: [VRFC 10-311] analyzing module xpm_fifo_axis
INFO: [VRFC 10-2263] Analyzing SystemVerilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/xpm_memory.sv" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module xpm_memory_base
INFO: [VRFC 10-311] analyzing module asym_bwe_bb
INFO: [VRFC 10-311] analyzing module xpm_memory_dpdistram
INFO: [VRFC 10-311] analyzing module xpm_memory_dprom
INFO: [VRFC 10-311] analyzing module xpm_memory_sdpram
INFO: [VRFC 10-311] analyzing module xpm_memory_spram
INFO: [VRFC 10-311] analyzing module xpm_memory_sprom
INFO: [VRFC 10-311] analyzing module xpm_memory_tdpram
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module nf_sume_sdnet
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/sim/nf_sume_sdnet_ip.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module nf_sume_sdnet_ip
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/small_fifo.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module small_fifo
WARNING: [VRFC 10-2845] overwriting previous definition of module small_fifo [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/small_fifo.v:44]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/fallthrough_small_fifo.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module fallthrough_small_fifo
WARNING: [VRFC 10-2845] overwriting previous definition of module fallthrough_small_fifo [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/fallthrough_small_fifo.v:46]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter_cpu_regs.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module input_arbiter_cpu_regs
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module input_arbiter
INFO: [VRFC 10-2458] undeclared symbol resetn_sync, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter.v:390]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/sim/input_arbiter_ip.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module input_arbiter_ip
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip_clk_wiz.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module clk_wiz_ip_clk_wiz
INFO: [VRFC 10-2458] undeclared symbol clk_out1_clk_wiz_ip_en_clk, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip_clk_wiz.v:207]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module clk_wiz_ip
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/axi_clocking.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module axi_clocking
INFO: [VRFC 10-2458] undeclared symbol clkin1, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/axi_clocking.v:64]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module nf_datapath
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_sim.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module top_sim
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module top_tb
INFO: [VRFC 10-2458] undeclared symbol pcie_7x_mgt_rxn, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:115]
INFO: [VRFC 10-2458] undeclared symbol pcie_7x_mgt_rxp, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:116]
INFO: [VRFC 10-2458] undeclared symbol pcie_7x_mgt_txn, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:117]
INFO: [VRFC 10-2458] undeclared symbol pcie_7x_mgt_txp, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:118]
INFO: [VRFC 10-2458] undeclared symbol rxp, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:121]
INFO: [VRFC 10-2458] undeclared symbol rxn, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:122]
INFO: [VRFC 10-2458] undeclared symbol txp, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:123]
INFO: [VRFC 10-2458] undeclared symbol txn, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:124]
INFO: [VRFC 10-2458] undeclared symbol i2c_clk, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:137]
INFO: [VRFC 10-2458] undeclared symbol i2c_data, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:138]
INFO: [VRFC 10-2458] undeclared symbol si5324_rst_n, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:139]
INFO: [VRFC 10-2458] undeclared symbol led_0, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:146]
INFO: [VRFC 10-2458] undeclared symbol led_1, assumed default net type wire [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top_tb.v:147]
INFO: [VRFC 10-2263] Analyzing Verilog file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim/glbl.v" into library xil_defaultlib
INFO: [VRFC 10-311] analyzing module glbl
xvhdl --incr --relax -prj top_tb_vhdl.prj
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/lib_pkg_v1_0_2/hdl/lib_pkg_v1_0_rfs.vhd" into library lib_pkg_v1_0_2
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/lib_srl_fifo_v1_0_2/hdl/lib_srl_fifo_v1_0_rfs.vhd" into library lib_srl_fifo_v1_0_2
INFO: [VRFC 10-307] analyzing entity cntr_incr_decr_addn_f
INFO: [VRFC 10-307] analyzing entity dynshreg_f
INFO: [VRFC 10-307] analyzing entity srl_fifo_rbu_f
INFO: [VRFC 10-307] analyzing entity srl_fifo_f
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_sim_transactor_ip/hdl/axis_sim_pkg/axis_sim_pkg.vhd" into library xil_defaultlib
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_sim_transactor_ip/hdl/transactor_fifos.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity transactor_fifos
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_sim_transactor_ip/hdl/axi_sim_transactor.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axi_sim_transactor
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_sim_transactor_ip/sim/axi_sim_transactor_ip.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axi_sim_transactor_ip
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ipshared/7aff/hdl/fifo_generator_v13_2_rfs.vhd" into library fifo_generator_v13_2_2
INFO: [VRFC 10-307] analyzing entity input_blk
INFO: [VRFC 10-307] analyzing entity output_blk
INFO: [VRFC 10-307] analyzing entity shft_wrapper
INFO: [VRFC 10-307] analyzing entity shft_ram
INFO: [VRFC 10-307] analyzing entity wr_pf_as
INFO: [VRFC 10-307] analyzing entity wr_pf_ss
INFO: [VRFC 10-307] analyzing entity rd_pe_as
INFO: [VRFC 10-307] analyzing entity rd_pe_ss
INFO: [VRFC 10-307] analyzing entity synchronizer_ff
INFO: [VRFC 10-307] analyzing entity delay
INFO: [VRFC 10-307] analyzing entity bin_cntr
INFO: [VRFC 10-307] analyzing entity clk_x_pntrs_builtin
INFO: [VRFC 10-307] analyzing entity logic_builtin
INFO: [VRFC 10-307] analyzing entity builtin_prim
INFO: [VRFC 10-307] analyzing entity builtin_extdepth
INFO: [VRFC 10-307] analyzing entity builtin_top
INFO: [VRFC 10-307] analyzing entity reset_builtin
INFO: [VRFC 10-307] analyzing entity builtin_prim_v6
INFO: [VRFC 10-307] analyzing entity builtin_extdepth_v6
INFO: [VRFC 10-307] analyzing entity builtin_extdepth_low_latency
INFO: [VRFC 10-307] analyzing entity builtin_top_v6
INFO: [VRFC 10-307] analyzing entity fifo_generator_v13_2_2_builtin
INFO: [VRFC 10-307] analyzing entity bram_sync_reg
INFO: [VRFC 10-307] analyzing entity bram_fifo_rstlogic
INFO: [VRFC 10-307] analyzing entity reset_blk_ramfifo
INFO: [VRFC 10-307] analyzing entity axi_reg_slice
INFO: [VRFC 10-307] analyzing entity fifo_generator_top
INFO: [VRFC 10-307] analyzing entity fifo_generator_v13_2_2_synth
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip4/hdl/axis_sim_pkg/axis_sim_pkg.vhd" into library xil_defaultlib
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip4/hdl/axis_sim_stim.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip4/sim/axis_sim_stim_ip4.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim_ip4
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip3/hdl/axis_sim_pkg/axis_sim_pkg.vhd" into library xil_defaultlib
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip3/hdl/axis_sim_stim.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip3/sim/axis_sim_stim_ip3.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim_ip3
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip2/hdl/axis_sim_pkg/axis_sim_pkg.vhd" into library xil_defaultlib
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip2/hdl/axis_sim_stim.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip2/sim/axis_sim_stim_ip2.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim_ip2
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip1/hdl/axis_sim_pkg/axis_sim_pkg.vhd" into library xil_defaultlib
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip1/hdl/axis_sim_stim.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip1/sim/axis_sim_stim_ip1.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim_ip1
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip0/hdl/axis_sim_pkg/axis_sim_pkg.vhd" into library xil_defaultlib
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip0/hdl/axis_sim_stim.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axis_sim_stim_ip0/sim/axis_sim_stim_ip0.vhd" into library xil_defaultlib
INFO: [VRFC 10-307] analyzing entity axis_sim_stim_ip0
INFO: [VRFC 10-163] Analyzing VHDL file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.ip_user_files/ipstatic/fifo_generator_v13_2_2/hdl/fifo_generator_v13_2_rfs.vhd" into library fifo_generator_v13_2_2
INFO: [VRFC 10-307] analyzing entity input_blk
INFO: [VRFC 10-307] analyzing entity output_blk
INFO: [VRFC 10-307] analyzing entity shft_wrapper
INFO: [VRFC 10-307] analyzing entity shft_ram
INFO: [VRFC 10-307] analyzing entity wr_pf_as
INFO: [VRFC 10-307] analyzing entity wr_pf_ss
INFO: [VRFC 10-307] analyzing entity rd_pe_as
INFO: [VRFC 10-307] analyzing entity rd_pe_ss
INFO: [VRFC 10-307] analyzing entity synchronizer_ff
INFO: [VRFC 10-307] analyzing entity delay
INFO: [VRFC 10-307] analyzing entity bin_cntr
INFO: [VRFC 10-307] analyzing entity clk_x_pntrs_builtin
INFO: [VRFC 10-307] analyzing entity logic_builtin
INFO: [VRFC 10-307] analyzing entity builtin_prim
INFO: [VRFC 10-307] analyzing entity builtin_extdepth
INFO: [VRFC 10-307] analyzing entity builtin_top
INFO: [VRFC 10-307] analyzing entity reset_builtin
INFO: [VRFC 10-307] analyzing entity builtin_prim_v6
INFO: [VRFC 10-307] analyzing entity builtin_extdepth_v6
INFO: [VRFC 10-307] analyzing entity builtin_extdepth_low_latency
INFO: [VRFC 10-307] analyzing entity builtin_top_v6
INFO: [VRFC 10-307] analyzing entity fifo_generator_v13_2_2_builtin
INFO: [VRFC 10-307] analyzing entity bram_sync_reg
INFO: [VRFC 10-307] analyzing entity bram_fifo_rstlogic
INFO: [VRFC 10-307] analyzing entity reset_blk_ramfifo
INFO: [VRFC 10-307] analyzing entity axi_reg_slice
INFO: [VRFC 10-307] analyzing entity fifo_generator_top
INFO: [VRFC 10-307] analyzing entity fifo_generator_v13_2_2_synth
run_program: Time (s): cpu = 00:00:04 ; elapsed = 00:00:07 . Memory (MB): peak = 2136.641 ; gain = 0.000 ; free physical = 10172 ; free virtual = 15212
INFO: [USF-XSim-69] 'compile' step finished in '6' seconds
INFO: [USF-XSim-3] XSim::Elaborate design
INFO: [USF-XSim-61] Executing 'ELABORATE' step in '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim'
Vivado Simulator 2018.2
Copyright 1986-1999, 2001-2018 Xilinx, Inc. All Rights Reserved.
Running: /opt/Xilinx/Vivado/2018.2/bin/unwrapped/lnx64.o/xelab -wto 052c3aaad82142c3bb9ab669730da72f --incr --debug typical --relax --mt 8 -d SIMULATION=1 -L xil_defaultlib -L lib_pkg_v1_0_2 -L lib_srl_fifo_v1_0_2 -L axi_infrastructure_v1_1_0 -L fifo_generator_v13_2_2 -L axi_clock_converter_v2_1_16 -L generic_baseblocks_v2_1_0 -L axi_register_slice_v2_1_17 -L axi_data_fifo_v2_1_16 -L axi_crossbar_v2_1_18 -L axi_mmu_v2_1_15 -L axi_protocol_converter_v2_1_17 -L blk_mem_gen_v8_4_1 -L axis_infrastructure_v1_1_0 -L axis_data_fifo_v1_1_18 -L unisims_ver -L unimacro_ver -L secureip -L xpm --snapshot top_tb_behav xil_defaultlib.top_tb xil_defaultlib.glbl -log elaborate.log 
Using 8 slave threads.
Starting static elaboration
ERROR: [VRFC 10-426] cannot find port tuple_out_sume_metadata_DATA on this module [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:219]
ERROR: [VRFC 10-426] cannot find port tuple_out_sume_metadata_VALID on this module [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:218]
ERROR: [VRFC 10-426] cannot find port tuple_in_sume_metadata_DATA on this module [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:185]
ERROR: [VRFC 10-426] cannot find port tuple_in_sume_metadata_VALID on this module [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:184]
ERROR: [VRFC 10-2063] Module <S_RESETTER_line> not found while processing module instance <S_RESET_clk_line> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:332]
ERROR: [VRFC 10-2063] Module <S_RESETTER_lookup> not found while processing module instance <S_RESET_clk_lookup> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:343]
ERROR: [VRFC 10-2063] Module <S_RESETTER_control> not found while processing module instance <S_RESET_clk_control> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:354]
ERROR: [VRFC 10-2063] Module <TopParser_t> not found while processing module instance <TopParser> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:436]
ERROR: [VRFC 10-2063] Module <TopPipe_lvl_t> not found while processing module instance <TopPipe_lvl> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:474]
ERROR: [VRFC 10-2063] Module <dummy_table_for_netpfga_t> not found while processing module instance <dummy_table_for_netpfga> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:502]
ERROR: [VRFC 10-2063] Module <TopPipe_lvl_0_t> not found while processing module instance <TopPipe_lvl_0> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:533]
ERROR: [VRFC 10-2063] Module <TopDeparser_t> not found while processing module instance <TopDeparser> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:561]
ERROR: [VRFC 10-2063] Module <S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request> not found while processing module instance <S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:603]
ERROR: [VRFC 10-2063] Module <S_PROTOCOL_ADAPTER_INGRESS> not found while processing module instance <S_PROTOCOL_ADAPTER_INGRESS> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:617]
ERROR: [VRFC 10-2063] Module <S_PROTOCOL_ADAPTER_EGRESS> not found while processing module instance <S_PROTOCOL_ADAPTER_EGRESS> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:640]
ERROR: [VRFC 10-2063] Module <S_SYNCER_for_TopParser> not found while processing module instance <S_SYNCER_for_TopParser> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:662]
ERROR: [VRFC 10-2063] Module <S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser> not found while processing module instance <S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:704]
ERROR: [VRFC 10-2063] Module <S_SYNCER_for_S_SYNCER_for_TopDeparser> not found while processing module instance <S_SYNCER_for_S_SYNCER_for_TopDeparser> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:778]
ERROR: [VRFC 10-2063] Module <S_SYNCER_for_TopDeparser> not found while processing module instance <S_SYNCER_for_TopDeparser> [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:868]
INFO: [#UNDEF] Sorry, too many errors..
ERROR: [XSIM 43-3322] Static elaboration of top level Verilog design unit(s) in library work failed.
INFO: [USF-XSim-69] 'elaborate' step finished in '1' seconds
INFO: [USF-XSim-99] Step results log file:'/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim/elaborate.log'
ERROR: [USF-XSim-62] 'elaborate' step failed with error(s). Please check the Tcl console output or '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.sim/sim_1/behav/xsim/elaborate.log' file for more information.
ERROR: [Vivado 12-4473] Detected error while running simulation. Please correct the issue and retry this operation.
launch_simulation: Time (s): cpu = 00:00:10 ; elapsed = 00:00:13 . Memory (MB): peak = 2136.641 ; gain = 115.234 ; free physical = 10172 ; free virtual = 15212
ERROR: [Common 17-39] 'launch_simulation' failed due to earlier errors.

    while executing
"launch_simulation -simset sim_1 -mode behavioral"
    (file "/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/tcl/simple_sume_switch_sim.tcl" line 181)
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 19:43:04 2019...
Makefile:120: recipe for target 'sim' failed
make: *** [sim] Error 1
make: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test'
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_0_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_1_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_2_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/nf_interface_3_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/dma_0_log.axi': No such file or directory
cp: cannot stat '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/reg_stim.log': No such file or directory
NetFPGA environment:
   Root dir:       /home/nico/projects/P4-NetFPGA
   Project name:   simple_sume_switch
   Project dir:    /tmp/nico/test/simple_sume_switch
   Work dir:       /tmp/nico
512
=== Work directory is /tmp/nico/test/simple_sume_switch
=== Setting up test in /tmp/nico/test/simple_sume_switch/sim_switch_default
=== Running test /tmp/nico/test/simple_sume_switch/sim_switch_default ... using cmd ['/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/test/sim_switch_default/run.py', '--sim', 'xsim']
+ [  = no ]
+ cd /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch
+ make
make -C hw distclean
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
rm -rf proj_* vivado*.* *.*~ .Xil* /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/ip_repo/ /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/
rm -rf *[0-9]_{stim,expected,log}.axi
rm -f *.axi
rm -f portconfig.sim
rm -f seed
rm -f *.log
rm -f ../test/Makefile
rm -rf ../test/*.log
rm -rf ../test/*.axi
rm -rf ../test/seed
rm -rf ../test/*.sim
rm -rf ../test/proj_*
rm -rf ../test/ip_repo
rm -f ../test/vivado*.*
rm -f ../test/*_*_*/reg_defines_simple_sume_switch.py
rm -f ../test/*_*_*/reg_defines_simple_sume_switch.pyc
rm -rfv project;\
	rm -rfv ../sw/embedded/project;\
	rm -rfv vivado*;\
	rm -rfv *.log;\
	rm -rfv .Xil;\
	rm -rfv ..rej;\
	rm -rfv .srcs;\
	rm -rfv webtalk*;\
	rm -rfv *.*~;\
	rm -rfv ip_repo;\
	rm -rfv ip_proj;\
	rm -rfv std;\
                
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
make -C sw/embedded/ distclean
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/sw/embedded'
rm -rf `find . -name "SDK_Workspace"`
rm -rf `find . -name "*.log"`
rm -rf `find . -name "*.jou"`
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/sw/embedded'
rm -rfv vivado*;\

make -C hw project
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
rm -f ../hw/create_ip/id_rom16x32.coe
cp /home/nico/projects/P4-NetFPGA/tools/scripts/epoch.sh . && sh epoch.sh && rm -f epoch.sh
echo 16028002 >> rom_data.txt
echo `/home/nico/projects/P4-NetFPGA/run_tag.sh` >> rom_data.txt
grep: ../../../RELEASE_NOTES: No such file or directory
echo 00000204 >> rom_data.txt
echo 0000FFFF >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
cp /home/nico/projects/P4-NetFPGA/tools/scripts/format_coe.py . && python format_coe.py && rm -f format_coe.py 
16

mv -f id_rom16x32.coe ../hw/create_ip/
mv -f rom_data.txt ../hw/create_ip/
echo "Create reference project under folder /project";\
if test -d project/; then\
	echo "Project already exists"; \
else \
	vivado -mode batch -source tcl/simple_sume_switch.tcl;\
	if [ -f patch/simple_sume_switch.patch ]; then\
		patch -p1 < patch/simple_sume_switch.patch;\
	fi;\
fi;\

Create reference project under folder /project

****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source tcl/simple_sume_switch.tcl
# set design $::env(NF_PROJECT_NAME) 
# set top top
# set device xc7vx690t-3-ffg1761
# set proj_dir ./project
# set public_repo_dir $::env(SUME_FOLDER)/lib/hw/
# set xilinx_repo_dir $::env(XILINX_VIVADO)/data/ip/xilinx/
# set repo_dir ./ip_repo
# set bit_settings $::env(CONSTRAINTS)/generic_bit.xdc 
# set project_constraints ./constraints/nf_sume_general.xdc
# set nf_10g_constraints ./constraints/nf_sume_10g.xdc
# source ./tcl/$::env(NF_PROJECT_NAME)_defines.tcl
## set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
## set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
## set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
## set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
## set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
## set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
## set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
## set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
## set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
## set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
## set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
## set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
## set M00_BASEADDR 0x44000000
## set M00_HIGHADDR 0x44000FFF
## set M00_SIZEADDR 0x1000
## set M01_BASEADDR 0x44010000
## set M01_HIGHADDR 0x44010FFF
## set M01_SIZEADDR 0x1000
## set M02_BASEADDR 0x44020000
## set M02_HIGHADDR 0x44020FFF
## set M02_SIZEADDR 0x1000
## set M03_BASEADDR 0x44030000
## set M03_HIGHADDR 0x44030FFF
## set M03_SIZEADDR 0x1000
## set M04_BASEADDR 0x44040000
## set M04_HIGHADDR 0x44040FFF
## set M04_SIZEADDR 0x1000
## set M05_BASEADDR 0x44050000
## set M05_HIGHADDR 0x44050FFF
## set M05_SIZEADDR 0x1000
## set M06_BASEADDR 0x44060000
## set M06_HIGHADDR 0x44060FFF
## set M06_SIZEADDR 0x1000
## set M07_BASEADDR 0x44070000
## set M07_HIGHADDR 0x44070FFF
## set M07_SIZEADDR 0x1000
## set M08_BASEADDR 0x44080000
## set M08_HIGHADDR 0x44080FFF
## set M08_SIZEADDR 0x1000
## set IDENTIFIER_BASEADDR $M00_BASEADDR
## set IDENTIFIER_HIGHADDR $M00_HIGHADDR
## set IDENTIFIER_SIZEADDR $M00_SIZEADDR
## set INPUT_ARBITER_BASEADDR $M01_BASEADDR
## set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
## set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
## set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
## set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
## set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
## set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
## set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
## set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
## set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
## set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
## set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
## set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
## set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
## set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
## set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
## set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
## set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
## set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
## set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
## set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
## set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
## set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
## set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
# source ./tcl/export_registers.tcl
## set DEF_LIST {
## 	{MICROBLAZE_AXI_IIC 0 0 ""} \
## 	{MICROBLAZE_UARTLITE 0 0 ""} \
## 	{MICROBLAZE_DLMB_BRAM 0 0 ""} \
## 	{MICROBLAZE_ILMB_BRAM 0 0 ""} \
## 	{MICROBLAZE_AXI_INTC 0 0 ""} \
## 	{INPUT_ARBITER 0 1 input_arbiter_v1_0_0/data/input_arbiter_regs_defines.txt} \
## 	{OUTPUT_QUEUES 0 1 output_queues_v1_0_0/data/output_queues_regs_defines.txt} \
## 	{OUTPUT_PORT_LOOKUP 0 1 switch_output_port_lookup_v1_0_1/data/output_port_lookup_regs_defines.txt} \
## 	{NF_10G_INTERFACE0 0 1 nf_10ge_interface_shared_v1_0_0/data/nf_10g_interface_shared_regs_defines.txt} \
## 	{NF_10G_INTERFACE1 1 1 nf_10ge_interface_v1_0_0/data/nf_10g_interface_regs_defines.txt} \
## 	{NF_10G_INTERFACE2 2 1 nf_10ge_interface_v1_0_0/data/nf_10g_interface_regs_defines.txt} \
## 	{NF_10G_INTERFACE3 3 1 nf_10ge_interface_v1_0_0/data/nf_10g_interface_regs_defines.txt} \
## 	{NF_RIFFA_DMA 0 1 nf_riffa_dma_v1_0_0/data/nf_riffa_dma_regs_defines.txt} \
## 
## 
## }
## set target_path $::env(NF_DESIGN_DIR)/sw/embedded/src/
## set target_file $target_path/sume_register_defines.h
## proc write_header { target_file } {
## 
## # creat a blank header file
## # do a fresh rewrite in case the file already exits
## file delete -force $target_file
## open $target_file "w"
## set h_file [open $target_file "w"]
## 
## 
## puts $h_file "//-"
## puts $h_file "// Copyright (c) 2015 University of Cambridge"
## puts $h_file "// All rights reserved."
## puts $h_file "//"
## puts $h_file "// This software was developed by Stanford University and the University of Cambridge Computer Laboratory "
## puts $h_file "// under National Science Foundation under Grant No. CNS-0855268,"
## puts $h_file "// the University of Cambridge Computer Laboratory under EPSRC INTERNET Project EP/H040536/1 and"
## puts $h_file "// by the University of Cambridge Computer Laboratory under DARPA/AFRL contract FA8750-11-C-0249 (\"MRC2\"), "
## puts $h_file "// as part of the DARPA MRC research programme."
## puts $h_file "//"
## puts $h_file "// @NETFPGA_LICENSE_HEADER_START@"
## puts $h_file "//"
## puts $h_file "// Licensed to NetFPGA C.I.C. (NetFPGA) under one or more contributor"
## puts $h_file "// license agreements.  See the NOTICE file distributed with this work for"
## puts $h_file "// additional information regarding copyright ownership.  NetFPGA licenses this"
## puts $h_file "// file to you under the NetFPGA Hardware-Software License, Version 1.0 (the"
## puts $h_file "// \"License\"); you may not use this file except in compliance with the"
## puts $h_file "// License.  You may obtain a copy of the License at:"
## puts $h_file "//"
## puts $h_file "//   http://www.netfpga-cic.org"
## puts $h_file "//"
## puts $h_file "// Unless required by applicable law or agreed to in writing, Work distributed"
## puts $h_file "// under the License is distributed on an \"AS IS\" BASIS, WITHOUT WARRANTIES OR"
## puts $h_file "// CONDITIONS OF ANY KIND, either express or implied.  See the License for the"
## puts $h_file "// specific language governing permissions and limitations under the License."
## puts $h_file "//"
## puts $h_file "// @NETFPGA_LICENSE_HEADER_END@"
## puts $h_file "/////////////////////////////////////////////////////////////////////////////////"
## puts $h_file "// This is an automatically generated header definitions file"
## puts $h_file "/////////////////////////////////////////////////////////////////////////////////"
## puts $h_file ""
## 
## close $h_file 
## 
## };
## proc write_core {target_file prefix id has_registers lib_name} {
## 
## 
## set h_file [open $target_file "a"]
## 
## #First, read the memory map information from the reference_project defines file
## source $::env(NF_DESIGN_DIR)/hw/tcl/$::env(NF_PROJECT_NAME)_defines.tcl
## set public_repo_dir $::env(SUME_FOLDER)/lib/hw/
## 
## 
## set baseaddr [set $prefix\_BASEADDR]
## set highaddr [set $prefix\_HIGHADDR]
## set sizeaddr [set $prefix\_SIZEADDR]
## 
## puts $h_file "//######################################################"
## puts $h_file "//# Definitions for $prefix"
## puts $h_file "//######################################################"
## 
## puts $h_file "#define SUME_$prefix\_BASEADDR $baseaddr"
## puts $h_file "#define SUME_$prefix\_HIGHADDR $highaddr"
## puts $h_file "#define SUME_$prefix\_SIZEADDR $sizeaddr"
## puts $h_file ""
## 
## #Second, read the registers information from the library defines file
## if $has_registers {
## 	set lib_path "$public_repo_dir/std/cores/$lib_name"
## 	set regs_h_define_file $lib_path
## 	set regs_h_define_file_read [open $regs_h_define_file r]
## 	set regs_h_define_file_data [read $regs_h_define_file_read]
## 	close $regs_h_define_file_read
## 	set regs_h_define_file_data_line [split $regs_h_define_file_data "\n"]
## 
##        foreach read_line $regs_h_define_file_data_line {
##             if {[regexp "#define" $read_line]} {
##                 puts $h_file "#define SUME_[lindex $read_line 2]\_$id\_[lindex $read_line 3]\_[lindex $read_line 4] [lindex $read_line 5]"
##             }
## 	}
## }
## puts $h_file ""
## close $h_file 
## };
## write_header  $target_file 
## foreach lib_item $DEF_LIST { 
##      write_core  $target_file [lindex $lib_item 0] [lindex $lib_item 1] [lindex $lib_item 2] [lindex $lib_item 3] 
## }
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
# create_project -name ${design} -force -dir "./${proj_dir}" -part ${device}
# set_property source_mgmt_mode DisplayOnly [current_project]
# set_property top ${top} [current_fileset]
# puts "Creating User Datapath reference project"
Creating User Datapath reference project
# create_fileset -constrset -quiet constraints
# file copy ${public_repo_dir}/ ${repo_dir}
# set_property ip_repo_paths ${repo_dir} [current_fileset]
# add_files -fileset constraints -norecurse ${bit_settings}
# add_files -fileset constraints -norecurse ${project_constraints}
# add_files -fileset constraints -norecurse ${nf_10g_constraints}
# set_property is_enabled true [get_files ${project_constraints}]
# set_property is_enabled true [get_files ${bit_settings}]
# set_property is_enabled true [get_files ${nf_10g_constraints}]
# set_property constrset constraints [get_runs synth_1]
# set_property constrset constraints [get_runs impl_1]
# update_ip_catalog
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/ip_repo'.
INFO: [IP_Flow 19-2313] Loaded Vivado IP repository '/opt/Xilinx/Vivado/2018.2/data/ip'.
# create_ip -name input_arbiter -vendor NetFPGA -library NetFPGA -module_name input_arbiter_ip
# set_property generate_synth_checkpoint false [get_files input_arbiter_ip.xci]
# reset_target all [get_ips input_arbiter_ip]
# generate_target all [get_ips input_arbiter_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'input_arbiter_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'input_arbiter_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'input_arbiter_ip'...
# create_ip -name sss_output_queues -vendor NetFPGA -library NetFPGA -module_name sss_output_queues_ip
# set_property generate_synth_checkpoint false [get_files sss_output_queues_ip.xci]
# reset_target all [get_ips sss_output_queues_ip]
# generate_target all [get_ips sss_output_queues_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'sss_output_queues_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'sss_output_queues_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'sss_output_queues_ip'...
# source ./tcl/control_sub.tcl
## set scripts_vivado_version 2018.2
## set current_vivado_version [version -short]
## if { [string first $scripts_vivado_version $current_vivado_version] == -1 } {
##    puts ""
##    puts "ERROR: This script was created for Vivado <$scripts_vivado_version> and is being run in <$current_vivado_version> of Vivado. Please run the script in Vivado <$scripts_vivado_version> then open the design in Vivado <$current_vivado_version>. Upgrade the design by running \"Tools => Report => Report IP Status...\", then run write_bd_tcl to create an updated script."
## 
##    return 1
## }
## set design_name control_sub
## if { [get_projects -quiet] eq "" } {
##    puts "ERROR: Please open or create a project!"
##    return 1
## }
## set errMsg ""
## set nRet 0
## set cur_design [current_bd_design -quiet]
## set list_cells [get_bd_cells -quiet]
## if { ${design_name} eq "" } {
##    # USE CASES:
##    #    1) Design_name not set
## 
##    set errMsg "ERROR: Please set the variable <design_name> to a non-empty value."
##    set nRet 1
## 
## } elseif { ${cur_design} ne "" && ${list_cells} eq "" } {
##    # USE CASES:
##    #    2): Current design opened AND is empty AND names same.
##    #    3): Current design opened AND is empty AND names diff; design_name NOT in project.
##    #    4): Current design opened AND is empty AND names diff; design_name exists in project.
## 
##    if { $cur_design ne $design_name } {
##       puts "INFO: Changing value of <design_name> from <$design_name> to <$cur_design> since current design is empty."
##       set design_name [get_property NAME $cur_design]
##    }
##    puts "INFO: Constructing design in IPI design <$cur_design>..."
## 
## } elseif { ${cur_design} ne "" && $list_cells ne "" && $cur_design eq $design_name } {
##    # USE CASES:
##    #    5) Current design opened AND has components AND same names.
## 
##    set errMsg "ERROR: Design <$design_name> already exists in your project, please set the variable <design_name> to another value."
##    set nRet 1
## } elseif { [get_files -quiet ${design_name}.bd] ne "" } {
##    # USE CASES:
##    #    6) Current opened design, has components, but diff names, design_name exists in project.
##    #    7) No opened design, design_name exists in project.
## 
##    set errMsg "ERROR: Design <$design_name> already exists in your project, please set the variable <design_name> to another value."
##    set nRet 2
## 
## } else {
##    # USE CASES:
##    #    8) No opened design, design_name not in project.
##    #    9) Current opened design, has components, but diff names, design_name not in project.
## 
##    puts "INFO: Currently there is no design <$design_name> in project, so creating one..."
## 
##    create_bd_design $design_name
## 
##    puts "INFO: Making design <$design_name> as current_bd_design."
##    current_bd_design $design_name
## 
## }
INFO: Currently there is no design <control_sub> in project, so creating one...
Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd> 
INFO: Making design <control_sub> as current_bd_design.
## puts "INFO: Currently the variable <design_name> is equal to \"$design_name\"."
INFO: Currently the variable <design_name> is equal to "control_sub".
## if { $nRet != 0 } {
##    puts $errMsg
##    return $nRet
## }
## proc create_hier_cell_microblaze_0_local_memory { parentCell nameHier } {
## 
##   if { $parentCell eq "" || $nameHier eq "" } {
##      puts "ERROR: create_hier_cell_microblaze_0_local_memory() - Empty argument(s)!"
##      return
##   }
## 
##   # Get object for parentCell
##   set parentObj [get_bd_cells $parentCell]
##   if { $parentObj == "" } {
##      puts "ERROR: Unable to find parent cell <$parentCell>!"
##      return
##   }
## 
##   # Make sure parentObj is hier blk
##   set parentType [get_property TYPE $parentObj]
##   if { $parentType ne "hier" } {
##      puts "ERROR: Parent <$parentObj> has TYPE = <$parentType>. Expected to be <hier>."
##      return
##   }
## 
##   # Save current instance; Restore later
##   set oldCurInst [current_bd_instance .]
## 
##   # Set parent object as current
##   current_bd_instance $parentObj
## 
##   # Create cell and set as current instance
##   set hier_obj [create_bd_cell -type hier $nameHier]
##   current_bd_instance $hier_obj
## 
##   # Create interface pins
##   create_bd_intf_pin -mode MirroredMaster -vlnv xilinx.com:interface:lmb_rtl:1.0 DLMB
##   create_bd_intf_pin -mode MirroredMaster -vlnv xilinx.com:interface:lmb_rtl:1.0 ILMB
## 
##   # Create pins
##   create_bd_pin -dir I -type clk LMB_Clk
##   create_bd_pin -dir I -from 0 -to 0 -type rst LMB_Rst
## 
##   # Create instance: dlmb_bram_if_cntlr, and set properties
##   set dlmb_bram_if_cntlr [ create_bd_cell -type ip -vlnv xilinx.com:ip:lmb_bram_if_cntlr:4.0 dlmb_bram_if_cntlr ]
##   set_property -dict [ list CONFIG.C_ECC {0}  ] $dlmb_bram_if_cntlr
## 
##   # Create instance: dlmb_v10, and set properties
##   set dlmb_v10 [ create_bd_cell -type ip -vlnv xilinx.com:ip:lmb_v10:3.0 dlmb_v10 ]
## 
##   # Create instance: ilmb_bram_if_cntlr, and set properties
##   set ilmb_bram_if_cntlr [ create_bd_cell -type ip -vlnv xilinx.com:ip:lmb_bram_if_cntlr:4.0 ilmb_bram_if_cntlr ]
##   set_property -dict [ list CONFIG.C_ECC {0}  ] $ilmb_bram_if_cntlr
## 
##   # Create instance: ilmb_v10, and set properties
##   set ilmb_v10 [ create_bd_cell -type ip -vlnv xilinx.com:ip:lmb_v10:3.0 ilmb_v10 ]
## 
##   # Create instance: lmb_bram, and set properties
##   set lmb_bram [ create_bd_cell -type ip -vlnv xilinx.com:ip:blk_mem_gen:8.4 lmb_bram ]
##   set_property -dict [ list CONFIG.Memory_Type {True_Dual_Port_RAM} CONFIG.use_bram_block {BRAM_Controller}  ] $lmb_bram
## 
##   # Create interface connections
##   connect_bd_intf_net -intf_net microblaze_0_dlmb [get_bd_intf_pins DLMB] [get_bd_intf_pins dlmb_v10/LMB_M]
##   connect_bd_intf_net -intf_net microblaze_0_dlmb_bus [get_bd_intf_pins dlmb_bram_if_cntlr/SLMB] [get_bd_intf_pins dlmb_v10/LMB_Sl_0]
##   connect_bd_intf_net -intf_net microblaze_0_dlmb_cntlr [get_bd_intf_pins dlmb_bram_if_cntlr/BRAM_PORT] [get_bd_intf_pins lmb_bram/BRAM_PORTA]
##   connect_bd_intf_net -intf_net microblaze_0_ilmb [get_bd_intf_pins ILMB] [get_bd_intf_pins ilmb_v10/LMB_M]
##   connect_bd_intf_net -intf_net microblaze_0_ilmb_bus [get_bd_intf_pins ilmb_bram_if_cntlr/SLMB] [get_bd_intf_pins ilmb_v10/LMB_Sl_0]
##   connect_bd_intf_net -intf_net microblaze_0_ilmb_cntlr [get_bd_intf_pins ilmb_bram_if_cntlr/BRAM_PORT] [get_bd_intf_pins lmb_bram/BRAM_PORTB]
## 
##   # Create port connections
##   connect_bd_net -net microblaze_0_Clk [get_bd_pins LMB_Clk] [get_bd_pins dlmb_bram_if_cntlr/LMB_Clk] [get_bd_pins dlmb_v10/LMB_Clk] [get_bd_pins ilmb_bram_if_cntlr/LMB_Clk] [get_bd_pins ilmb_v10/LMB_Clk]
##   connect_bd_net -net microblaze_0_LMB_Rst [get_bd_pins LMB_Rst] [get_bd_pins dlmb_bram_if_cntlr/LMB_Rst] [get_bd_pins dlmb_v10/SYS_Rst] [get_bd_pins ilmb_bram_if_cntlr/LMB_Rst] [get_bd_pins ilmb_v10/SYS_Rst]
## 
##   # Restore current instance
##   current_bd_instance $oldCurInst
## }
## proc create_hier_cell_mbsys { parentCell nameHier } {
## 
##   if { $parentCell eq "" || $nameHier eq "" } {
##      puts "ERROR: create_hier_cell_mbsys() - Empty argument(s)!"
##      return
##   }
## 
##   # Get object for parentCell
##   set parentObj [get_bd_cells $parentCell]
##   if { $parentObj == "" } {
##      puts "ERROR: Unable to find parent cell <$parentCell>!"
##      return
##   }
## 
##   # Make sure parentObj is hier blk
##   set parentType [get_property TYPE $parentObj]
##   if { $parentType ne "hier" } {
##      puts "ERROR: Parent <$parentObj> has TYPE = <$parentType>. Expected to be <hier>."
##      return
##   }
## 
##   # Save current instance; Restore later
##   set oldCurInst [current_bd_instance .]
## 
##   # Set parent object as current
##   current_bd_instance $parentObj
## 
##   # Create cell and set as current instance
##   set hier_obj [create_bd_cell -type hier $nameHier]
##   current_bd_instance $hier_obj
## 
##   # Create interface pins
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M01_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M02_AXI
## 
##   # Create pins
##   create_bd_pin -dir I -type clk Clk
##   create_bd_pin -dir I -from 0 -to 0 In0
##   create_bd_pin -dir I -from 0 -to 0 In1
##   create_bd_pin -dir I dcm_locked
##   create_bd_pin -dir I -type rst ext_reset_in
##   create_bd_pin -dir O -from 0 -to 0 -type rst peripheral_aresetn
## 
##   # Create instance: mdm_1, and set properties
##   set mdm_1 [ create_bd_cell -type ip -vlnv xilinx.com:ip:mdm:3.2 mdm_1 ]
## 
##   # Create instance: microblaze_0, and set properties
##   set microblaze_0 [ create_bd_cell -type ip -vlnv xilinx.com:ip:microblaze:10.0 microblaze_0 ]
##   set_property -dict [ list CONFIG.C_DEBUG_ENABLED {1} CONFIG.C_D_AXI {1} CONFIG.C_D_LMB {1} CONFIG.C_I_LMB {1}  ] $microblaze_0
## 
##   # Create instance: microblaze_0_axi_intc, and set properties
##   set microblaze_0_axi_intc [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_intc:4.1 microblaze_0_axi_intc ]
##   set_property -dict [ list CONFIG.C_HAS_FAST {1}  ] $microblaze_0_axi_intc
## 
##   # Create instance: microblaze_0_axi_periph, and set properties
##   set microblaze_0_axi_periph [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_interconnect:2.1 microblaze_0_axi_periph ]
##   set_property -dict [ list CONFIG.NUM_MI {3}  ] $microblaze_0_axi_periph
## 
##   # Create instance: microblaze_0_local_memory
##   create_hier_cell_microblaze_0_local_memory $hier_obj microblaze_0_local_memory
## 
##   # Create instance: microblaze_0_xlconcat, and set properties
##   set microblaze_0_xlconcat [ create_bd_cell -type ip -vlnv xilinx.com:ip:xlconcat:2.1 microblaze_0_xlconcat ]
## 
##   # Create instance: rst_clk_wiz_1_100M, and set properties
##   set rst_clk_wiz_1_100M [ create_bd_cell -type ip -vlnv xilinx.com:ip:proc_sys_reset:5.0 rst_clk_wiz_1_100M ]
## 
##   # Create interface connections
##   connect_bd_intf_net -intf_net Conn1 [get_bd_intf_pins M01_AXI] [get_bd_intf_pins microblaze_0_axi_periph/M01_AXI]
##   connect_bd_intf_net -intf_net Conn2 [get_bd_intf_pins M02_AXI] [get_bd_intf_pins microblaze_0_axi_periph/M02_AXI]
##   connect_bd_intf_net -intf_net microblaze_0_axi_dp [get_bd_intf_pins microblaze_0/M_AXI_DP] [get_bd_intf_pins microblaze_0_axi_periph/S00_AXI]
##   connect_bd_intf_net -intf_net microblaze_0_debug [get_bd_intf_pins mdm_1/MBDEBUG_0] [get_bd_intf_pins microblaze_0/DEBUG]
##   connect_bd_intf_net -intf_net microblaze_0_dlmb_1 [get_bd_intf_pins microblaze_0/DLMB] [get_bd_intf_pins microblaze_0_local_memory/DLMB]
##   connect_bd_intf_net -intf_net microblaze_0_ilmb_1 [get_bd_intf_pins microblaze_0/ILMB] [get_bd_intf_pins microblaze_0_local_memory/ILMB]
##   connect_bd_intf_net -intf_net microblaze_0_intc_axi [get_bd_intf_pins microblaze_0_axi_intc/s_axi] [get_bd_intf_pins microblaze_0_axi_periph/M00_AXI]
##   connect_bd_intf_net -intf_net microblaze_0_interrupt [get_bd_intf_pins microblaze_0/INTERRUPT] [get_bd_intf_pins microblaze_0_axi_intc/interrupt]
## 
##   # Create port connections
##   connect_bd_net -net In0_1 [get_bd_pins In0] [get_bd_pins microblaze_0_xlconcat/In0]
##   connect_bd_net -net In1_1 [get_bd_pins In1] [get_bd_pins microblaze_0_xlconcat/In1]
##   connect_bd_net -net clk_wiz_1_locked [get_bd_pins dcm_locked] [get_bd_pins rst_clk_wiz_1_100M/dcm_locked]
##   connect_bd_net -net mdm_1_debug_sys_rst [get_bd_pins mdm_1/Debug_SYS_Rst] [get_bd_pins rst_clk_wiz_1_100M/mb_debug_sys_rst]
##   connect_bd_net -net microblaze_0_Clk [get_bd_pins Clk] [get_bd_pins microblaze_0/Clk] [get_bd_pins microblaze_0_axi_intc/processor_clk] [get_bd_pins microblaze_0_axi_intc/s_axi_aclk] [get_bd_pins microblaze_0_axi_periph/ACLK] [get_bd_pins microblaze_0_axi_periph/M00_ACLK] [get_bd_pins microblaze_0_axi_periph/M01_ACLK] [get_bd_pins microblaze_0_axi_periph/M02_ACLK] [get_bd_pins microblaze_0_axi_periph/S00_ACLK] [get_bd_pins microblaze_0_local_memory/LMB_Clk] [get_bd_pins rst_clk_wiz_1_100M/slowest_sync_clk]
##   connect_bd_net -net microblaze_0_intr [get_bd_pins microblaze_0_axi_intc/intr] [get_bd_pins microblaze_0_xlconcat/dout]
##   connect_bd_net -net reset_1 [get_bd_pins ext_reset_in] [get_bd_pins rst_clk_wiz_1_100M/ext_reset_in]
##   connect_bd_net -net rst_clk_wiz_1_100M_bus_struct_reset [get_bd_pins microblaze_0_local_memory/LMB_Rst] [get_bd_pins rst_clk_wiz_1_100M/bus_struct_reset]
##   connect_bd_net -net rst_clk_wiz_1_100M_interconnect_aresetn [get_bd_pins microblaze_0_axi_periph/ARESETN] [get_bd_pins rst_clk_wiz_1_100M/interconnect_aresetn]
##   connect_bd_net -net rst_clk_wiz_1_100M_mb_reset [get_bd_pins microblaze_0/Reset] [get_bd_pins microblaze_0_axi_intc/processor_rst] [get_bd_pins rst_clk_wiz_1_100M/mb_reset]
##   connect_bd_net -net rst_clk_wiz_1_100M_peripheral_aresetn [get_bd_pins peripheral_aresetn] [get_bd_pins microblaze_0_axi_intc/s_axi_aresetn] [get_bd_pins microblaze_0_axi_periph/M00_ARESETN] [get_bd_pins microblaze_0_axi_periph/M01_ARESETN] [get_bd_pins microblaze_0_axi_periph/M02_ARESETN] [get_bd_pins microblaze_0_axi_periph/S00_ARESETN] [get_bd_pins rst_clk_wiz_1_100M/peripheral_aresetn]
## 
##   # Restore current instance
##   current_bd_instance $oldCurInst
## }
## proc create_hier_cell_nf_mbsys { parentCell nameHier } {
## 
##   if { $parentCell eq "" || $nameHier eq "" } {
##      puts "ERROR: create_hier_cell_nf_mbsys() - Empty argument(s)!"
##      return
##   }
## 
##   # Get object for parentCell
##   set parentObj [get_bd_cells $parentCell]
##   if { $parentObj == "" } {
##      puts "ERROR: Unable to find parent cell <$parentCell>!"
##      return
##   }
## 
##   # Make sure parentObj is hier blk
##   set parentType [get_property TYPE $parentObj]
##   if { $parentType ne "hier" } {
##      puts "ERROR: Parent <$parentObj> has TYPE = <$parentType>. Expected to be <hier>."
##      return
##   }
## 
##   # Save current instance; Restore later
##   set oldCurInst [current_bd_instance .]
## 
##   # Set parent object as current
##   current_bd_instance $parentObj
## 
##   # Create cell and set as current instance
##   set hier_obj [create_bd_cell -type hier $nameHier]
##   current_bd_instance $hier_obj
## 
##   # Create interface pins
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:iic_rtl:1.0 iic_fpga
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:uart_rtl:1.0 uart
## 
##   # Create pins
##   create_bd_pin -dir O -from 1 -to 0 iic_reset
##   create_bd_pin -dir I -type rst reset
##   create_bd_pin -dir I -type clk sysclk
## 
##   # Create instance: axi_iic_0, and set properties
##   set axi_iic_0 [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_iic:2.0 axi_iic_0 ]
##   set_property -dict [ list CONFIG.C_GPO_WIDTH {2} CONFIG.C_SCL_INERTIAL_DELAY {5} CONFIG.C_SDA_INERTIAL_DELAY {5}  ] $axi_iic_0
## 
##   # Create instance: axi_uartlite_0, and set properties
##   set axi_uartlite_0 [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_uartlite:2.0 axi_uartlite_0 ]
##   set_property -dict [ list CONFIG.C_BAUDRATE {115200}  ] $axi_uartlite_0
## 
##   # Create instance: clk_wiz_1, and set properties
##   set clk_wiz_1 [ create_bd_cell -type ip -vlnv xilinx.com:ip:clk_wiz:6.0 clk_wiz_1 ]
## #  set_property -dict [ list CONFIG.PRIM_IN_FREQ {200.000} CONFIG.PRIM_SOURCE {No_buffer}  ] $clk_wiz_1
## 
##   # config 100MHz input clk
##   set_property -dict [list CONFIG.PRIM_IN_FREQ {100.000} CONFIG.PRIM_SOURCE {No_buffer} \
##   CONFIG.CLKIN1_JITTER_PS {100.0} CONFIG.MMCM_CLKFBOUT_MULT_F {10.000} \
##   CONFIG.MMCM_CLKIN1_PERIOD {10.0} CONFIG.CLKOUT1_JITTER {130.958} \
##   CONFIG.CLKOUT1_PHASE_ERROR {98.575}] $clk_wiz_1
## 
## 
##   # Create instance: mbsys
##   create_hier_cell_mbsys $hier_obj mbsys
## 
##   # Create interface connections
##   connect_bd_intf_net -intf_net axi_iic_0_IIC [get_bd_intf_pins iic_fpga] [get_bd_intf_pins axi_iic_0/IIC]
##   connect_bd_intf_net -intf_net axi_uartlite_0_UART [get_bd_intf_pins uart] [get_bd_intf_pins axi_uartlite_0/UART]
##   connect_bd_intf_net -intf_net mbsys_M01_AXI [get_bd_intf_pins axi_iic_0/S_AXI] [get_bd_intf_pins mbsys/M01_AXI]
##   connect_bd_intf_net -intf_net mbsys_M02_AXI [get_bd_intf_pins axi_uartlite_0/S_AXI] [get_bd_intf_pins mbsys/M02_AXI]
## 
##   # Create port connections
##   connect_bd_net -net axi_iic_0_gpo [get_bd_pins iic_reset] [get_bd_pins axi_iic_0/gpo]
##   connect_bd_net -net axi_iic_0_iic2intc_irpt [get_bd_pins axi_iic_0/iic2intc_irpt] [get_bd_pins mbsys/In0]
##   connect_bd_net -net axi_uartlite_0_interrupt [get_bd_pins axi_uartlite_0/interrupt] [get_bd_pins mbsys/In1]
##   connect_bd_net -net clk_wiz_1_locked [get_bd_pins clk_wiz_1/locked] [get_bd_pins mbsys/dcm_locked]
##   connect_bd_net -net mbsys_peripheral_aresetn [get_bd_pins axi_iic_0/s_axi_aresetn] [get_bd_pins axi_uartlite_0/s_axi_aresetn] [get_bd_pins mbsys/peripheral_aresetn]
##   connect_bd_net -net microblaze_0_Clk [get_bd_pins axi_iic_0/s_axi_aclk] [get_bd_pins axi_uartlite_0/s_axi_aclk] [get_bd_pins clk_wiz_1/clk_out1] [get_bd_pins mbsys/Clk]
##   connect_bd_net -net reset_1 [get_bd_pins reset] [get_bd_pins clk_wiz_1/reset] [get_bd_pins mbsys/ext_reset_in]
##   connect_bd_net -net sysclk_1 [get_bd_pins sysclk] [get_bd_pins clk_wiz_1/clk_in1]
## 
##   # Restore current instance
##   current_bd_instance $oldCurInst
## }
## proc create_hier_cell_dma_sub { parentCell nameHier } {
## 
##   if { $parentCell eq "" || $nameHier eq "" } {
##      puts "ERROR: create_hier_cell_dma_sub() - Empty argument(s)!"
##      return
##   }
## 
##   # Get object for parentCell
##   set parentObj [get_bd_cells $parentCell]
##   if { $parentObj == "" } {
##      puts "ERROR: Unable to find parent cell <$parentCell>!"
##      return
##   }
## 
##   # Make sure parentObj is hier blk
##   set parentType [get_property TYPE $parentObj]
##   if { $parentType ne "hier" } {
##      puts "ERROR: Parent <$parentObj> has TYPE = <$parentType>. Expected to be <hier>."
##      return
##   }
## 
##   # Save current instance; Restore later
##   set oldCurInst [current_bd_instance .]
## 
##   # Set parent object as current
##   current_bd_instance $parentObj
## 
##   # Create cell and set as current instance
##   set hier_obj [create_bd_cell -type hier $nameHier]
##   current_bd_instance $hier_obj
## 
##   # Create interface pins
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M00_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M01_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M02_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M03_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M04_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M05_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M06_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M07_AXI
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:axis_rtl:1.0 m_axis_dma_tx
##   create_bd_intf_pin -mode Master -vlnv xilinx.com:interface:pcie_7x_mgt_rtl:1.0 pcie_7x_mgt
##   create_bd_intf_pin -mode Slave -vlnv xilinx.com:interface:axis_rtl:1.0 s_axis_dma_rx
## 
##   # Create pins
##   create_bd_pin -dir I -type clk axi_lite_aclk
##   create_bd_pin -dir I -type rst axi_lite_aresetn
##   create_bd_pin -dir I -type clk axis_datapath_aclk
##   create_bd_pin -dir I -type rst axis_datapath_aresetn
##   create_bd_pin -dir I -type clk sys_clk
##   create_bd_pin -dir I -type rst sys_reset
## 
##   create_bd_pin -dir I -type clk M00_ACLK
##   create_bd_pin -dir I -type rst M00_ARESETN
##   create_bd_pin -dir I -type clk M01_ACLK
##   create_bd_pin -dir I -type rst M01_ARESETN
##   create_bd_pin -dir I -type clk M02_ACLK
##   create_bd_pin -dir I -type rst M02_ARESETN
##   create_bd_pin -dir I -type clk M03_ACLK
##   create_bd_pin -dir I -type rst M03_ARESETN
##   create_bd_pin -dir I -type clk M04_ACLK
##   create_bd_pin -dir I -type rst M04_ARESETN
##   create_bd_pin -dir I -type clk M05_ACLK
##   create_bd_pin -dir I -type rst M05_ARESETN
##   create_bd_pin -dir I -type clk M06_ACLK
##   create_bd_pin -dir I -type rst M06_ARESETN
##   create_bd_pin -dir I -type clk M07_ACLK
##   create_bd_pin -dir I -type rst M07_ARESETN
## 
##   # Create instance: axi_interconnect_0, and set properties
##   set axi_interconnect_0 [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_interconnect:2.1 axi_interconnect_0 ]
##   set_property -dict [ list CONFIG.NUM_MI {9}  ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M00_HAS_REGSLICE {3} CONFIG.M00_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M01_HAS_REGSLICE {3} CONFIG.M01_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M02_HAS_REGSLICE {3} CONFIG.M02_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M03_HAS_REGSLICE {3} CONFIG.M03_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M04_HAS_REGSLICE {3} CONFIG.M04_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M05_HAS_REGSLICE {3} CONFIG.M05_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M06_HAS_REGSLICE {3} CONFIG.M06_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M07_HAS_REGSLICE {3} CONFIG.M07_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.M08_HAS_REGSLICE {3} CONFIG.M08_HAS_DATA_FIFO {1} ] $axi_interconnect_0
##   set_property -dict [list CONFIG.S00_HAS_REGSLICE {3} CONFIG.S00_HAS_DATA_FIFO {1} ] $axi_interconnect_0
## 
##   # AXIS: clock domain crossing FIFO, TX (PCIe->FPGA) user_fifo_reset (user_clk)
##   set pcie_reset_inv [create_bd_cell -type ip -vlnv xilinx.com:ip:util_vector_logic pcie_reset_inv]
##   set_property -dict [list CONFIG.C_SIZE {1} CONFIG.C_OPERATION {not}] [get_bd_cells pcie_reset_inv]
## 
##   # Create instance: axis_dwidth_converter
##   set axis_dwidth_dma_tx [ create_bd_cell -type ip -vlnv xilinx.com:ip:axis_dwidth_converter:1.1 axis_dwidth_dma_tx]
##   set_property -dict [list CONFIG.HAS_TKEEP.VALUE_SRC USER CONFIG.HAS_TLAST.VALUE_SRC USER \
##            CONFIG.HAS_TSTRB.VALUE_SRC USER CONFIG.S_TDATA_NUM_BYTES.VALUE_SRC USER \
## 	   CONFIG.TUSER_BITS_PER_BYTE.VALUE_SRC USER] $axis_dwidth_dma_tx
## 
##   set_property -dict [list CONFIG.S_TDATA_NUM_BYTES {16} CONFIG.M_TDATA_NUM_BYTES {32} \
## 	   CONFIG.TUSER_BITS_PER_BYTE {8} CONFIG.HAS_TLAST {1} CONFIG.HAS_TSTRB {0} \
## 	   CONFIG.HAS_TKEEP {1} CONFIG.HAS_MI_TKEEP {1}] $axis_dwidth_dma_tx
## 
## 
## 
##   set axis_dwidth_dma_rx [ create_bd_cell -type ip -vlnv xilinx.com:ip:axis_dwidth_converter:1.1 axis_dwidth_dma_rx]
## 
##   set_property -dict [list CONFIG.HAS_TKEEP.VALUE_SRC USER CONFIG.HAS_TLAST.VALUE_SRC USER \
##              CONFIG.HAS_TSTRB.VALUE_SRC USER CONFIG.S_TDATA_NUM_BYTES.VALUE_SRC USER \
##              CONFIG.TUSER_BITS_PER_BYTE.VALUE_SRC USER] $axis_dwidth_dma_rx
## 
##   set_property -dict [list CONFIG.S_TDATA_NUM_BYTES {32} CONFIG.M_TDATA_NUM_BYTES {16} \
##              CONFIG.TUSER_BITS_PER_BYTE {8} CONFIG.HAS_TLAST {1} CONFIG.HAS_TSTRB {0} \
## 	     CONFIG.HAS_TKEEP {1} CONFIG.HAS_MI_TKEEP {1}] $axis_dwidth_dma_rx
## 
##  # Create instance: axis_fifo_10g_rx, and set properties
##  set axis_fifo_10g_rx [create_bd_cell -type ip -vlnv xilinx.com:ip:axis_data_fifo:1.1 axis_fifo_10g_rx]
##  set_property -dict [list CONFIG.TDATA_NUM_BYTES {16} CONFIG.TUSER_WIDTH {128} CONFIG.IS_ACLK_ASYNC {1} CONFIG.FIFO_DEPTH {32}] $axis_fifo_10g_rx
## 
##   # Create instance: axis_fifo_10g_tx, and set properties
##  set axis_fifo_10g_tx [create_bd_cell -type ip -vlnv xilinx.com:ip:axis_data_fifo:1.1 axis_fifo_10g_tx]
##  set_property -dict [list CONFIG.TDATA_NUM_BYTES {16} CONFIG.TUSER_WIDTH {128} CONFIG.IS_ACLK_ASYNC {1} CONFIG.FIFO_DEPTH {32}] $axis_fifo_10g_tx
## 
##   # Create instance: nf_riffa_dma_1, and set properties
##   set nf_riffa_dma_1 [ create_bd_cell -type ip -vlnv NetFPGA:NetFPGA:nf_riffa_dma:1.0 nf_riffa_dma_1 ]
## 
##   # Create instance: axi_clock_converter_0, and set properties
##   set axi_clock_converter_0 [ create_bd_cell -type ip -vlnv xilinx.com:ip:axi_clock_converter:2.1 axi_clock_converter_0 ]
## 
##   # Create instance: pcie3_7x_1, and set properties
##   set pcie3_7x_1 [ create_bd_cell -type ip -vlnv xilinx.com:ip:pcie3_7x:4.3 pcie3_7x_1 ]
##   set_property -dict [ list CONFIG.PF0_DEVICE_ID {7028} \
## CONFIG.PF0_INTERRUPT_PIN {NONE} CONFIG.PF1_DEVICE_ID {7011} \
## CONFIG.PL_LINK_CAP_MAX_LINK_SPEED {5.0_GT/s} CONFIG.PL_LINK_CAP_MAX_LINK_WIDTH {X8} \
## CONFIG.axisten_freq {250} CONFIG.axisten_if_enable_client_tag {false} \
## CONFIG.axisten_if_width {128_bit} CONFIG.cfg_ctl_if {false} \
## CONFIG.cfg_ext_if {false} CONFIG.cfg_mgmt_if {false} \
## CONFIG.cfg_tx_msg_if {false} CONFIG.en_ext_clk {false} \
## CONFIG.extended_tag_field {true} CONFIG.gen_x0y0 {false} \
## CONFIG.mode_selection {Advanced} CONFIG.pcie_blk_locn {X0Y1} \
## CONFIG.per_func_status_if {false} CONFIG.pf0_bar0_size {1} \
## CONFIG.pf0_dev_cap_max_payload {128_bytes} CONFIG.rcv_msg_if {false} \
## CONFIG.tx_fc_if {false} CONFIG.xlnx_ref_board {None} \
##  ] $pcie3_7x_1
## 
##   # Create interface connections
##   connect_bd_intf_net -intf_net axi_interconnect_0_M00_AXI [get_bd_intf_pins M00_AXI] [get_bd_intf_pins axi_interconnect_0/M00_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M01_AXI [get_bd_intf_pins M01_AXI] [get_bd_intf_pins axi_interconnect_0/M01_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M02_AXI [get_bd_intf_pins M02_AXI] [get_bd_intf_pins axi_interconnect_0/M02_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M03_AXI [get_bd_intf_pins M03_AXI] [get_bd_intf_pins axi_interconnect_0/M03_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M04_AXI [get_bd_intf_pins M04_AXI] [get_bd_intf_pins axi_interconnect_0/M04_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M05_AXI [get_bd_intf_pins M05_AXI] [get_bd_intf_pins axi_interconnect_0/M05_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M06_AXI [get_bd_intf_pins M06_AXI] [get_bd_intf_pins axi_interconnect_0/M06_AXI]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M07_AXI [get_bd_intf_pins M07_AXI] [get_bd_intf_pins axi_interconnect_0/M07_AXI]
## 
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_s_axis_dma_rx [get_bd_intf_pins s_axis_dma_rx] [get_bd_intf_pins axis_dwidth_dma_rx/S_AXIS]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_fifo_dwidth_rx [get_bd_intf_pins axis_fifo_10g_rx/S_AXIS] [get_bd_intf_pins axis_dwidth_dma_rx/M_AXIS]
##   connect_bd_intf_net -intf_net axis_fifo_10g_rx_M_AXIS [get_bd_intf_pins axis_fifo_10g_rx/M_AXIS] [get_bd_intf_pins nf_riffa_dma_1/s_axis_xge_rx]
## 
## 
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_m_axis_dma_tx [get_bd_intf_pins m_axis_dma_tx] [get_bd_intf_pins axis_dwidth_dma_tx/M_AXIS]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_fifo_dwidth_tx [get_bd_intf_pins axis_fifo_10g_tx/M_AXIS] [get_bd_intf_pins axis_dwidth_dma_tx/S_AXIS]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_dwidth_conv_tx [get_bd_intf_pins axis_fifo_10g_tx/S_AXIS] [get_bd_intf_pins nf_riffa_dma_1/m_axis_xge_tx]
## 
## 
## 
## # connect_bd_intf_net -intf_net nf_riffa_dma_1_pcie3_cfg_interrupt [get_bd_intf_pins nf_riffa_dma_1/cfg_interrupt] [get_bd_intf_pins pcie3_7x_1/pcie3_cfg_interrupt]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_pcie3_cfg_msi [get_bd_intf_pins nf_riffa_dma_1/cfg_interrupt_msi] [get_bd_intf_pins pcie3_7x_1/pcie3_cfg_msi]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_pcie3_cfg_status [get_bd_intf_pins nf_riffa_dma_1/cfg] [get_bd_intf_pins pcie3_7x_1/pcie3_cfg_status]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_pcie_cfg_fc [get_bd_intf_pins nf_riffa_dma_1/cfg_fc] [get_bd_intf_pins pcie3_7x_1/pcie_cfg_fc]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_s_axis_cc [get_bd_intf_pins nf_riffa_dma_1/s_axis_cc] [get_bd_intf_pins pcie3_7x_1/s_axis_cc]
##   connect_bd_intf_net -intf_net nf_riffa_dma_1_s_axis_rq [get_bd_intf_pins nf_riffa_dma_1/s_axis_rq] [get_bd_intf_pins pcie3_7x_1/s_axis_rq]
##   connect_bd_intf_net -intf_net pcie3_7x_1_m_axis_cq [get_bd_intf_pins nf_riffa_dma_1/m_axis_cq] [get_bd_intf_pins pcie3_7x_1/m_axis_cq]
##   connect_bd_intf_net -intf_net pcie3_7x_1_m_axis_rc [get_bd_intf_pins nf_riffa_dma_1/m_axis_rc] [get_bd_intf_pins pcie3_7x_1/m_axis_rc]
##   connect_bd_intf_net -intf_net pcie3_7x_1_pcie_7x_mgt [get_bd_intf_pins pcie_7x_mgt] [get_bd_intf_pins pcie3_7x_1/pcie_7x_mgt]
##   connect_bd_intf_net -intf_net s00_axi_1 [get_bd_intf_pins axi_interconnect_0/S00_AXI] [get_bd_intf_pins nf_riffa_dma_1/m_axi_lite]
## 
##   #Clock converter connections
##   connect_bd_intf_net -intf_net axi_clock_converter_0_M_AXI [get_bd_intf_pins axi_clock_converter_0/M_AXI] [get_bd_intf_pins nf_riffa_dma_1/s_axi_lite]
##   connect_bd_intf_net -intf_net axi_interconnect_0_M08_AXI [get_bd_intf_pins axi_clock_converter_0/S_AXI] [get_bd_intf_pins axi_interconnect_0/M08_AXI]
## set_property -dict [ list CONFIG.FREQ_HZ {250000000}  ] [get_bd_intf_pins nf_riffa_dma_1/s_axi_lite]
## 
## 
## 
##   # Create port connections
##   connect_bd_net -net axi_lite_clk_1 [get_bd_pins axi_lite_aclk]  [get_bd_pins axi_interconnect_0/S00_ACLK] [get_bd_pins nf_riffa_dma_1/m_axi_lite_aclk]
## 
## 
## connect_bd_net -net M00_ACLK_i [get_bd_pins M00_ACLK] [get_bd_pins axi_interconnect_0/M00_ACLK]
## connect_bd_net -net M01_ACLK_i [get_bd_pins M01_ACLK] [get_bd_pins axi_interconnect_0/M01_ACLK]
## connect_bd_net -net M02_ACLK_i [get_bd_pins M02_ACLK] [get_bd_pins axi_interconnect_0/M02_ACLK]
## connect_bd_net -net M03_ACLK_i [get_bd_pins M03_ACLK] [get_bd_pins axi_interconnect_0/M03_ACLK]
## connect_bd_net -net M04_ACLK_i [get_bd_pins M04_ACLK] [get_bd_pins axi_interconnect_0/M04_ACLK]
## connect_bd_net -net M05_ACLK_i [get_bd_pins M05_ACLK] [get_bd_pins axi_interconnect_0/M05_ACLK]
## connect_bd_net -net M06_ACLK_i [get_bd_pins M06_ACLK] [get_bd_pins axi_interconnect_0/M06_ACLK]
## connect_bd_net -net M07_ACLK_i [get_bd_pins M07_ACLK] [get_bd_pins axi_interconnect_0/M07_ACLK]
## 
##   connect_bd_net -net axi_lite_rstn_1  [get_bd_pins axi_interconnect_0/S00_ARESETN] [get_bd_pins axi_lite_aresetn] [get_bd_pins nf_riffa_dma_1/m_axi_lite_aresetn]
## 
## 
## connect_bd_net -net M00_ARESETN_i [get_bd_pins M00_ARESETN] [get_bd_pins axi_interconnect_0/M00_ARESETN]
## connect_bd_net -net M01_ARESETN_i [get_bd_pins M01_ARESETN]  [get_bd_pins axi_interconnect_0/M01_ARESETN]
## connect_bd_net -net M02_ARESETN_i [get_bd_pins M02_ARESETN]  [get_bd_pins axi_interconnect_0/M02_ARESETN]
## connect_bd_net -net M03_ARESETN_i [get_bd_pins M03_ARESETN]  [get_bd_pins axi_interconnect_0/M03_ARESETN]
## connect_bd_net -net M04_ARESETN_i [get_bd_pins M04_ARESETN]  [get_bd_pins axi_interconnect_0/M04_ARESETN]
## connect_bd_net -net M05_ARESETN_i [get_bd_pins M05_ARESETN]  [get_bd_pins axi_interconnect_0/M05_ARESETN]
## connect_bd_net -net M06_ARESETN_i [get_bd_pins M06_ARESETN]  [get_bd_pins axi_interconnect_0/M06_ARESETN]
## connect_bd_net -net M07_ARESETN_i [get_bd_pins M07_ARESETN]  [get_bd_pins axi_interconnect_0/M07_ARESETN]
## 
##   connect_bd_net -net axis_10g_clk_1 [get_bd_pins axis_datapath_aclk] [get_bd_pins axi_clock_converter_0/s_axi_aclk] [get_bd_pins axi_interconnect_0/ACLK] [get_bd_pins axi_interconnect_0/M08_ACLK] [get_bd_pins axis_dwidth_dma_rx/aclk] [get_bd_pins axis_dwidth_dma_tx/aclk] [get_bd_pins axis_fifo_10g_rx/s_axis_aclk] [get_bd_pins axis_fifo_10g_tx/m_axis_aclk]
## 
##   connect_bd_net -net axis_rx_sys_reset_0_peripheral_aresetn [get_bd_pins axis_datapath_aresetn] [get_bd_pins axi_clock_converter_0/s_axi_aresetn] [get_bd_pins axi_interconnect_0/ARESETN] [get_bd_pins axi_interconnect_0/M08_ARESETN] [get_bd_pins axis_dwidth_dma_rx/aresetn] [get_bd_pins axis_dwidth_dma_tx/aresetn] [get_bd_pins axis_fifo_10g_rx/s_axis_aresetn] [get_bd_pins axis_fifo_10g_tx/m_axis_aresetn]
## 
##   connect_bd_net -net axis_tx_sys_reset_0_peripheral_aresetn [get_bd_pins axi_clock_converter_0/m_axi_aresetn] [get_bd_pins axis_fifo_10g_rx/m_axis_aresetn] [get_bd_pins axis_fifo_10g_tx/s_axis_aresetn] [get_bd_pins pcie_reset_inv/Res]
## 
##   connect_bd_net -net pcie3_7x_1_user_clk [get_bd_pins axi_clock_converter_0/m_axi_aclk] [get_bd_pins axis_fifo_10g_rx/m_axis_aclk] [get_bd_pins axis_fifo_10g_tx/s_axis_aclk] [get_bd_pins nf_riffa_dma_1/user_clk] [get_bd_pins pcie3_7x_1/user_clk]
## 
##   connect_bd_net -net pcie3_7x_1_user_lnk_up [get_bd_pins nf_riffa_dma_1/user_lnk_up] [get_bd_pins pcie3_7x_1/user_lnk_up]
##   connect_bd_net -net pcie3_7x_1_user_reset [get_bd_pins pcie_reset_inv/Op1] [get_bd_pins nf_riffa_dma_1/user_reset] [get_bd_pins pcie3_7x_1/user_reset]
##   connect_bd_net -net sys_clk_1 [get_bd_pins sys_clk] [get_bd_pins pcie3_7x_1/sys_clk]
##   connect_bd_net -net sys_reset_1 [get_bd_pins sys_reset] [get_bd_pins pcie3_7x_1/sys_reset]
## 
##   # Restore current instance
##   current_bd_instance $oldCurInst
## }
## proc create_root_design { parentCell } {
## 
##   if { $parentCell eq "" } {
##      set parentCell [get_bd_cells /]
##   }
## 
##   # Get object for parentCell
##   set parentObj [get_bd_cells $parentCell]
##   if { $parentObj == "" } {
##      puts "ERROR: Unable to find parent cell <$parentCell>!"
##      return
##   }
## 
##   # Make sure parentObj is hier blk
##   set parentType [get_property TYPE $parentObj]
##   if { $parentType ne "hier" } {
##      puts "ERROR: Parent <$parentObj> has TYPE = <$parentType>. Expected to be <hier>."
##      return
##   }
## 
##   # Save current instance; Restore later
##   set oldCurInst [current_bd_instance .]
## 
##   # Set parent object as current
##   current_bd_instance $parentObj
## 
## 
##   # Create interface ports
##   set M00_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M00_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M00_AXI
##   set M01_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M01_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M01_AXI
##   set M02_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M02_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M02_AXI
##   set M03_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M03_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M03_AXI
##   set M04_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M04_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M04_AXI
##   set M05_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M05_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M05_AXI
##   set M06_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M06_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M06_AXI
##   set M07_AXI [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:aximm_rtl:1.0 M07_AXI ]
##   set_property -dict [ list CONFIG.ADDR_WIDTH {12} CONFIG.DATA_WIDTH {32} CONFIG.PROTOCOL {AXI4LITE}  ] $M07_AXI
##   set iic_fpga [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:iic_rtl:1.0 iic_fpga ]
##   set m_axis_dma_tx [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:axis_rtl:1.0 m_axis_dma_tx ]
##   set pcie_7x_mgt [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:pcie_7x_mgt_rtl:1.0 pcie_7x_mgt ]
##   set s_axis_dma_rx [ create_bd_intf_port -mode Slave -vlnv xilinx.com:interface:axis_rtl:1.0 s_axis_dma_rx ]
##   set_property -dict [ list CONFIG.FREQ_HZ {100000000} CONFIG.HAS_TKEEP {1} CONFIG.HAS_TLAST {1} CONFIG.HAS_TREADY {1} CONFIG.HAS_TSTRB {0} CONFIG.LAYERED_METADATA {undef} CONFIG.PHASE {0.000} CONFIG.TDATA_NUM_BYTES {32} CONFIG.TDEST_WIDTH {0} CONFIG.TID_WIDTH {0} CONFIG.TUSER_WIDTH {128}  ] $s_axis_dma_rx
##   set uart [ create_bd_intf_port -mode Master -vlnv xilinx.com:interface:uart_rtl:1.0 uart ]
## 
##   # Create ports
##   set axi_lite_aclk [ create_bd_port -dir I -type clk axi_lite_aclk ]
##   set axi_lite_aresetn [ create_bd_port -dir I -type rst axi_lite_aresetn ]
##   set_property -dict [ list CONFIG.POLARITY {ACTIVE_LOW}] $axi_lite_aresetn
##   set axis_datapath_aclk [ create_bd_port -dir I -type clk axis_datapath_aclk ]
##   set axis_datapath_aresetn [ create_bd_port -dir I -type rst axis_datapath_aresetn ]
##   set_property -dict [ list CONFIG.POLARITY {ACTIVE_LOW}  ] $axis_datapath_aresetn
##   set iic_reset [ create_bd_port -dir O -from 1 -to 0 iic_reset ]
##   set sys_clk [ create_bd_port -dir I -type clk sys_clk ]
##   set_property -dict [ list CONFIG.FREQ_HZ {100000000}  ] $sys_clk
##   set sys_reset [ create_bd_port -dir I -type rst sys_reset ]
##   set_property -dict [ list CONFIG.POLARITY {ACTIVE_HIGH}  ] $sys_reset
## 
## 
## 
##   # Create instance: dma_sub
##   create_hier_cell_dma_sub [current_bd_instance .] dma_sub
## 
##   # Create instance: nf_mbsys
##   create_hier_cell_nf_mbsys [current_bd_instance .] nf_mbsys
## 
##   # Create interface connections
##   connect_bd_intf_net -intf_net dma_sub_M00_AXI [get_bd_intf_ports M00_AXI] [get_bd_intf_pins dma_sub/M00_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M01_AXI [get_bd_intf_ports M01_AXI] [get_bd_intf_pins dma_sub/M01_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M02_AXI [get_bd_intf_ports M02_AXI] [get_bd_intf_pins dma_sub/M02_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M03_AXI [get_bd_intf_ports M03_AXI] [get_bd_intf_pins dma_sub/M03_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M04_AXI [get_bd_intf_ports M04_AXI] [get_bd_intf_pins dma_sub/M04_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M05_AXI [get_bd_intf_ports M05_AXI] [get_bd_intf_pins dma_sub/M05_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M06_AXI [get_bd_intf_ports M06_AXI] [get_bd_intf_pins dma_sub/M06_AXI]
##   connect_bd_intf_net -intf_net dma_sub_M07_AXI [get_bd_intf_ports M07_AXI] [get_bd_intf_pins dma_sub/M07_AXI]
##   connect_bd_intf_net -intf_net dma_sub_m_axis_dma_tx [get_bd_intf_ports m_axis_dma_tx] [get_bd_intf_pins dma_sub/m_axis_dma_tx]
##   connect_bd_intf_net -intf_net dma_sub_pcie_7x_mgt [get_bd_intf_ports pcie_7x_mgt] [get_bd_intf_pins dma_sub/pcie_7x_mgt]
##   connect_bd_intf_net -intf_net nf_mbsys_iic_fpga [get_bd_intf_ports iic_fpga] [get_bd_intf_pins nf_mbsys/iic_fpga]
##   connect_bd_intf_net -intf_net nf_mbsys_uart [get_bd_intf_ports uart] [get_bd_intf_pins nf_mbsys/uart]
##   connect_bd_intf_net -intf_net s_axis_dma_rx_1 [get_bd_intf_ports s_axis_dma_rx] [get_bd_intf_pins dma_sub/s_axis_dma_rx]
## 
##   # Create port connections
##   connect_bd_net -net axi_lite_aclk_1 [get_bd_ports axi_lite_aclk] [get_bd_pins dma_sub/axi_lite_aclk]
##   connect_bd_net -net axi_lite_aresetn_1 [get_bd_ports axi_lite_aresetn] [get_bd_pins dma_sub/axi_lite_aresetn]
##   connect_bd_net -net axis_datapath_aclk_1 [get_bd_ports axis_datapath_aclk] [get_bd_pins dma_sub/axis_datapath_aclk] [get_bd_pins dma_sub/M00_ACLK] [get_bd_pins dma_sub/M01_ACLK] [get_bd_pins dma_sub/M02_ACLK] [get_bd_pins dma_sub/M03_ACLK] [get_bd_pins dma_sub/M04_ACLK] [get_bd_pins dma_sub/M05_ACLK] [get_bd_pins dma_sub/M06_ACLK] [get_bd_pins dma_sub/M07_ACLK]
##   connect_bd_net -net axis_datapath_aresetn_1 [get_bd_ports axis_datapath_aresetn] [get_bd_pins dma_sub/axis_datapath_aresetn]  [get_bd_pins dma_sub/M00_ARESETN] [get_bd_pins dma_sub/M01_ARESETN] [get_bd_pins dma_sub/M02_ARESETN] [get_bd_pins dma_sub/M03_ARESETN] [get_bd_pins dma_sub/M04_ARESETN] [get_bd_pins dma_sub/M05_ARESETN] [get_bd_pins dma_sub/M06_ARESETN] [get_bd_pins dma_sub/M07_ARESETN]
##   connect_bd_net -net nf_mbsys_iic_reset [get_bd_ports iic_reset] [get_bd_pins nf_mbsys/iic_reset]
##   connect_bd_net -net sys_clk_1 [get_bd_ports sys_clk] [get_bd_pins dma_sub/sys_clk] [get_bd_pins nf_mbsys/sysclk]
##   connect_bd_net -net sys_reset_1 [get_bd_ports sys_reset] [get_bd_pins dma_sub/sys_reset] [get_bd_pins nf_mbsys/reset]
## 
## 
##   # Create address segments
##   source ./tcl/$::env(NF_PROJECT_NAME)_defines.tcl
##   create_bd_addr_seg -range $M00_SIZEADDR -offset $M00_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M00_AXI/Reg] SEG_M00_AXI_Reg
##   create_bd_addr_seg -range $M01_SIZEADDR -offset $M01_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M01_AXI/Reg] SEG_M01_AXI_Reg
##   create_bd_addr_seg -range $M02_SIZEADDR -offset $M02_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M02_AXI/Reg] SEG_M02_AXI_Reg
##   create_bd_addr_seg -range $M03_SIZEADDR -offset $M03_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M03_AXI/Reg] SEG_M03_AXI_Reg
##   create_bd_addr_seg -range $M04_SIZEADDR -offset $M04_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M04_AXI/Reg] SEG_M04_AXI_Reg
##   create_bd_addr_seg -range $M05_SIZEADDR -offset $M05_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M05_AXI/Reg] SEG_M05_AXI_Reg
##   create_bd_addr_seg -range $M06_SIZEADDR -offset $M06_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M06_AXI/Reg] SEG_M06_AXI_Reg
##   create_bd_addr_seg -range $M07_SIZEADDR -offset $M07_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs M07_AXI/Reg] SEG_M07_AXI_Reg
##   create_bd_addr_seg -range $M08_SIZEADDR -offset $M08_BASEADDR [get_bd_addr_spaces dma_sub/nf_riffa_dma_1/m_axi_lite] [get_bd_addr_segs  dma_sub/nf_riffa_dma_1/s_axi_lite/reg0] SEG_nf_riffa_dma_1_reg0
## 
##   create_bd_addr_seg -range $MICROBLAZE_AXI_IIC_SIZEADDR -offset $MICROBLAZE_AXI_IIC_BASEADDR [get_bd_addr_spaces nf_mbsys/mbsys/microblaze_0/Data] [get_bd_addr_segs nf_mbsys/axi_iic_0/S_AXI/Reg] SEG_axi_iic_0_Reg
##   create_bd_addr_seg -range $MICROBLAZE_UARTLITE_SIZEADDR -offset $MICROBLAZE_UARTLITE_BASEADDR [get_bd_addr_spaces nf_mbsys/mbsys/microblaze_0/Data] [get_bd_addr_segs nf_mbsys/axi_uartlite_0/S_AXI/Reg] SEG_axi_uartlite_0_Reg
##   create_bd_addr_seg -range $MICROBLAZE_DLMB_BRAM_SIZEADDR -offset $MICROBLAZE_DLMB_BRAM_BASEADDR [get_bd_addr_spaces nf_mbsys/mbsys/microblaze_0/Data] [get_bd_addr_segs nf_mbsys/mbsys/microblaze_0_local_memory/dlmb_bram_if_cntlr/SLMB/Mem] SEG_dlmb_bram_if_cntlr_Mem
##   create_bd_addr_seg -range $MICROBLAZE_ILMB_BRAM_SIZEADDR -offset $MICROBLAZE_ILMB_BRAM_BASEADDR [get_bd_addr_spaces nf_mbsys/mbsys/microblaze_0/Instruction] [get_bd_addr_segs nf_mbsys/mbsys/microblaze_0_local_memory/ilmb_bram_if_cntlr/SLMB/Mem] SEG_ilmb_bram_if_cntlr_Mem
##   create_bd_addr_seg -range $MICROBLAZE_AXI_INTC_SIZEADDR -offset $MICROBLAZE_AXI_INTC_BASEADDR [get_bd_addr_spaces nf_mbsys/mbsys/microblaze_0/Data] [get_bd_addr_segs nf_mbsys/mbsys/microblaze_0_axi_intc/s_axi/Reg] SEG_microblaze_0_axi_intc_Reg
## 
## 
##   # Restore current instance
##   current_bd_instance $oldCurInst
## 
##   save_bd_design
## }
## create_root_design ""
CRITICAL WARNING: [BD 41-737] Cannot set the parameter FREQ_HZ on /dma_sub/nf_riffa_dma_1/s_axi_lite. It is read-only.
create_bd_cell: Time (s): cpu = 00:00:23 ; elapsed = 00:00:58 . Memory (MB): peak = 1703.027 ; gain = 287.730 ; free physical = 10382 ; free virtual = 15354
WARNING: [IP_Flow 19-3374] An attempt to modify the value of disabled parameter 'MMCM_CLKIN1_PERIOD' from '10.000' to '10.0' has been ignored for IP 'nf_mbsys/clk_wiz_1'
INFO: [Device 21-403] Loading part xc7vx690tffg1761-3
### set MICROBLAZE_AXI_IIC_BASEADDR 0x40800000
### set MICROBLAZE_AXI_IIC_HIGHADDR 0x4080FFFF
### set MICROBLAZE_AXI_IIC_SIZEADDR 0x10000
### set MICROBLAZE_UARTLITE_BASEADDR 0x40600000
### set MICROBLAZE_UARTLITE_HIGHADDR 0x4060FFFF
### set MICROBLAZE_UARTLITE_SIZEADDR 0x10000
### set MICROBLAZE_DLMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_DLMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_DLMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_ILMB_BRAM_BASEADDR 0x00000000
### set MICROBLAZE_ILMB_BRAM_HIGHADDR 0x0000FFFF
### set MICROBLAZE_ILMB_BRAM_SIZEADDR 0x10000
### set MICROBLAZE_AXI_INTC_BASEADDR 0x41200000
### set MICROBLAZE_AXI_INTC_HIGHADDR 0x4120FFFF
### set MICROBLAZE_AXI_INTC_SIZEADDR 0x10000
### set M00_BASEADDR 0x44000000
### set M00_HIGHADDR 0x44000FFF
### set M00_SIZEADDR 0x1000
### set M01_BASEADDR 0x44010000
### set M01_HIGHADDR 0x44010FFF
### set M01_SIZEADDR 0x1000
### set M02_BASEADDR 0x44020000
### set M02_HIGHADDR 0x44020FFF
### set M02_SIZEADDR 0x1000
### set M03_BASEADDR 0x44030000
### set M03_HIGHADDR 0x44030FFF
### set M03_SIZEADDR 0x1000
### set M04_BASEADDR 0x44040000
### set M04_HIGHADDR 0x44040FFF
### set M04_SIZEADDR 0x1000
### set M05_BASEADDR 0x44050000
### set M05_HIGHADDR 0x44050FFF
### set M05_SIZEADDR 0x1000
### set M06_BASEADDR 0x44060000
### set M06_HIGHADDR 0x44060FFF
### set M06_SIZEADDR 0x1000
### set M07_BASEADDR 0x44070000
### set M07_HIGHADDR 0x44070FFF
### set M07_SIZEADDR 0x1000
### set M08_BASEADDR 0x44080000
### set M08_HIGHADDR 0x44080FFF
### set M08_SIZEADDR 0x1000
### set IDENTIFIER_BASEADDR $M00_BASEADDR
### set IDENTIFIER_HIGHADDR $M00_HIGHADDR
### set IDENTIFIER_SIZEADDR $M00_SIZEADDR
### set INPUT_ARBITER_BASEADDR $M01_BASEADDR
### set INPUT_ARBITER_HIGHADDR $M01_HIGHADDR
### set INPUT_ARBITER_SIZEADDR $M01_SIZEADDR
### set OUTPUT_QUEUES_BASEADDR $M03_BASEADDR
### set OUTPUT_QUEUES_HIGHADDR $M03_HIGHADDR
### set OUTPUT_QUEUES_SIZEADDR $M03_SIZEADDR
### set OUTPUT_PORT_LOOKUP_BASEADDR $M02_BASEADDR
### set OUTPUT_PORT_LOOKUP_HIGHADDR $M02_HIGHADDR
### set OUTPUT_PORT_LOOKUP_SIZEADDR $M02_SIZEADDR
### set NF_10G_INTERFACE0_BASEADDR $M04_BASEADDR
### set NF_10G_INTERFACE0_HIGHADDR $M04_HIGHADDR
### set NF_10G_INTERFACE0_SIZEADDR $M04_SIZEADDR
### set NF_10G_INTERFACE1_BASEADDR $M05_BASEADDR
### set NF_10G_INTERFACE1_HIGHADDR $M05_HIGHADDR
### set NF_10G_INTERFACE1_SIZEADDR $M05_SIZEADDR
### set NF_10G_INTERFACE2_BASEADDR $M06_BASEADDR
### set NF_10G_INTERFACE2_HIGHADDR $M06_HIGHADDR
### set NF_10G_INTERFACE2_SIZEADDR $M06_SIZEADDR
### set NF_10G_INTERFACE3_BASEADDR $M07_BASEADDR
### set NF_10G_INTERFACE3_HIGHADDR $M07_HIGHADDR
### set NF_10G_INTERFACE3_SIZEADDR $M07_SIZEADDR
### set NF_RIFFA_DMA_BASEADDR $M08_BASEADDR
### set NF_RIFFA_DMA_HIGHADDR $M08_HIGHADDR
### set NF_RIFFA_DMA_SIZEADDR $M08_SIZEADDR
Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd> 
# create_ip -name nf_sume_sdnet -vendor NetFPGA -library NetFPGA -module_name nf_sume_sdnet_ip
# set_property generate_synth_checkpoint false [get_files nf_sume_sdnet_ip.xci]
# reset_target all [get_ips nf_sume_sdnet_ip]
# generate_target all [get_ips nf_sume_sdnet_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'nf_sume_sdnet_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'nf_sume_sdnet_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'nf_sume_sdnet_ip'...
# source ./create_ip/nf_10ge_interface.tcl
## set sharedLogic          "FALSE"
## set tdataWidth           256
## set convWidth [expr $tdataWidth/8]
## if { $sharedLogic eq "True" || $sharedLogic eq "TRUE" || $sharedLogic eq "true" } {
##    set supportLevel 1
## } else {
##    set supportLevel 0
## }
## create_ip -name axi_10g_ethernet -vendor xilinx.com -library ip -version 3.1 -module_name axi_10g_ethernet_nonshared
WARNING: [IP_Flow 19-4832] The IP name 'axi_10g_ethernet_nonshared' you have specified is long. The Windows operating system has path length limitations. It is recommended you use shorter names to reduce the likelihood of issues.
## set_property -dict [list CONFIG.Management_Interface {false}] [get_ips axi_10g_ethernet_nonshared]
WARNING: [BD 5-233] No interface ports matched 'get_bd_intf_ports -filter {Mode=="Slave" && VLNV=="xilinx.com:interface:aximm_rtl:1.0"}'
## set_property -dict [list CONFIG.base_kr {BASE-R}] [get_ips axi_10g_ethernet_nonshared]
WARNING: [BD 5-233] No interface ports matched 'get_bd_intf_ports -filter {Mode=="Slave" && VLNV=="xilinx.com:interface:aximm_rtl:1.0"}'
## set_property -dict [list CONFIG.SupportLevel $supportLevel] [get_ips axi_10g_ethernet_nonshared]
## set_property -dict [list CONFIG.autonegotiation {0}] [get_ips axi_10g_ethernet_nonshared]
## set_property -dict [list CONFIG.fec {0}] [get_ips axi_10g_ethernet_nonshared]
## set_property -dict [list CONFIG.Statistics_Gathering {0}] [get_ips axi_10g_ethernet_nonshared]
## set_property generate_synth_checkpoint false [get_files axi_10g_ethernet_nonshared.xci]
## reset_target all [get_ips axi_10g_ethernet_nonshared]
## generate_target all [get_ips axi_10g_ethernet_nonshared]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axi_10g_ethernet_nonshared'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axi_10g_ethernet_nonshared'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axi_10g_ethernet_nonshared'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'axi_10g_ethernet_nonshared'...
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
Exporting to file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_10g_ethernet_nonshared/bd_0/hw_handoff/axi_10g_ethernet_nonshared.hwh
Generated Block Design Tcl file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_10g_ethernet_nonshared/bd_0/hw_handoff/axi_10g_ethernet_nonshared_bd.tcl
Generated Hardware Definition File /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_10g_ethernet_nonshared/bd_0/synth/axi_10g_ethernet_nonshared.hwdef
generate_target: Time (s): cpu = 00:00:06 ; elapsed = 00:00:09 . Memory (MB): peak = 1942.422 ; gain = 43.977 ; free physical = 10123 ; free virtual = 15139
## create_ip -name fifo_generator -vendor xilinx.com -library ip -version 13.2 -module_name fifo_generator_status
## set_property -dict [list CONFIG.Fifo_Implementation {Independent_Clocks_Block_RAM}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Performance_Options {First_Word_Fall_Through}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Input_Data_Width {458} CONFIG.Input_Depth {16}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Reset_Pin {false}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Output_Data_Width {458} CONFIG.Output_Depth {16}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Full_Flags_Reset_Value {0}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Use_Dout_Reset {false}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Data_Count_Width {4}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Write_Data_Count_Width {4}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Read_Data_Count_Width {4}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Full_Threshold_Assert_Value {15}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Full_Threshold_Negate_Value {14}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Empty_Threshold_Assert_Value {4}] [get_ips fifo_generator_status]
## set_property -dict [list CONFIG.Empty_Threshold_Negate_Value {5}] [get_ips fifo_generator_status]
## set_property generate_synth_checkpoint false [get_files fifo_generator_status.xci]
## reset_target all [get_ips fifo_generator_status]
## generate_target all [get_ips fifo_generator_status]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'fifo_generator_status'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'fifo_generator_status'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'fifo_generator_status'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'fifo_generator_status'...
## create_ip -name util_vector_logic -vendor xilinx.com -library ip -version 2.0 -module_name inverter_0
WARNING: [Coretcl 2-1618] The 'xilinx.com:ip:util_vector_logic:2.0' IP is intended for use in IPI only.
## set_property -dict [list CONFIG.C_SIZE {1}] [get_ips inverter_0]
## set_property -dict [list CONFIG.C_OPERATION {not}] [get_ips inverter_0]
## set_property generate_synth_checkpoint false [get_files inverter_0.xci]
## reset_target all [get_ips inverter_0]
## generate_target all [get_ips inverter_0]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'inverter_0'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'inverter_0'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'inverter_0'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'inverter_0'...
## create_ip -name fifo_generator -vendor xilinx.com -library ip -version 13.2 -module_name fifo_generator_1_9
## set_property -dict [list CONFIG.Fifo_Implementation {Independent_Clocks_Block_RAM} CONFIG.Performance_Options {First_Word_Fall_Through} CONFIG.Input_Data_Width {1} CONFIG.Input_Depth {16} CONFIG.Output_Data_Width {1} CONFIG.Output_Depth {16} CONFIG.Data_Count_Width {4} CONFIG.Write_Data_Count_Width {4} CONFIG.Read_Data_Count_Width {4} CONFIG.Full_Threshold_Assert_Value {13} CONFIG.Full_Threshold_Negate_Value {12}] [get_ips fifo_generator_1_9]
WARNING: [IP_Flow 19-3374] An attempt to modify the value of disabled parameter 'Full_Threshold_Assert_Value' from '15' to '13' has been ignored for IP 'fifo_generator_1_9'
WARNING: [IP_Flow 19-3374] An attempt to modify the value of disabled parameter 'Full_Threshold_Negate_Value' from '14' to '12' has been ignored for IP 'fifo_generator_1_9'
## set_property generate_synth_checkpoint false [get_files fifo_generator_1_9.xci]
## reset_target all [get_ips fifo_generator_1_9]
## generate_target all [get_ips fifo_generator_1_9]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'fifo_generator_1_9'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'fifo_generator_1_9'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'fifo_generator_1_9'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'fifo_generator_1_9'...
# create_ip -name nf_10ge_interface -vendor NetFPGA -library NetFPGA -module_name nf_10g_interface_ip
# set_property generate_synth_checkpoint false [get_files nf_10g_interface_ip.xci]
# reset_target all [get_ips nf_10g_interface_ip]
# generate_target all [get_ips nf_10g_interface_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'nf_10g_interface_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'nf_10g_interface_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'nf_10g_interface_ip'...
generate_target: Time (s): cpu = 00:00:10 ; elapsed = 00:00:16 . Memory (MB): peak = 1986.980 ; gain = 37.527 ; free physical = 10044 ; free virtual = 15124
# source ./create_ip/nf_10ge_interface_shared.tcl
## set sharedLogic         "TRUE"
## set tdataWidth          256
## set convWidth [expr $tdataWidth/8]
## if { $sharedLogic eq "True" || $sharedLogic eq "TRUE" || $sharedLogic eq "true" } {
##    set supportLevel 1
## } else {
##    set supportLevel 0
## }
## create_ip -name axi_10g_ethernet -vendor xilinx.com -library ip -version 3.1 -module_name axi_10g_ethernet_shared
## set_property -dict [list CONFIG.Management_Interface {false}] [get_ips axi_10g_ethernet_shared]
WARNING: [BD 5-233] No interface ports matched 'get_bd_intf_ports -filter {Mode=="Slave" && VLNV=="xilinx.com:interface:aximm_rtl:1.0"}'
## set_property -dict [list CONFIG.base_kr {BASE-R}] [get_ips axi_10g_ethernet_shared]
WARNING: [BD 5-233] No interface ports matched 'get_bd_intf_ports -filter {Mode=="Slave" && VLNV=="xilinx.com:interface:aximm_rtl:1.0"}'
## set_property -dict [list CONFIG.SupportLevel $supportLevel] [get_ips axi_10g_ethernet_shared]
WARNING: [BD 41-1306] The connection to interface pin /xpcs/refclk_p is being overridden by the user. This pin will not be connected as a part of interface connection refclk_diff_port
WARNING: [BD 41-1306] The connection to interface pin /xpcs/refclk_n is being overridden by the user. This pin will not be connected as a part of interface connection refclk_diff_port
WARNING: [BD 5-233] No interface ports matched 'get_bd_intf_ports -filter {Mode=="Slave" && VLNV=="xilinx.com:interface:aximm_rtl:1.0"}'
## set_property -dict [list CONFIG.autonegotiation {0}] [get_ips axi_10g_ethernet_shared]
## set_property -dict [list CONFIG.fec {0}] [get_ips axi_10g_ethernet_shared]
## set_property -dict [list CONFIG.Statistics_Gathering {0}] [get_ips axi_10g_ethernet_shared]
## set_property generate_synth_checkpoint false [get_files axi_10g_ethernet_shared.xci]
## reset_target all [get_ips axi_10g_ethernet_shared]
## generate_target all [get_ips axi_10g_ethernet_shared]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'axi_10g_ethernet_shared'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'axi_10g_ethernet_shared'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'axi_10g_ethernet_shared'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'axi_10g_ethernet_shared'...
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
WARNING: [IP_Flow 19-650] IP license key 'ten_gig_eth_pcs_pma_basekr@2015.04' is enabled with a Design_Linking license.
Exporting to file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_10g_ethernet_shared/bd_0/hw_handoff/axi_10g_ethernet_shared.hwh
Generated Block Design Tcl file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_10g_ethernet_shared/bd_0/hw_handoff/axi_10g_ethernet_shared_bd.tcl
Generated Hardware Definition File /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/axi_10g_ethernet_shared/bd_0/synth/axi_10g_ethernet_shared.hwdef
generate_target: Time (s): cpu = 00:00:06 ; elapsed = 00:00:09 . Memory (MB): peak = 2002.312 ; gain = 15.328 ; free physical = 9994 ; free virtual = 15074
# create_ip -name nf_10ge_interface_shared -vendor NetFPGA -library NetFPGA -module_name nf_10g_interface_shared_ip
WARNING: [IP_Flow 19-4832] The IP name 'nf_10g_interface_shared_ip' you have specified is long. The Windows operating system has path length limitations. It is recommended you use shorter names to reduce the likelihood of issues.
# set_property generate_synth_checkpoint false [get_files nf_10g_interface_shared_ip.xci]
# reset_target all [get_ips nf_10g_interface_shared_ip]
# generate_target all [get_ips nf_10g_interface_shared_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'nf_10g_interface_shared_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'nf_10g_interface_shared_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'nf_10g_interface_shared_ip'...
generate_target: Time (s): cpu = 00:00:09 ; elapsed = 00:00:16 . Memory (MB): peak = 2039.840 ; gain = 37.527 ; free physical = 9974 ; free virtual = 15073
# create_ip -name clk_wiz -vendor xilinx.com -library ip -version 6.0 -module_name clk_wiz_ip
# set_property -dict [list CONFIG.PRIM_IN_FREQ {200.00} CONFIG.CLKOUT1_REQUESTED_OUT_FREQ {200.000} CONFIG.USE_SAFE_CLOCK_STARTUP {true} CONFIG.RESET_TYPE {ACTIVE_LOW} CONFIG.CLKIN1_JITTER_PS {50.0} CONFIG.CLKOUT1_DRIVES {BUFGCE} CONFIG.CLKOUT2_DRIVES {BUFGCE} CONFIG.CLKOUT3_DRIVES {BUFGCE} CONFIG.CLKOUT4_DRIVES {BUFGCE} CONFIG.CLKOUT5_DRIVES {BUFGCE} CONFIG.CLKOUT6_DRIVES {BUFGCE} CONFIG.CLKOUT7_DRIVES {BUFGCE} CONFIG.MMCM_CLKFBOUT_MULT_F {5.000} CONFIG.MMCM_CLKIN1_PERIOD {5.0} CONFIG.MMCM_CLKOUT0_DIVIDE_F {5.000} CONFIG.RESET_PORT {resetn} CONFIG.CLKOUT1_JITTER {98.146} CONFIG.CLKOUT1_PHASE_ERROR {89.971}] [get_ips clk_wiz_ip]
WARNING: [IP_Flow 19-3374] An attempt to modify the value of disabled parameter 'MMCM_CLKIN1_PERIOD' from '5.000' to '5.0' has been ignored for IP 'clk_wiz_ip'
# set_property generate_synth_checkpoint false [get_files clk_wiz_ip.xci]
# reset_target all [get_ips clk_wiz_ip]
# generate_target all [get_ips clk_wiz_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Implementation' target for IP 'clk_wiz_ip'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'clk_wiz_ip'...
# create_ip -name proc_sys_reset -vendor xilinx.com -library ip -version 5.0 -module_name proc_sys_reset_ip
# set_property -dict [list CONFIG.C_EXT_RESET_HIGH {0} CONFIG.C_AUX_RESET_HIGH {0}] [get_ips proc_sys_reset_ip]
# set_property -dict [list CONFIG.C_NUM_PERP_RST {1} CONFIG.C_NUM_PERP_ARESETN {1}] [get_ips proc_sys_reset_ip]
# set_property generate_synth_checkpoint false [get_files proc_sys_reset_ip.xci]
# reset_target all [get_ips proc_sys_reset_ip]
# generate_target all [get_ips proc_sys_reset_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'proc_sys_reset_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'proc_sys_reset_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'proc_sys_reset_ip'...
INFO: [IP_Flow 19-1686] Generating 'Implementation' target for IP 'proc_sys_reset_ip'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'proc_sys_reset_ip'...
# create_ip -name blk_mem_gen -vendor xilinx.com -library ip -version 8.4 -module_name identifier_ip
# set_property -dict [list CONFIG.Interface_Type {AXI4} CONFIG.AXI_Type {AXI4_Lite} CONFIG.AXI_Slave_Type {Memory_Slave} CONFIG.Use_AXI_ID {false} CONFIG.Load_Init_File {true} CONFIG.Coe_File {/../../../../../../create_ip/id_rom16x32.coe} CONFIG.Fill_Remaining_Memory_Locations {true} CONFIG.Remaining_Memory_Locations {DEADDEAD} CONFIG.Memory_Type {Simple_Dual_Port_RAM} CONFIG.Use_Byte_Write_Enable {true} CONFIG.Byte_Size {8} CONFIG.Assume_Synchronous_Clk {true} CONFIG.Write_Width_A {32} CONFIG.Write_Depth_A {4096} CONFIG.Read_Width_A {32} CONFIG.Operating_Mode_A {READ_FIRST} CONFIG.Write_Width_B {32} CONFIG.Read_Width_B {32} CONFIG.Operating_Mode_B {READ_FIRST} CONFIG.Enable_B {Use_ENB_Pin} CONFIG.Register_PortA_Output_of_Memory_Primitives {false} CONFIG.Register_PortB_Output_of_Memory_Primitives {false} CONFIG.Use_RSTB_Pin {true} CONFIG.Reset_Type {ASYNC} CONFIG.Port_A_Write_Rate {50} CONFIG.Port_B_Clock {100} CONFIG.Port_B_Enable_Rate {100}] [get_ips identifier_ip]
# set_property generate_synth_checkpoint false [get_files identifier_ip.xci]
# reset_target all [get_ips identifier_ip]
# generate_target all [get_ips identifier_ip]
INFO: [IP_Flow 19-1686] Generating 'Instantiation Template' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Synthesis' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Simulation' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Miscellaneous' target for IP 'identifier_ip'...
INFO: [IP_Flow 19-1686] Generating 'Change Log' target for IP 'identifier_ip'...
# read_verilog "./hdl/axi_clocking.v"
# read_verilog "./hdl/nf_datapath.v"
# read_verilog "./hdl/top.v"
# create_run -flow {Vivado Synthesis 2018} synth
Run is defaulting to srcset: sources_1
Run is defaulting to constrset: constraints
Run is defaulting to part: xc7vx690tffg1761-3
# create_run impl -parent_run synth -flow {Vivado Implementation 2018} 
Run is defaulting to parent run srcset: sources_1
Run is defaulting to parent run constrset: constraints
Run is defaulting to parent run part: xc7vx690tffg1761-3
# set_property steps.phys_opt_design.is_enabled true [get_runs impl_1]
# set_property STEPS.PHYS_OPT_DESIGN.ARGS.DIRECTIVE ExploreWithHoldFix [get_runs impl_1]
# set_property STEPS.PLACE_DESIGN.ARGS.DIRECTIVE Explore [get_runs impl_1]
# set_property STEPS.POST_ROUTE_PHYS_OPT_DESIGN.is_enabled true [get_runs impl_1]
# set_property STEPS.POST_ROUTE_PHYS_OPT_DESIGN.ARGS.DIRECTIVE AggressiveExplore [get_runs impl_1]
# set_property SEVERITY {Warning} [get_drc_checks UCIO-1]
# launch_runs synth
INFO: [xilinx.com:ip:axi_intc:4.1-1] /nf_mbsys/mbsys/microblaze_0_axi_intc: The AXI INTC core has been configured to operate with synchronous clocks.
INFO: [xilinx.com:ip:axi_intc:4.1-1] /nf_mbsys/mbsys/microblaze_0_axi_intc: The AXI INTC core has been configured to operate with synchronous clocks.
CRITICAL WARNING: [BD 41-759] The input pins (listed below) are either not connected or do not have a source port, and they don't have a tie-off specified. These pins are tied-off to all 0's to avoid error in Implementation flow.
Please check your design and connect them as needed: 
/dma_sub/nf_riffa_dma_1/cfg_interrupt_sent

Wrote  : </home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/control_sub.bd> 
VHDL Output written to : /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/synth/control_sub.v
VHDL Output written to : /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/sim/control_sub.v
VHDL Output written to : /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/hdl/control_sub_wrapper.v
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/axi_iic_0 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/axi_uartlite_0 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/clk_wiz_1 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/mdm_1 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_axi_intc .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_xlconcat .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/rst_clk_wiz_1_100M .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_local_memory/dlmb_bram_if_cntlr .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_local_memory/dlmb_v10 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_local_memory/ilmb_bram_if_cntlr .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_local_memory/ilmb_v10 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_local_memory/lmb_bram .
INFO: [BD 41-1029] Generation completed for the IP Integrator block nf_mbsys/mbsys/microblaze_0_axi_periph/xbar .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/pcie_reset_inv .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axis_dwidth_dma_tx .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axis_dwidth_dma_rx .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axis_fifo_10g_rx .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axis_fifo_10g_tx .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/nf_riffa_dma_1 .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_axi_clock_converter_0_0/control_sub_axi_clock_converter_0_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_clock_converter_0 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/pcie3_7x_1 .
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/xbar .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m08_data_fifo_0/control_sub_m08_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m08_couplers/m08_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m07_data_fifo_0/control_sub_m07_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m07_couplers/m07_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m06_data_fifo_0/control_sub_m06_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m06_couplers/m06_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m05_data_fifo_0/control_sub_m05_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m05_couplers/m05_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m04_data_fifo_0/control_sub_m04_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m04_couplers/m04_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m03_data_fifo_0/control_sub_m03_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m03_couplers/m03_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m02_data_fifo_0/control_sub_m02_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m02_couplers/m02_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m01_data_fifo_0/control_sub_m01_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m01_couplers/m01_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_m00_data_fifo_0/control_sub_m00_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/m00_couplers/m00_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_s00_data_fifo_0/control_sub_s00_data_fifo_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/s00_couplers/s00_data_fifo .
WARNING: [IP_Flow 19-4994] Overwriting existing constraint file '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/ip/control_sub_auto_cc_0/control_sub_auto_cc_0_ooc.xdc'
INFO: [BD 41-1029] Generation completed for the IP Integrator block dma_sub/axi_interconnect_0/s00_couplers/auto_cc .
Exporting to file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/hw_handoff/control_sub.hwh
Generated Block Design Tcl file /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/hw_handoff/control_sub_bd.tcl
Generated Hardware Definition File /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/bd/control_sub/synth/control_sub.hwdef
[Sat Jul 13 19:45:37 2019] Launched control_sub_m07_data_fifo_0_synth_1, control_sub_mdm_1_0_synth_1, control_sub_clk_wiz_1_0_synth_1, control_sub_axi_uartlite_0_0_synth_1, control_sub_axi_iic_0_0_synth_1, control_sub_ilmb_v10_0_synth_1, control_sub_lmb_bram_0_synth_1, control_sub_xbar_1_synth_1, control_sub_pcie_reset_inv_0_synth_1, control_sub_axis_dwidth_dma_tx_0_synth_1, control_sub_axis_dwidth_dma_rx_0_synth_1, control_sub_axis_fifo_10g_rx_0_synth_1, control_sub_axis_fifo_10g_tx_0_synth_1, control_sub_nf_riffa_dma_1_0_synth_1, control_sub_axi_clock_converter_0_0_synth_1, control_sub_pcie3_7x_1_0_synth_1, control_sub_xbar_0_synth_1, control_sub_microblaze_0_0_synth_1, control_sub_microblaze_0_axi_intc_0_synth_1, control_sub_microblaze_0_xlconcat_0_synth_1, control_sub_rst_clk_wiz_1_100M_0_synth_1, control_sub_dlmb_bram_if_cntlr_0_synth_1, control_sub_dlmb_v10_0_synth_1, control_sub_ilmb_bram_if_cntlr_0_synth_1, control_sub_m05_data_fifo_0_synth_1, control_sub_m04_data_fifo_0_synth_1, control_sub_m03_data_fifo_0_synth_1, control_sub_m02_data_fifo_0_synth_1, control_sub_m01_data_fifo_0_synth_1, control_sub_m00_data_fifo_0_synth_1, control_sub_s00_data_fifo_0_synth_1, control_sub_auto_cc_0_synth_1, control_sub_m08_data_fifo_0_synth_1, control_sub_m06_data_fifo_0_synth_1...
Run output will be captured here:
control_sub_m07_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m07_data_fifo_0_synth_1/runme.log
control_sub_mdm_1_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_mdm_1_0_synth_1/runme.log
control_sub_clk_wiz_1_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_clk_wiz_1_0_synth_1/runme.log
control_sub_axi_uartlite_0_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_uartlite_0_0_synth_1/runme.log
control_sub_axi_iic_0_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_iic_0_0_synth_1/runme.log
control_sub_ilmb_v10_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_ilmb_v10_0_synth_1/runme.log
control_sub_lmb_bram_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_lmb_bram_0_synth_1/runme.log
control_sub_xbar_1_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_xbar_1_synth_1/runme.log
control_sub_pcie_reset_inv_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_pcie_reset_inv_0_synth_1/runme.log
control_sub_axis_dwidth_dma_tx_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axis_dwidth_dma_tx_0_synth_1/runme.log
control_sub_axis_dwidth_dma_rx_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axis_dwidth_dma_rx_0_synth_1/runme.log
control_sub_axis_fifo_10g_rx_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axis_fifo_10g_rx_0_synth_1/runme.log
control_sub_axis_fifo_10g_tx_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axis_fifo_10g_tx_0_synth_1/runme.log
control_sub_nf_riffa_dma_1_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_nf_riffa_dma_1_0_synth_1/runme.log
control_sub_axi_clock_converter_0_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_axi_clock_converter_0_0_synth_1/runme.log
control_sub_pcie3_7x_1_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_pcie3_7x_1_0_synth_1/runme.log
control_sub_xbar_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_xbar_0_synth_1/runme.log
control_sub_microblaze_0_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_0_synth_1/runme.log
control_sub_microblaze_0_axi_intc_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_axi_intc_0_synth_1/runme.log
control_sub_microblaze_0_xlconcat_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_microblaze_0_xlconcat_0_synth_1/runme.log
control_sub_rst_clk_wiz_1_100M_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_rst_clk_wiz_1_100M_0_synth_1/runme.log
control_sub_dlmb_bram_if_cntlr_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_dlmb_bram_if_cntlr_0_synth_1/runme.log
control_sub_dlmb_v10_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_dlmb_v10_0_synth_1/runme.log
control_sub_ilmb_bram_if_cntlr_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_ilmb_bram_if_cntlr_0_synth_1/runme.log
control_sub_m05_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m05_data_fifo_0_synth_1/runme.log
control_sub_m04_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m04_data_fifo_0_synth_1/runme.log
control_sub_m03_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m03_data_fifo_0_synth_1/runme.log
control_sub_m02_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m02_data_fifo_0_synth_1/runme.log
control_sub_m01_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m01_data_fifo_0_synth_1/runme.log
control_sub_m00_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m00_data_fifo_0_synth_1/runme.log
control_sub_s00_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_s00_data_fifo_0_synth_1/runme.log
control_sub_auto_cc_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_auto_cc_0_synth_1/runme.log
control_sub_m08_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m08_data_fifo_0_synth_1/runme.log
control_sub_m06_data_fifo_0_synth_1: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/control_sub_m06_data_fifo_0_synth_1/runme.log
[Sat Jul 13 19:45:37 2019] Launched synth...
Run output will be captured here: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/synth/runme.log
launch_runs: Time (s): cpu = 00:00:13 ; elapsed = 00:00:15 . Memory (MB): peak = 2864.801 ; gain = 824.957 ; free physical = 9752 ; free virtual = 14927
# wait_on_run synth
[Sat Jul 13 19:45:37 2019] Waiting for synth to finish...

*** Running vivado
    with args -log top.vds -m64 -product Vivado -mode batch -messageDb vivado.pb -notrace -source top.tcl


****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source top.tcl -notrace
Command: synth_design -top top -part xc7vx690tffg1761-3
Starting synth_design
WARNING: [Vivado_Tcl 4-393] The 'Synthesis' target of the following IPs are stale, please generate the output products using the generate_target or synth_ip command before running synth_design.
/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/identifier_ip/identifier_ip.xci

Attempting to get a license for feature 'Synthesis' and/or device 'xc7vx690t'
INFO: [Common 17-349] Got license for feature 'Synthesis' and/or device 'xc7vx690t'
INFO: Launching helper process for spawning children vivado processes
INFO: Helper process launched with PID 30469 
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_single [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:153]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_gray [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:284]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_handshake [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:469]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_pulse [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:715]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_array_single [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:903]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_sync_rst [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:1055]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_cdc_async_rst [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:1171]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_base [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_rst [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1478]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_counter_updn [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_reg_vec [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1733]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_reg_bit [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1755]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_reg_pipe_bit [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1774]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_sync [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_async [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_fifo_axis [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:2076]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_base [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
WARNING: [Synth 8-2490] overwriting previous definition of module asym_bwe_bb [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:6541]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_dpdistram [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:6600]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_dprom [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:6734]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_sdpram [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:6888]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_spram [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:7043]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_sprom [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:7189]
WARNING: [Synth 8-2490] overwriting previous definition of module xpm_memory_tdpram [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:7325]
WARNING: [Synth 8-2507] parameter declaration becomes local in small_fifo with formal parameter declaration list [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/small_fifo.v:67]
WARNING: [Synth 8-2507] parameter declaration becomes local in sss_small_fifo with formal parameter declaration list [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_small_fifo.v:69]
WARNING: [Synth 8-2306] macro REG_ID_DEFAULT redefined [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/sss_output_queues_ip/hdl/sss_output_queues_cpu_regs_defines.v:44]
WARNING: [Synth 8-2306] macro REG_ID_DEFAULT redefined [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_10g_interface_ip/hdl/nf_10g_interface_cpu_regs_defines.v:44]
WARNING: [Synth 8-2306] macro REG_PKTIN_ADDR redefined [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_10g_interface_ip/hdl/nf_10g_interface_cpu_regs_defines.v:75]
WARNING: [Synth 8-2306] macro REG_PKTOUT_ADDR redefined [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_10g_interface_ip/hdl/nf_10g_interface_cpu_regs_defines.v:80]
---------------------------------------------------------------------------------
Starting RTL Elaboration : Time (s): cpu = 00:00:10 ; elapsed = 00:00:24 . Memory (MB): peak = 1470.590 ; gain = 149.371 ; free physical = 9162 ; free virtual = 14464
---------------------------------------------------------------------------------
INFO: [Synth 8-6157] synthesizing module 'top' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:43]
	Parameter C_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_TUSER_WIDTH bound to: 128 - type: integer 
	Parameter IF_SFP0 bound to: 8'b00000001 
	Parameter IF_SFP1 bound to: 8'b00000100 
	Parameter IF_SFP2 bound to: 8'b00010000 
	Parameter IF_SFP3 bound to: 8'b01000000 
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:152]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:153]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:154]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:155]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:156]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:157]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:166]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:167]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:168]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:169]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:170]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:171]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:180]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:181]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:182]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:183]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:184]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:185]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:194]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:195]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:196]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:197]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:198]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:199]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:259]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:260]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:261]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:262]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:263]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:264]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:265]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:266]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:267]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:268]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:269]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:270]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:271]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:272]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:273]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:274]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:275]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:276]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:277]
INFO: [Synth 8-5534] Detected attribute (* ASYNC_REG = "TRUE" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:431]
INFO: [Synth 8-6157] synthesizing module 'OBUF' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:27275]
	Parameter CAPACITANCE bound to: DONT_CARE - type: string 
	Parameter DRIVE bound to: 12 - type: integer 
	Parameter IOSTANDARD bound to: DEFAULT - type: string 
	Parameter SLEW bound to: SLOW - type: string 
INFO: [Synth 8-6155] done synthesizing module 'OBUF' (1#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:27275]
INFO: [Synth 8-6157] synthesizing module 'IBUF' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:19473]
	Parameter CAPACITANCE bound to: DONT_CARE - type: string 
	Parameter IBUF_DELAY_VALUE bound to: 0 - type: string 
	Parameter IBUF_LOW_PWR bound to: TRUE - type: string 
	Parameter IFD_DELAY_VALUE bound to: AUTO - type: string 
	Parameter IOSTANDARD bound to: DEFAULT - type: string 
INFO: [Synth 8-6155] done synthesizing module 'IBUF' (2#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:19473]
INFO: [Synth 8-6157] synthesizing module 'IBUFDS_GTE2' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:19625]
	Parameter CLKCM_CFG bound to: TRUE - type: string 
	Parameter CLKRCV_TRST bound to: TRUE - type: string 
	Parameter CLKSWING_CFG bound to: 2'b11 
INFO: [Synth 8-6155] done synthesizing module 'IBUFDS_GTE2' (3#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:19625]
INFO: [Synth 8-6157] synthesizing module 'IOBUF' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:22660]
	Parameter DRIVE bound to: 12 - type: integer 
	Parameter IBUF_LOW_PWR bound to: TRUE - type: string 
	Parameter IOSTANDARD bound to: DEFAULT - type: string 
	Parameter SLEW bound to: SLOW - type: string 
INFO: [Synth 8-6155] done synthesizing module 'IOBUF' (4#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:22660]
INFO: [Synth 8-6157] synthesizing module 'axi_clocking' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/axi_clocking.v:44]
INFO: [Synth 8-6157] synthesizing module 'IBUFDS' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:19488]
	Parameter CAPACITANCE bound to: DONT_CARE - type: string 
	Parameter DIFF_TERM bound to: FALSE - type: string 
	Parameter DQS_BIAS bound to: FALSE - type: string 
	Parameter IBUF_DELAY_VALUE bound to: 0 - type: string 
	Parameter IBUF_LOW_PWR bound to: TRUE - type: string 
	Parameter IFD_DELAY_VALUE bound to: AUTO - type: string 
	Parameter IOSTANDARD bound to: DEFAULT - type: string 
INFO: [Synth 8-6155] done synthesizing module 'IBUFDS' (5#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:19488]
INFO: [Synth 8-6157] synthesizing module 'clk_wiz_ip' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip.v:70]
INFO: [Synth 8-6157] synthesizing module 'clk_wiz_ip_clk_wiz' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip_clk_wiz.v:68]
INFO: [Synth 8-5534] Detected attribute (* KEEP = "TRUE" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip_clk_wiz.v:126]
INFO: [Synth 8-5534] Detected attribute (* ASYNC_REG = "TRUE" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip_clk_wiz.v:126]
INFO: [Synth 8-6157] synthesizing module 'MMCME2_ADV' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:25762]
	Parameter BANDWIDTH bound to: OPTIMIZED - type: string 
	Parameter CLKFBOUT_MULT_F bound to: 5.000000 - type: float 
	Parameter CLKFBOUT_PHASE bound to: 0.000000 - type: float 
	Parameter CLKFBOUT_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKIN1_PERIOD bound to: 5.000000 - type: float 
	Parameter CLKIN2_PERIOD bound to: 0.000000 - type: float 
	Parameter CLKOUT0_DIVIDE_F bound to: 5.000000 - type: float 
	Parameter CLKOUT0_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT0_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT0_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKOUT1_DIVIDE bound to: 1 - type: integer 
	Parameter CLKOUT1_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT1_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT1_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKOUT2_DIVIDE bound to: 1 - type: integer 
	Parameter CLKOUT2_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT2_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT2_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKOUT3_DIVIDE bound to: 1 - type: integer 
	Parameter CLKOUT3_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT3_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT3_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKOUT4_CASCADE bound to: FALSE - type: string 
	Parameter CLKOUT4_DIVIDE bound to: 1 - type: integer 
	Parameter CLKOUT4_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT4_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT4_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKOUT5_DIVIDE bound to: 1 - type: integer 
	Parameter CLKOUT5_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT5_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT5_USE_FINE_PS bound to: FALSE - type: string 
	Parameter CLKOUT6_DIVIDE bound to: 1 - type: integer 
	Parameter CLKOUT6_DUTY_CYCLE bound to: 0.500000 - type: float 
	Parameter CLKOUT6_PHASE bound to: 0.000000 - type: float 
	Parameter CLKOUT6_USE_FINE_PS bound to: FALSE - type: string 
	Parameter COMPENSATION bound to: ZHOLD - type: string 
	Parameter DIVCLK_DIVIDE bound to: 1 - type: integer 
	Parameter IS_CLKINSEL_INVERTED bound to: 1'b0 
	Parameter IS_PSEN_INVERTED bound to: 1'b0 
	Parameter IS_PSINCDEC_INVERTED bound to: 1'b0 
	Parameter IS_PWRDWN_INVERTED bound to: 1'b0 
	Parameter IS_RST_INVERTED bound to: 1'b0 
	Parameter REF_JITTER1 bound to: 0.010000 - type: float 
	Parameter REF_JITTER2 bound to: 0.010000 - type: float 
	Parameter SS_EN bound to: FALSE - type: string 
	Parameter SS_MODE bound to: CENTER_HIGH - type: string 
	Parameter SS_MOD_PERIOD bound to: 10000 - type: integer 
	Parameter STARTUP_WAIT bound to: FALSE - type: string 
INFO: [Synth 8-6155] done synthesizing module 'MMCME2_ADV' (6#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:25762]
INFO: [Synth 8-6157] synthesizing module 'BUFG' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:609]
INFO: [Synth 8-6155] done synthesizing module 'BUFG' (7#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:609]
INFO: [Synth 8-6157] synthesizing module 'BUFGCE' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:619]
	Parameter CE_TYPE bound to: SYNC - type: string 
	Parameter IS_CE_INVERTED bound to: 1'b0 
	Parameter IS_I_INVERTED bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'BUFGCE' (8#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:619]
INFO: [Synth 8-6157] synthesizing module 'BUFH' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:808]
INFO: [Synth 8-6155] done synthesizing module 'BUFH' (9#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:808]
INFO: [Synth 8-6155] done synthesizing module 'clk_wiz_ip_clk_wiz' (10#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip_clk_wiz.v:68]
INFO: [Synth 8-6155] done synthesizing module 'clk_wiz_ip' (11#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/clk_wiz_ip/clk_wiz_ip.v:70]
INFO: [Synth 8-6155] done synthesizing module 'axi_clocking' (12#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/axi_clocking.v:44]
INFO: [Synth 8-638] synthesizing module 'proc_sys_reset_ip' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/synth/proc_sys_reset_ip.vhd:74]
	Parameter C_FAMILY bound to: virtex7 - type: string 
	Parameter C_EXT_RST_WIDTH bound to: 4 - type: integer 
	Parameter C_AUX_RST_WIDTH bound to: 4 - type: integer 
	Parameter C_EXT_RESET_HIGH bound to: 1'b0 
	Parameter C_AUX_RESET_HIGH bound to: 1'b0 
	Parameter C_NUM_BUS_RST bound to: 1 - type: integer 
	Parameter C_NUM_PERP_RST bound to: 1 - type: integer 
	Parameter C_NUM_INTERCONNECT_ARESETN bound to: 1 - type: integer 
	Parameter C_NUM_PERP_ARESETN bound to: 1 - type: integer 
INFO: [Synth 8-3491] module 'proc_sys_reset' declared at '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1264' bound to instance 'U0' of component 'proc_sys_reset' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/synth/proc_sys_reset_ip.vhd:129]
INFO: [Synth 8-638] synthesizing module 'proc_sys_reset' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1323]
	Parameter C_FAMILY bound to: virtex7 - type: string 
	Parameter C_EXT_RST_WIDTH bound to: 4 - type: integer 
	Parameter C_AUX_RST_WIDTH bound to: 4 - type: integer 
	Parameter C_EXT_RESET_HIGH bound to: 1'b0 
	Parameter C_AUX_RESET_HIGH bound to: 1'b0 
	Parameter C_NUM_BUS_RST bound to: 1 - type: integer 
	Parameter C_NUM_PERP_RST bound to: 1 - type: integer 
	Parameter C_NUM_INTERCONNECT_ARESETN bound to: 1 - type: integer 
	Parameter C_NUM_PERP_ARESETN bound to: 1 - type: integer 
	Parameter INIT bound to: 1'b1 
	Parameter IS_C_INVERTED bound to: 1'b0 
	Parameter IS_D_INVERTED bound to: 1'b0 
	Parameter IS_R_INVERTED bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'FDRE_inst' to cell 'FDRE' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1392]
	Parameter INIT bound to: 1'b1 
	Parameter IS_C_INVERTED bound to: 1'b0 
	Parameter IS_D_INVERTED bound to: 1'b0 
	Parameter IS_R_INVERTED bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'FDRE_BSR' to cell 'FDRE' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1408]
	Parameter INIT bound to: 1'b0 
	Parameter IS_C_INVERTED bound to: 1'b0 
	Parameter IS_D_INVERTED bound to: 1'b0 
	Parameter IS_R_INVERTED bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'FDRE_BSR_N' to cell 'FDRE' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1434]
	Parameter INIT bound to: 1'b1 
	Parameter IS_C_INVERTED bound to: 1'b0 
	Parameter IS_D_INVERTED bound to: 1'b0 
	Parameter IS_R_INVERTED bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'FDRE_PER' to cell 'FDRE' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1457]
	Parameter INIT bound to: 1'b0 
	Parameter IS_C_INVERTED bound to: 1'b0 
	Parameter IS_D_INVERTED bound to: 1'b0 
	Parameter IS_R_INVERTED bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'FDRE_PER_N' to cell 'FDRE' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1481]
INFO: [Synth 8-638] synthesizing module 'lpf' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:816]
	Parameter C_EXT_RST_WIDTH bound to: 4 - type: integer 
	Parameter C_AUX_RST_WIDTH bound to: 4 - type: integer 
	Parameter C_EXT_RESET_HIGH bound to: 1'b0 
	Parameter C_AUX_RESET_HIGH bound to: 1'b0 
INFO: [Synth 8-3491] module 'SRL16' declared at '/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:50695' bound to instance 'POR_SRL_I' of component 'SRL16' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:868]
INFO: [Synth 8-6157] synthesizing module 'SRL16' [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:50695]
	Parameter INIT bound to: 16'b0000000000000000 
INFO: [Synth 8-6155] done synthesizing module 'SRL16' (13#1) [/opt/Xilinx/Vivado/2018.2/scripts/rt/data/unisim_comp.v:50695]
INFO: [Synth 8-638] synthesizing module 'cdc_sync' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:106]
	Parameter C_CDC_TYPE bound to: 1 - type: integer 
	Parameter C_RESET_STATE bound to: 0 - type: integer 
	Parameter C_SINGLE_BIT bound to: 1 - type: integer 
	Parameter C_FLOP_INPUT bound to: 0 - type: integer 
	Parameter C_VECTOR_WIDTH bound to: 2 - type: integer 
	Parameter C_MTBF_STAGES bound to: 4 - type: integer 
	Parameter INIT bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'CROSS_PLEVEL_IN2SCNDRY_IN_cdc_to' to cell 'FDR' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:514]
	Parameter INIT bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'CROSS_PLEVEL_IN2SCNDRY_s_level_out_d2' to cell 'FDR' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:545]
	Parameter INIT bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'CROSS_PLEVEL_IN2SCNDRY_s_level_out_d3' to cell 'FDR' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:554]
	Parameter INIT bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'CROSS_PLEVEL_IN2SCNDRY_s_level_out_d4' to cell 'FDR' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:564]
	Parameter INIT bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'CROSS_PLEVEL_IN2SCNDRY_s_level_out_d5' to cell 'FDR' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:574]
	Parameter INIT bound to: 1'b0 
INFO: [Synth 8-113] binding component instance 'CROSS_PLEVEL_IN2SCNDRY_s_level_out_d6' to cell 'FDR' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:584]
INFO: [Synth 8-256] done synthesizing module 'cdc_sync' (14#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/lib_cdc_v1_0_rfs.vhd:106]
INFO: [Synth 8-256] done synthesizing module 'lpf' (15#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:816]
INFO: [Synth 8-638] synthesizing module 'sequence_psr' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:301]
INFO: [Synth 8-638] synthesizing module 'upcnt_n' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:125]
	Parameter C_SIZE bound to: 6 - type: integer 
INFO: [Synth 8-256] done synthesizing module 'upcnt_n' (16#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:125]
INFO: [Synth 8-256] done synthesizing module 'sequence_psr' (17#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:301]
INFO: [Synth 8-256] done synthesizing module 'proc_sys_reset' (18#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/hdl/proc_sys_reset_v5_0_vh_rfs.vhd:1323]
INFO: [Synth 8-256] done synthesizing module 'proc_sys_reset_ip' (19#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/proc_sys_reset_ip/synth/proc_sys_reset_ip.vhd:74]
INFO: [Synth 8-6157] synthesizing module 'nf_datapath' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:44]
	Parameter C_S_AXI_DATA_WIDTH bound to: 32 - type: integer 
	Parameter C_S_AXI_ADDR_WIDTH bound to: 12 - type: integer 
	Parameter C_BASEADDR bound to: 0 - type: integer 
	Parameter C_M_AXIS_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_S_AXIS_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_M_AXIS_TUSER_WIDTH bound to: 128 - type: integer 
	Parameter C_S_AXIS_TUSER_WIDTH bound to: 128 - type: integer 
	Parameter NUM_QUEUES bound to: 5 - type: integer 
	Parameter DIGEST_WIDTH bound to: 80 - type: integer 
	Parameter C_AXIS_TUSER_DIGEST_WIDTH bound to: 304 - type: integer 
	Parameter Q_SIZE_WIDTH bound to: 16 - type: integer 
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:194]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:195]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:196]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:197]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:198]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:199]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:201]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:202]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:203]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:204]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:205]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:206]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:209]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:210]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:211]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:212]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:213]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:321]
INFO: [Synth 8-5534] Detected attribute (* mark_debug = "true" *) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:322]
INFO: [Synth 8-6157] synthesizing module 'input_arbiter_ip' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/synth/input_arbiter_ip.v:57]
INFO: [Synth 8-6157] synthesizing module 'input_arbiter' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter.v:55]
	Parameter C_M_AXIS_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_S_AXIS_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_M_AXIS_TUSER_WIDTH bound to: 128 - type: integer 
	Parameter C_S_AXIS_TUSER_WIDTH bound to: 128 - type: integer 
	Parameter NUM_QUEUES bound to: 5 - type: integer 
	Parameter C_S_AXI_DATA_WIDTH bound to: 32 - type: integer 
	Parameter C_S_AXI_ADDR_WIDTH bound to: 12 - type: integer 
	Parameter C_BASEADDR bound to: 0 - type: integer 
	Parameter NUM_QUEUES_WIDTH bound to: 3 - type: integer 
	Parameter NUM_STATES bound to: 1 - type: integer 
	Parameter IDLE bound to: 0 - type: integer 
	Parameter WR_PKT bound to: 1 - type: integer 
	Parameter MAX_PKT_SIZE bound to: 2000 - type: integer 
	Parameter IN_FIFO_DEPTH_BIT bound to: 6 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'fallthrough_small_fifo' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/fallthrough_small_fifo.v:46]
	Parameter WIDTH bound to: 417 - type: integer 
	Parameter MAX_DEPTH_BITS bound to: 6 - type: integer 
	Parameter PROG_FULL_THRESHOLD bound to: 63 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'small_fifo' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/small_fifo.v:44]
	Parameter WIDTH bound to: 417 - type: integer 
	Parameter MAX_DEPTH_BITS bound to: 6 - type: integer 
	Parameter PROG_FULL_THRESHOLD bound to: 63 - type: integer 
	Parameter MAX_DEPTH bound to: 64 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'small_fifo' (20#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/small_fifo.v:44]
INFO: [Synth 8-6155] done synthesizing module 'fallthrough_small_fifo' (21#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/fallthrough_small_fifo.v:46]
INFO: [Synth 8-6157] synthesizing module 'input_arbiter_cpu_regs' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter_cpu_regs.v:42]
	Parameter C_BASE_ADDRESS bound to: 0 - type: integer 
	Parameter C_S_AXI_DATA_WIDTH bound to: 32 - type: integer 
	Parameter C_S_AXI_ADDR_WIDTH bound to: 12 - type: integer 
INFO: [Synth 8-155] case statement is not full and has no default [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter_cpu_regs.v:305]
INFO: [Synth 8-6155] done synthesizing module 'input_arbiter_cpu_regs' (22#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter_cpu_regs.v:42]
INFO: [Synth 8-6155] done synthesizing module 'input_arbiter' (23#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/hdl/input_arbiter.v:55]
INFO: [Synth 8-6155] done synthesizing module 'input_arbiter_ip' (24#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/input_arbiter_ip/synth/input_arbiter_ip.v:57]
INFO: [Synth 8-6157] synthesizing module 'nf_sume_sdnet_ip' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/synth/nf_sume_sdnet_ip.v:57]
INFO: [Synth 8-6157] synthesizing module 'nf_sume_sdnet' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:44]
	Parameter C_M_AXIS_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_S_AXIS_DATA_WIDTH bound to: 256 - type: integer 
	Parameter C_M_AXIS_TUSER_WIDTH bound to: 304 - type: integer 
	Parameter C_S_AXIS_TUSER_WIDTH bound to: 128 - type: integer 
	Parameter C_S_AXI_DATA_WIDTH bound to: 32 - type: integer 
	Parameter C_S_AXI_ADDR_WIDTH bound to: 12 - type: integer 
	Parameter SDNET_ADDR_WIDTH bound to: 12 - type: integer 
	Parameter DIGEST_WIDTH bound to: 256 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'sume_to_sdnet' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/sume_to_sdnet.v:41]
	Parameter FIRST bound to: 0 - type: integer 
	Parameter WAIT bound to: 1 - type: integer 
INFO: [Synth 8-155] case statement is not full and has no default [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/sume_to_sdnet.v:72]
INFO: [Synth 8-6155] done synthesizing module 'sume_to_sdnet' (25#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/sume_to_sdnet.v:41]
INFO: [Synth 8-6157] synthesizing module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/SimpleSumeSwitch.v:36]
INFO: [Synth 8-6157] synthesizing module 'S_RESETTER_line' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_line.v:40]
INFO: [Synth 8-6155] done synthesizing module 'S_RESETTER_line' (26#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_line.v:40]
INFO: [Synth 8-6157] synthesizing module 'S_RESETTER_lookup' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_lookup.v:40]
INFO: [Synth 8-6155] done synthesizing module 'S_RESETTER_lookup' (27#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_lookup.v:40]
INFO: [Synth 8-6157] synthesizing module 'S_RESETTER_control' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_control.v:40]
INFO: [Synth 8-6155] done synthesizing module 'S_RESETTER_control' (28#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_RESETTER.HDL/S_RESETTER_control.v:40]
INFO: [Synth 8-6157] synthesizing module 'TopParser_t' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopParser_t.HDL/TopParser_t.v:169]
INFO: [Synth 8-6155] done synthesizing module 'TopParser_t' (181#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopParser_t.HDL/TopParser_t.v:169]
INFO: [Synth 8-6157] synthesizing module 'TopPipe_lvl_t' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_t.HDL/TopPipe_lvl_t.v:172]
INFO: [Synth 8-6155] done synthesizing module 'TopPipe_lvl_t' (188#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_t.HDL/TopPipe_lvl_t.v:172]
INFO: [Synth 8-6157] synthesizing module 'dummy_table_for_netpfga_t' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/dummy_table_for_netpfga_t.v:36]
	Parameter K bound to: 48 - type: integer 
	Parameter V bound to: 10 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_tdpram' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:7325]
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-1] MEMORY_PRIMITIVE (0) instructs Vivado Synthesis to choose the memory primitive type. Depending on their values, other XPM_MEMORY parameters may preclude the choice of certain memory primitive types. Review XPM_MEMORY documentation and parameter values to understand any limitations, or set MEMORY_PRIMITIVE to a different value.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:467]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base' (190#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_tdpram' (191#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:7325]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 

Warning: Trying to implement RAM in registers. Block RAM or DRAM implementation is not possible for one or more of the following reasons :
	1: Invalid write to RAM. 
	2: Unable to determine number of words or word size in RAM. 
	3: No valid read/write found for RAM. 
RAM dissolved into registers
WARNING: [Synth 8-4767] Trying to implement RAM 'CamPtrBck_reg' in registers. Block RAM or DRAM implementation is not possible; see log for reasons.
Reason is one or more of the following :
	1: RAM has multiple writes via different ports in same process. If RAM inferencing intended, write to one port per process. 
	2: Unable to determine number of words or word size in RAM. 
	3: No valid read/write found for RAM. 
RAM "CamPtrBck_reg" dissolved into registers
WARNING: [Synth 8-4767] Trying to implement RAM 'CamPtrFwd_reg' in registers. Block RAM or DRAM implementation is not possible; see log for reasons.
Reason is one or more of the following :
	1: RAM has multiple writes via different ports in same process. If RAM inferencing intended, write to one port per process. 
	2: Unable to determine number of words or word size in RAM. 
	3: No valid read/write found for RAM. 
RAM "CamPtrFwd_reg" dissolved into registers
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_b.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "yes" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'dummy_table_for_netpfga_t' (204#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/dummy_table_for_netpfga_t.HDL/dummy_table_for_netpfga_t.v:36]
INFO: [Synth 8-6157] synthesizing module 'TopPipe_lvl_0_t' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_0_t.HDL/TopPipe_lvl_0_t.v:174]
INFO: [Synth 8-6155] done synthesizing module 'TopPipe_lvl_0_t' (222#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopPipe_lvl_0_t.HDL/TopPipe_lvl_0_t.v:174]
INFO: [Synth 8-6157] synthesizing module 'TopDeparser_t' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopDeparser_t.HDL/TopDeparser_t.v:169]
INFO: [Synth 8-6155] done synthesizing module 'TopDeparser_t' (682#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/TopDeparser_t.HDL/TopDeparser_t.v:169]
INFO: [Synth 8-6157] synthesizing module 'S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.v:36]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: 1651663213 - type: integer 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 48 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 128 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: std - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 48 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 3 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 48 - type: integer 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 48 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 128 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 48 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 3 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 48 - type: integer 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 12288 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 128 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 3 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 12288 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 48 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 48 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 48 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 48 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 48 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 48 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 48 - type: integer 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 48 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 48 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 48 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 48 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 48 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 48 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 48 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "no" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized0' (682#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6157] synthesizing module 'xpm_cdc_gray' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:284]
	Parameter DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter INIT_SYNC_FF bound to: 1 - type: integer 
	Parameter REG_OUTPUT bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter SIM_LOSSLESS_GRAY_CHK bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter WIDTH bound to: 8 - type: integer 
INFO: [Synth 8-5534] Detected attribute (* ASYNC_REG = "TRUE" *) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:358]
WARNING: [Synth 8-6014] Unused sequential element dest_out_bin_ff_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:417]
INFO: [Synth 8-6155] done synthesizing module 'xpm_cdc_gray' (683#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:284]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_reg_vec' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1733]
	Parameter REG_WIDTH bound to: 8 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_reg_vec' (684#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1733]
INFO: [Synth 8-6157] synthesizing module 'xpm_cdc_gray__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:284]
	Parameter DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter INIT_SYNC_FF bound to: 1 - type: integer 
	Parameter REG_OUTPUT bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter SIM_LOSSLESS_GRAY_CHK bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter WIDTH bound to: 9 - type: integer 
WARNING: [Synth 8-6014] Unused sequential element dest_out_bin_ff_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:417]
INFO: [Synth 8-6155] done synthesizing module 'xpm_cdc_gray__parameterized0' (684#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:284]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_reg_vec__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1733]
	Parameter REG_WIDTH bound to: 9 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_reg_vec__parameterized0' (684#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1733]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_rst' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1478]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1638]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1663]
INFO: [Synth 8-6157] synthesizing module 'xpm_cdc_sync_rst' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:1055]
	Parameter DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter INIT bound to: 32'sb00000000000000000000000000000000 
	Parameter INIT_SYNC_FF bound to: 1 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter DEF_VAL bound to: 1'b0 
INFO: [Synth 8-5534] Detected attribute (* ASYNC_REG = "TRUE" *) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:1107]
INFO: [Synth 8-6155] done synthesizing module 'xpm_cdc_sync_rst' (685#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:1055]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_rst' (686#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1478]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_reg_bit' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1755]
	Parameter RST_VALUE bound to: 0 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_reg_bit' (687#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1755]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 9 - type: integer 
	Parameter RESET_VALUE bound to: 0 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn' (688#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 8 - type: integer 
	Parameter RESET_VALUE bound to: 1 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn__parameterized0' (688#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn__parameterized1' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 8 - type: integer 
	Parameter RESET_VALUE bound to: 2 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn__parameterized1' (688#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "no" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base' (689#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "no" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async' (690#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "no" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request' (691#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_BRIDGERs.HDL/S_BRIDGER_for_dummy_table_for_netpfga_tuple_in_request.v:36]
INFO: [Synth 8-6157] synthesizing module 'S_PROTOCOL_ADAPTER_INGRESS' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:36]
	Parameter IDLE bound to: 1 - type: integer 
	Parameter RX_SOF bound to: 2 - type: integer 
	Parameter RX_SOF_EOF bound to: 3 - type: integer 
	Parameter RX_PKT bound to: 4 - type: integer 
INFO: [Synth 8-4471] merging register 'tuple_out_control_VALID_reg' into 'packet_out_SOF_reg' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:182]
WARNING: [Synth 8-6014] Unused sequential element tuple_out_control_VALID_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:182]
INFO: [Synth 8-6155] done synthesizing module 'S_PROTOCOL_ADAPTER_INGRESS' (692#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_INGRESS.v:36]
INFO: [Synth 8-6157] synthesizing module 'S_PROTOCOL_ADAPTER_EGRESS' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v:36]
INFO: [Synth 8-6155] done synthesizing module 'S_PROTOCOL_ADAPTER_EGRESS' (693#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_PROTOCOL_ADAPTERs.HDL/S_PROTOCOL_ADAPTER_EGRESS.v:36]
INFO: [Synth 8-6157] synthesizing module 'S_SYNCER_for_TopParser' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v:40]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_sync' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 129 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 129 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:124]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
WARNING: [Synth 8-6104] Input port 'value' has an internal driver [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:126]
INFO: [Common 17-14] Message 'Synth 8-6104' appears 100 times and further instances of the messages will be disabled. Use the Tcl command set_msg_config to change the current settings.
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 129 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 129 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 136192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 129 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 129 - type: integer 
	Parameter PF_THRESH_MIN bound to: 3 - type: integer 
	Parameter PF_THRESH_MAX bound to: 509 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 509 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized1' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 136192 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 0 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 266 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 266 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 266 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 9 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 266 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 266 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 266 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 9 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 266 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 266 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 266 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 266 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 512 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 266 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 266 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 266 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "no" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-5772] Detected attribute (* ram_ecc = "no_ecc" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized1' (693#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_rst__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1478]
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_rst__parameterized0' (693#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1478]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn__parameterized2' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 10 - type: integer 
	Parameter RESET_VALUE bound to: 0 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn__parameterized2' (693#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn__parameterized3' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 9 - type: integer 
	Parameter RESET_VALUE bound to: 1 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn__parameterized3' (693#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn__parameterized4' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 9 - type: integer 
	Parameter RESET_VALUE bound to: 2 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn__parameterized4' (693#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
INFO: [Synth 8-5772] Detected attribute (* rw_addr_collision = "no" *) on RAM gen_wr_a.gen_word_narrow.mem_reg 
INFO: [Common 17-14] Message 'Synth 8-5772' appears 100 times and further instances of the messages will be disabled. Use the Tcl command set_msg_config to change the current settings.
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized0' (693#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_sync' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_sync__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 129 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: FWFT - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 129 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 1 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized1' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 129 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 1 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 129 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 1 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 512 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 127 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 127 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 507 - type: integer 
	Parameter PE_THRESH_MIN bound to: 5 - type: integer 
	Parameter PE_THRESH_MAX bound to: 507 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 2 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized2' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 512 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 1 - type: integer 
	Parameter CLOCKING_MODE bound to: 0 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 1 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 1 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 9 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 1 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 1 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 9 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 2 - type: integer 
	Parameter WRITE_MODE_B bound to: 1 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: distributed - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 1 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 1 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 1 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 1 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 512 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 1 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: yes - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 5 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 1 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
WARNING: [Synth 8-6014] Unused sequential element gen_rd_b.gen_doutb_pipe.enb_pipe_reg[0] was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:2588]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized2' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1161]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1207]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1218]
INFO: [Synth 8-6157] synthesizing module 'xpm_counter_updn__parameterized5' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
	Parameter COUNTER_WIDTH bound to: 2 - type: integer 
	Parameter RESET_VALUE bound to: 0 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_counter_updn__parameterized5' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1707]
INFO: [Synth 8-4471] merging register 'gen_fwft.empty_fwft_fb_reg' into 'gen_fwft.empty_fwft_i_reg' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
WARNING: [Synth 8-6014] Unused sequential element gen_fwft.empty_fwft_fb_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized1' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_sync__parameterized0' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized0' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 128 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 66 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 128 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 66 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized2' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 128 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 66 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 128 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 66 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 32768 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 66 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 66 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized3' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 32768 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 128 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 128 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 128 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 128 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 128 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 128 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 128 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 128 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 128 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 128 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 128 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 128 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 128 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized3' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized2' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized0' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized1' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 20 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 20 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized3' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 20 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 20 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 5120 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized4' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 5120 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 1 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 1 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 20 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 20 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 20 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 20 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 20 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 20 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 1 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: distributed - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 20 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 20 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 20 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 20 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 20 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 20 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: yes - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 20 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized4' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized3' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized1' (694#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
WARNING: [Synth 8-6014] Unused sequential element lje5zva3b7fpohnpjzm5_171_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v:353]
WARNING: [Synth 8-6014] Unused sequential element xzlkfmdns71h7e2v0d3kibu_144_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v:341]
WARNING: [Synth 8-6014] Unused sequential element vii2afgnndkx2se3zxe6zp2d_449_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v:355]
WARNING: [Synth 8-6014] Unused sequential element co0047przf303vs28oc7ca093adhe_403_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v:292]
INFO: [Synth 8-6155] done synthesizing module 'S_SYNCER_for_TopParser' (695#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopParser.v:40]
INFO: [Synth 8-6157] synthesizing module 'S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v:40]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_sync__parameterized1' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 135 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 135 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized4' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 135 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 135 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 136192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 135 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 135 - type: integer 
	Parameter PF_THRESH_MIN bound to: 3 - type: integer 
	Parameter PF_THRESH_MAX bound to: 509 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 509 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized4' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_sync__parameterized1' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_sync__parameterized2' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 135 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: FWFT - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 135 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 1 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized5' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 135 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 1 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 135 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 1 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 512 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 133 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 133 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 507 - type: integer 
	Parameter PE_THRESH_MIN bound to: 5 - type: integer 
	Parameter PE_THRESH_MAX bound to: 507 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 2 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1161]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1207]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1218]
INFO: [Synth 8-4471] merging register 'gen_fwft.empty_fwft_fb_reg' into 'gen_fwft.empty_fwft_i_reg' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
WARNING: [Synth 8-6014] Unused sequential element gen_fwft.empty_fwft_fb_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized5' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_sync__parameterized2' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized2' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized6' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 359168 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized5' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 359168 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 1403 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 1403 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 1403 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 1403 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 1403 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 1403 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 1403 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 1403 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 1403 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 1403 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 1403 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 1403 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 1403 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized5' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized6' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized2' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized3' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 160 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 160 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized7' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 160 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 160 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 40960 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized6' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 40960 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 160 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 160 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 160 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 160 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 160 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 160 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 160 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 160 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 160 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 160 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 160 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 160 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 160 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized6' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized7' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized3' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized4' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 256 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 256 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized8' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 256 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 256 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 65536 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized7' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 65536 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 256 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 256 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 256 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 256 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 256 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 256 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 256 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 256 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 256 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 256 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 256 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 256 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 256 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized7' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized8' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized4' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized5' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 128 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 128 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized9' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 128 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 128 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 32768 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized9' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized5' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized6' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 32 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 32 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized10' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 32 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 65 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 32 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 65 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 8192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 65 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized8' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 8192 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 1 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 1 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 32 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 32 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 32 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 32 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 32 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 32 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 1 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: distributed - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 32 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 32 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 32 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 32 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 32 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 32 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: yes - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 32 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized8' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized10' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized6' (695#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
WARNING: [Synth 8-6014] Unused sequential element klip4gackpvq52j270kq8x3_873_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v:557]
WARNING: [Synth 8-6014] Unused sequential element faomw3aac75nmdkmkr3la8iqnri9_539_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v:545]
WARNING: [Synth 8-6014] Unused sequential element ojvzuzwox0nctejl27aqo6kgzeptavw_778_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v:559]
WARNING: [Synth 8-6014] Unused sequential element m05ue9tq9sx0h78j_644_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v:452]
INFO: [Synth 8-6155] done synthesizing module 'S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser' (696#1) [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_S_SYNCER_for_TopDeparser.v:40]
INFO: [Synth 8-6157] synthesizing module 'S_SYNCER_for_S_SYNCER_for_TopDeparser' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v:40]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_sync__parameterized3' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 167 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 167 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized11' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 167 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 167 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 136192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 167 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 167 - type: integer 
	Parameter PF_THRESH_MIN bound to: 3 - type: integer 
	Parameter PF_THRESH_MAX bound to: 509 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 509 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized11' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_sync__parameterized3' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_sync__parameterized4' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 167 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: FWFT - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 167 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 1 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized12' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 167 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 1 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 167 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 1 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 512 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 165 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 165 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 507 - type: integer 
	Parameter PE_THRESH_MIN bound to: 5 - type: integer 
	Parameter PE_THRESH_MAX bound to: 507 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 2 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1161]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1207]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1218]
INFO: [Synth 8-4471] merging register 'gen_fwft.empty_fwft_fb_reg' into 'gen_fwft.empty_fwft_i_reg' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
WARNING: [Synth 8-6014] Unused sequential element gen_fwft.empty_fwft_fb_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized12' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_sync__parameterized4' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1800]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized7' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 256 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 256 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized13' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 256 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 256 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 65536 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized13' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized7' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized8' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized14' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1403 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 359168 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized14' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized8' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized9' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 16 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 16 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_base__parameterized15' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 16 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 16 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 4096 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6157] synthesizing module 'xpm_memory_base__parameterized9' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 4096 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 1 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 1 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 16 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 16 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 16 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 16 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 16 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 16 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 8 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 1 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: distributed - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 16 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 16 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 16 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 16 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 256 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 16 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 16 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 8 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: yes - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 16 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized9' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized15' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized9' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Synth 8-6157] synthesizing module 'xpm_fifo_async__parameterized10' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
INFO: [Common 17-14] Message 'Synth 8-6157' appears 100 times and further instances of the messages will be disabled. Use the Tcl command set_msg_config to change the current settings.
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 160 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 160 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 160 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 160 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 40960 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized16' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized10' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 128 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 128 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 128 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 81 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 128 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 81 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 32768 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 81 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_base__parameterized17' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:56]
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_async__parameterized11' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1937]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 128 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 11 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 7 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 33 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 11 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 7 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 33 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 128 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 11 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 7 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 33 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 11 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 7 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 33 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 128 - type: integer 
	Parameter FIFO_SIZE bound to: 1408 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 7 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 7 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 33 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 33 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 125 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 125 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 8 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 8 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 1408 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 1 - type: integer 
	Parameter CLOCKING_MODE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 1 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 11 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 11 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 11 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 7 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 11 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 11 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 11 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 7 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 1 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: distributed - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 11 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 11 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 11 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 11 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 128 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 11 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 11 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 7 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 7 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 7 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 7 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: yes - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 11 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
INFO: [Synth 8-6155] done synthesizing module 'xpm_memory_base__parameterized10' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:57]
	Parameter DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter INIT_SYNC_FF bound to: 1 - type: integer 
	Parameter REG_OUTPUT bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter SIM_LOSSLESS_GRAY_CHK bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter WIDTH bound to: 7 - type: integer 
WARNING: [Synth 8-6014] Unused sequential element dest_out_bin_ff_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:417]
INFO: [Synth 8-6155] done synthesizing module 'xpm_cdc_gray__parameterized1' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_cdc/hdl/xpm_cdc.sv:284]
	Parameter REG_WIDTH bound to: 7 - type: integer 
INFO: [Synth 8-6155] done synthesizing module 'xpm_fifo_reg_vec__parameterized1' (696#1) [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1733]
INFO: [Common 17-14] Message 'Synth 8-6155' appears 100 times and further instances of the messages will be disabled. Use the Tcl command set_msg_config to change the current settings.
	Parameter COUNTER_WIDTH bound to: 8 - type: integer 
	Parameter RESET_VALUE bound to: 0 - type: integer 
	Parameter COUNTER_WIDTH bound to: 7 - type: integer 
	Parameter RESET_VALUE bound to: 1 - type: integer 
	Parameter COUNTER_WIDTH bound to: 7 - type: integer 
	Parameter RESET_VALUE bound to: 2 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 20 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 84 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 20 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 84 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 20 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 84 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 20 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 84 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 5120 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 84 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 84 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 32 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 84 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 32 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 84 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 32 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 84 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 32 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 84 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 8192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 84 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 84 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
WARNING: [Synth 8-6014] Unused sequential element pnfqh25xbsdnaol7c6nkzwcvans1e_828_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v:659]
WARNING: [Synth 8-6014] Unused sequential element k413aw5mh35freumym0s5gc3w_743_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v:647]
WARNING: [Synth 8-6014] Unused sequential element orb2t9bgc7l675ethvajiqt5o2xrerg_387_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v:661]
WARNING: [Synth 8-6014] Unused sequential element tj4def1qaer2z3ro4lxaq_113_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_S_SYNCER_for_TopDeparser.v:532]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 143 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 143 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 266 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 143 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 266 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 143 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 136192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 143 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 143 - type: integer 
	Parameter PF_THRESH_MIN bound to: 3 - type: integer 
	Parameter PF_THRESH_MAX bound to: 509 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 509 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 143 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: FWFT - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 143 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 1 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 1 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 143 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 1 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 1 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 143 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 1 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 512 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 141 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 141 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 507 - type: integer 
	Parameter PE_THRESH_MIN bound to: 5 - type: integer 
	Parameter PE_THRESH_MAX bound to: 507 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 2 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1161]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1207]
INFO: [Synth 8-226] default block is never used [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1218]
INFO: [Synth 8-4471] merging register 'gen_fwft.empty_fwft_fb_reg' into 'gen_fwft.empty_fwft_i_reg' [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
WARNING: [Synth 8-6014] Unused sequential element gen_fwft.empty_fwft_fb_reg was removed.  [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_fifo/hdl/xpm_fifo.sv:1266]
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 20 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 72 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 20 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 72 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 20 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 72 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 20 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 72 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 5120 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 72 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 72 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
	Parameter FIFO_MEMORY_TYPE bound to: lutram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 32 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 72 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 32 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 72 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 1 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 32 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 72 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 32 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 72 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 1 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 8192 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 72 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 72 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
WARNING: [Synth 8-6014] Unused sequential element s7goz2l4stemczy85tpciujih8_270_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopDeparser.v:557]
WARNING: [Synth 8-6014] Unused sequential element k7v9ai7asbqumtk6fsulveqjzm_520_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopDeparser.v:545]
WARNING: [Synth 8-6014] Unused sequential element zw25w89we90ywaojvqm0h45_514_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopDeparser.v:559]
WARNING: [Synth 8-6014] Unused sequential element gy8637fcv1sd50c5i_239_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for_TopDeparser.v:452]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 290 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 135 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 290 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 135 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 1 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 1 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 512 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 290 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 135 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 290 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 9 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 135 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 512 - type: integer 
	Parameter FIFO_SIZE bound to: 148480 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 9 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 135 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 135 - type: integer 
	Parameter PF_THRESH_MIN bound to: 3 - type: integer 
	Parameter PF_THRESH_MAX bound to: 509 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 509 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 10 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
	Parameter MEMORY_TYPE bound to: 1 - type: integer 
	Parameter MEMORY_SIZE bound to: 148480 - type: integer 
	Parameter MEMORY_PRIMITIVE bound to: 2 - type: integer 
	Parameter CLOCKING_MODE bound to: 0 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter MEMORY_INIT_FILE bound to: none - type: string 
	Parameter MEMORY_INIT_PARAM bound to: (null) - type: string 
	Parameter USE_MEM_INIT bound to: 1 - type: integer 
	Parameter MEMORY_OPTIMIZATION bound to: true - type: string 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter AUTO_SLEEP_TIME bound to: 0 - type: integer 
	Parameter MESSAGE_CONTROL bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter USE_EMBEDDED_CONSTRAINT bound to: 0 - type: integer 
	Parameter WRITE_DATA_WIDTH_A bound to: 290 - type: integer 
	Parameter READ_DATA_WIDTH_A bound to: 290 - type: integer 
	Parameter BYTE_WRITE_WIDTH_A bound to: 290 - type: integer 
	Parameter ADDR_WIDTH_A bound to: 9 - type: integer 
	Parameter READ_RESET_VALUE_A bound to: 0 - type: string 
	Parameter READ_LATENCY_A bound to: 2 - type: integer 
	Parameter WRITE_MODE_A bound to: 2 - type: integer 
	Parameter WRITE_DATA_WIDTH_B bound to: 290 - type: integer 
	Parameter READ_DATA_WIDTH_B bound to: 290 - type: integer 
	Parameter BYTE_WRITE_WIDTH_B bound to: 290 - type: integer 
	Parameter ADDR_WIDTH_B bound to: 9 - type: integer 
	Parameter READ_RESET_VALUE_B bound to: 0 - type: string 
	Parameter READ_LATENCY_B bound to: 1 - type: integer 
	Parameter WRITE_MODE_B bound to: 2 - type: integer 
	Parameter P_MEMORY_PRIMITIVE bound to: block - type: string 
	Parameter P_MIN_WIDTH_DATA_A bound to: 290 - type: integer 
	Parameter P_MIN_WIDTH_DATA_B bound to: 290 - type: integer 
	Parameter P_MIN_WIDTH_DATA bound to: 290 - type: integer 
	Parameter P_MIN_WIDTH_DATA_ECC bound to: 290 - type: integer 
	Parameter P_MAX_DEPTH_DATA bound to: 512 - type: integer 
	Parameter P_ECC_MODE bound to: no_ecc - type: string 
	Parameter P_MEMORY_OPT bound to: yes - type: string 
	Parameter P_WIDTH_COL_WRITE_A bound to: 290 - type: integer 
	Parameter P_WIDTH_COL_WRITE_B bound to: 290 - type: integer 
	Parameter P_NUM_COLS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_COLS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_WRITE_B bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_A bound to: 1 - type: integer 
	Parameter P_NUM_ROWS_READ_B bound to: 1 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_A bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_WRITE_B bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_READ_A bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_READ_B bound to: 9 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_WRITE_B bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_A bound to: 0 - type: integer 
	Parameter P_WIDTH_ADDR_LSB_READ_B bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_A bound to: 0 - type: integer 
	Parameter P_ENABLE_BYTE_WRITE_B bound to: 0 - type: integer 
	Parameter P_SDP_WRITE_MODE bound to: no - type: string 
	Parameter NUM_CHAR_LOC bound to: 0 - type: integer 
	Parameter MAX_NUM_CHAR bound to: 0 - type: integer 
	Parameter P_MIN_WIDTH_DATA_SHFT bound to: 290 - type: integer 
	Parameter P_MIN_WIDTH_DATA_LDW bound to: 4 - type: integer 
INFO: [Synth 8-6059] Synth Info: [XPM_MEMORY 20-2] MEMORY_INIT_FILE (none), MEMORY_INIT_PARAM together specify no memory initialization. Initial memory contents will be all 0's.   [/opt/Xilinx/Vivado/2018.2/data/ip/xpm/xpm_memory/hdl/xpm_memory.sv:469]
	Parameter FIFO_MEMORY_TYPE bound to: bram - type: string 
	Parameter ECC_MODE bound to: no_ecc - type: string 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 256 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 66 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: STD - type: string 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 256 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 66 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_SYNC_STAGES bound to: 2 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter P_FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter P_COMMON_CLOCK bound to: 0 - type: integer 
	Parameter P_ECC_MODE bound to: 0 - type: integer 
	Parameter P_READ_MODE bound to: 0 - type: integer 
	Parameter P_WAKEUP_TIME bound to: 2 - type: integer 
	Parameter COMMON_CLOCK bound to: 0 - type: integer 
	Parameter RELATED_CLOCKS bound to: 0 - type: integer 
	Parameter FIFO_MEMORY_TYPE bound to: 2 - type: integer 
	Parameter ECC_MODE bound to: 0 - type: integer 
	Parameter FIFO_WRITE_DEPTH bound to: 256 - type: integer 
	Parameter WRITE_DATA_WIDTH bound to: 256 - type: integer 
	Parameter WR_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_FULL_THRESH bound to: 66 - type: integer 
	Parameter USE_ADV_FEATURES bound to: 0707 - type: string 
	Parameter READ_MODE bound to: 0 - type: integer 
	Parameter FIFO_READ_LATENCY bound to: 1 - type: integer 
	Parameter READ_DATA_WIDTH bound to: 256 - type: integer 
	Parameter RD_DATA_COUNT_WIDTH bound to: 8 - type: integer 
	Parameter PROG_EMPTY_THRESH bound to: 66 - type: integer 
	Parameter DOUT_RESET_VALUE bound to: 0 - type: string 
	Parameter CDC_DEST_SYNC_FF bound to: 2 - type: integer 
	Parameter FULL_RESET_VALUE bound to: 0 - type: integer 
	Parameter REMOVE_WR_RD_PROT_LOGIC bound to: 0 - type: integer 
	Parameter WAKEUP_TIME bound to: 0 - type: integer 
	Parameter VERSION bound to: 0 - type: integer 
	Parameter SIM_ASSERT_CHK bound to: 0 - type: integer 
	Parameter FIFO_MEM_TYPE bound to: 2 - type: integer 
	Parameter RD_MODE bound to: 0 - type: integer 
	Parameter ENABLE_ECC bound to: 0 - type: integer 
	Parameter FIFO_READ_DEPTH bound to: 256 - type: integer 
	Parameter FIFO_SIZE bound to: 65536 - type: integer 
	Parameter WR_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter RD_PNTR_WIDTH bound to: 8 - type: integer 
	Parameter FULL_RST_VAL bound to: 1'b0 
	Parameter WR_RD_RATIO bound to: 0 - type: integer 
	Parameter PF_THRESH_ADJ bound to: 66 - type: integer 
	Parameter PE_THRESH_ADJ bound to: 66 - type: integer 
	Parameter PF_THRESH_MIN bound to: 5 - type: integer 
	Parameter PF_THRESH_MAX bound to: 253 - type: integer 
	Parameter PE_THRESH_MIN bound to: 3 - type: integer 
	Parameter PE_THRESH_MAX bound to: 253 - type: integer 
	Parameter WR_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_DC_WIDTH_EXT bound to: 9 - type: integer 
	Parameter RD_LATENCY bound to: 1 - type: integer 
	Parameter EN_ADV_FEATURE bound to: 16'b0000011100000111 
	Parameter EN_OF bound to: 1'b1 
	Parameter EN_PF bound to: 1'b1 
	Parameter EN_WDC bound to: 1'b1 
	Parameter EN_AF bound to: 1'b0 
	Parameter EN_WACK bound to: 1'b0 
	Parameter FG_EQ_ASYM_DOUT bound to: 1'b0 
	Parameter EN_UF bound to: 1'b1 
	Parameter EN_PE bound to: 1'b1 
	Parameter EN_RDC bound to: 1'b1 
	Parameter EN_AE bound to: 1'b0 
	Parameter EN_DVLD bound to: 1'b0 
WARNING: [Synth 8-6014] Unused sequential element deb6c1bi780jezwi1p7degzak3d9ztru_464_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for__OUT_.v:302]
WARNING: [Synth 8-6014] Unused sequential element yavp89s4k9ktdj10imcapab_477_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for__OUT_.v:300]
WARNING: [Synth 8-6014] Unused sequential element nwb48nwf3wza6yas_820_reg was removed.  [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/SimpleSumeSwitch/S_SYNCERs.HDL/S_SYNCER_for__OUT_.v:337]
ERROR: [Synth 8-448] named port connection 'tuple_in_sume_metadata_VALID' does not exist for instance 'SimpleSumeSwitch_inst' of module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:184]
ERROR: [Synth 8-448] named port connection 'tuple_in_sume_metadata_DATA' does not exist for instance 'SimpleSumeSwitch_inst' of module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:185]
WARNING: [Synth 8-689] width (12) of port connection 'control_S_AXI_AWADDR' does not match port width (8) of module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:189]
WARNING: [Synth 8-689] width (12) of port connection 'control_S_AXI_ARADDR' does not match port width (8) of module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:199]
ERROR: [Synth 8-448] named port connection 'tuple_out_sume_metadata_VALID' does not exist for instance 'SimpleSumeSwitch_inst' of module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:218]
ERROR: [Synth 8-448] named port connection 'tuple_out_sume_metadata_DATA' does not exist for instance 'SimpleSumeSwitch_inst' of module 'SimpleSumeSwitch' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:219]
ERROR: [Synth 8-6156] failed synthesizing module 'nf_sume_sdnet' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/nf_sume_sdnet_ip/wrapper/nf_sume_sdnet.v:44]
ERROR: [Synth 8-6156] failed synthesizing module 'nf_sume_sdnet_ip' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.srcs/sources_1/ip/nf_sume_sdnet_ip/synth/nf_sume_sdnet_ip.v:57]
ERROR: [Synth 8-6156] failed synthesizing module 'nf_datapath' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/nf_datapath.v:44]
ERROR: [Synth 8-6156] failed synthesizing module 'top' [/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/hdl/top.v:43]
---------------------------------------------------------------------------------
Finished RTL Elaboration : Time (s): cpu = 00:01:28 ; elapsed = 00:01:54 . Memory (MB): peak = 2435.715 ; gain = 1114.496 ; free physical = 9076 ; free virtual = 14379
---------------------------------------------------------------------------------
RTL Elaboration failed
INFO: [Common 17-83] Releasing license: Synthesis
432 Infos, 163 Warnings, 0 Critical Warnings and 9 Errors encountered.
synth_design failed
ERROR: [Common 17-69] Command failed: Synthesis failed - please see the console or run log file for details
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 20:33:35 2019...
[Sat Jul 13 20:33:35 2019] synth finished
wait_on_run: Time (s): cpu = 00:27:54 ; elapsed = 00:47:58 . Memory (MB): peak = 2864.801 ; gain = 0.000 ; free physical = 9632 ; free virtual = 14935
# launch_runs impl_1 -to_step write_bitstream
[Sat Jul 13 20:33:37 2019] Launched synth_1...
Run output will be captured here: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/synth_1/runme.log
[Sat Jul 13 20:33:37 2019] Launched impl_1...
Run output will be captured here: /home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/project/simple_sume_switch.runs/impl_1/runme.log
# wait_on_run impl_1
[Sat Jul 13 20:33:37 2019] Waiting for impl_1 to finish...
[Sat Jul 13 20:35:42 2019] impl_1 finished
wait_on_run: Time (s): cpu = 00:01:38 ; elapsed = 00:02:06 . Memory (MB): peak = 2876.812 ; gain = 0.000 ; free physical = 9629 ; free virtual = 14934
# exit
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 20:35:42 2019...
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
make -C hw export_to_sdk
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
rm -f ../hw/create_ip/id_rom16x32.coe
cp /home/nico/projects/P4-NetFPGA/tools/scripts/epoch.sh . && sh epoch.sh && rm -f epoch.sh
echo 16028002 >> rom_data.txt
echo `/home/nico/projects/P4-NetFPGA/run_tag.sh` >> rom_data.txt
grep: ../../../RELEASE_NOTES: No such file or directory
echo 00000204 >> rom_data.txt
echo 0000FFFF >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
echo FFFF0000 >> rom_data.txt
cp /home/nico/projects/P4-NetFPGA/tools/scripts/format_coe.py . && python format_coe.py && rm -f format_coe.py 
16

mv -f id_rom16x32.coe ../hw/create_ip/
mv -f rom_data.txt ../hw/create_ip/
if test -d project; then\
	echo "export simple_sume_switch project to SDK"; \
	vivado -mode tcl -source tcl/export_hardware.tcl -tclargs simple_sume_switch;\
else \
	echo "Project simple_sume_switch does not exist.";\
	echo "Please run \"make project\" to create and build the project first";\
fi;\

export simple_sume_switch project to SDK

****** Vivado v2018.2 (64-bit)
  **** SW Build 2258646 on Thu Jun 14 20:02:38 MDT 2018
  **** IP Build 2256618 on Thu Jun 14 22:10:49 MDT 2018
    ** Copyright 1986-2018 Xilinx, Inc. All Rights Reserved.

source tcl/export_hardware.tcl
# set design [lindex $argv 0] 
# puts "\nOpening $design XPR project\n"

Opening simple_sume_switch XPR project

# open_project project/$design.xpr
Scanning sources...
Finished scanning sources
INFO: [IP_Flow 19-234] Refreshing IP repositories
INFO: [IP_Flow 19-1700] Loaded user IP repository '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/ip_repo'.
INFO: [IP_Flow 19-2313] Loaded Vivado IP repository '/opt/Xilinx/Vivado/2018.2/data/ip'.
WARNING: [IP_Flow 19-3664] IP 'bd_7ad4_xpcs_0' generated file not found '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/.Xil/Vivado-21647-nsg-System/coregen/bd_7ad4_xpcs_0_1/elaborate/configure_gt.tcl'. Please regenerate to continue.
WARNING: [IP_Flow 19-3664] IP 'bd_a1aa_xpcs_0' generated file not found '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw/.Xil/Vivado-21647-nsg-System/coregen/bd_a1aa_xpcs_0_2/elaborate/configure_gt.tcl'. Please regenerate to continue.
open_project: Time (s): cpu = 00:00:05 ; elapsed = 00:00:05 . Memory (MB): peak = 1365.711 ; gain = 188.977 ; free physical = 10356 ; free virtual = 15661
# puts "\nOpening $design Implementation design\n"

Opening simple_sume_switch Implementation design

# open_run impl_1
ERROR: [Common 17-69] Command failed: Run 'impl_1' has not been launched. Unable to open
Vivado%	quit
INFO: [Common 17-206] Exiting Vivado at Sat Jul 13 22:08:24 2019...
make[1]: Leaving directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/hw'
make -C sw/embedded/ project
make[1]: Entering directory '/home/nico/projects/P4-NetFPGA/contrib-projects/sume-sdnet-switch/projects/minip4/simple_sume_switch/sw/embedded'
mkdir ./SDK_Workspace
xsdk -batch -source ./tcl/simple_sume_switch_xsdk.tcl
