_discoverable: yes
---
_hidden: no
---
title: BGP Peering
---
subtitle: Manage your own address space
---
---
headline1: BGP Peering
---
headline2: Your own IP Space
---
headline3: At Data Center Light
---
header_background_color: #6298CB
---
header_text_color: text-light
---
content1_text:

## For whom is BGP peering?

If you have your own ASN with IPv6 or IPv4 address space, you can
announce it in our data centers.

## What is required for BGP peering

To be able to peer with us, you will need to have IP addresses in our
data center. This is the case if you have one of these products:

* [A Data Center Light VM](../virtual-machine-hosting/)
* [An IPv6 Only VM](../ipv6-only-hosting/)
* [Physical co-located hardware](../colocation/)

## How to setup BGP peering

Send a mail to support -at- ungleich.ch containing the following
information:

* Your ASN and the list of networks you intend to announce
* Your local IP addresses

Before we can peer, ensure that all objects in the RIPE database are
setup correctly. Specifically ensure that you have

* route6 / route objects
* inet6num / inetnum objects
* ROA / RPKI configured

## Pricing

Setting up peering has a 42 CHF one time fee.
